IEEE P802.11
Wireless LANs

|  |
| --- |
| Resolution CID 10569 |
| Date: 2016-01-19 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Santosh Abraham | Qualcomm | 5775 Morehouse Dr. San Diego, CA 92121 | +1-858 651 6107 | sabraham@qti.qualcomm.com |
| Abhishek Patil | Qualcomm | +1-858-845-4434 | appatil@qti.qualcomm.com |
| Jouni Malinen | Qualcomm |  | jouni@qca.qualcomm.com |
| George Cherian | Qualcomm | +1-858-651-6645 | gcherian@qti.qualcomm.com |

Abstract

This submission addresses CIDs 10569

 CID 10024

|  |  |  |  |
| --- | --- | --- | --- |
| CID | Comment | Proposed Change | Proposed Resolution |
| 10569 | "If the STA does not receive the FILS Container frame containing an IP assignment within the IP address request timeout period, then the STA may initiate an IP address assignment procedure using mechanisms that are out of scope of this specifica- tion." ---- what happens if the STA initiates an IP address assignment using other mechanisms, gets an IP, and the AP assigns afterwards a (different) IP address? | Insert a clarifying sentence to address the issue | Please adopt changes shown in doc 16/0140r1Note: the resolution also applies to lines 18-22 on pg 125 |

***Instruct the editor to modify section 10.47.3.3 of D6.3 as indicated:***

* + - 1. **FILS IP address configuration**

***Add following lines after lines 45-48 of page 125:***

If the STA does not receive the FILS Container frame containing an IP assignment within the IP address request timeout period, then the STA may initiate an IP address assignment procedure using mechanisms that are out of scope of this specification. If an STA has initiated an IP address assignment procedure (using mechanisms that are out of scope) due to the expiry of the timeout period, and subsequently receives an FILS container frame containing an IP assignment, it shall discard the IP address assignment received through the FILS container frame.

***Add following lines after lines 18-22 of page 125:***

If the STA does not receive the FILS Container frame containing IP assignment within IP address request timeout period, then the STA may initiate IP address assignment procedure using a FILS Container frame or mechanisms that are out of scope of this specification. If an STA has initiated an IP address assignment procedure (using mechanisms that are out of scope) due to the expiry of the timeout period, and subsequently receives an FILS container frame containing an IP assignment, it shall discard the IP address assignment received through the FILS container frame.