IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Resolutions for CID 22177 | | | | |
| Date: February 26, 2024 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Jianhan Liu | MediaTek |  |  | Jianhan.Liu@mediatek.com |
| Alfred Asterjadhi | Qualcomm |  |  |  |
| Bin Tian | Qualcomm |  |  |  |

Abstract

This submission proposes resolutions for the CID 22177 for SA ballot on draft 5.0.

**Revisions:**

* Rev 0: Initial version of the document.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Clause** | **Pg/Ln** | **Comment** | **Proposed Change** | **Resolution** |
| 22177 | 4.3.16a | 64.41 | "— Mandatory support for single spatial stream EHT-MCS 15 in an RU". Support of MCS15 should be optional. Another SDO is doing interoperability testing and MCS15 may be tested but as an optional feature. To avoid interoperability issue with already deployed 11be devices, I think it would be safer to make this feature optional and use one reserved bit of "EHT PHY Capabilities Information" field to indicate MCS15 support. For example B69 (currently reserved) could be renamed to "Support of MCS15 in an RU" and set to 1 is supported, 0 if not. It would not break existing device implementations IMHO. | As in comment (make MCS15 optional and use one reserved bit of "EHT PHY Capabilities Information" field to signal it) | **Revise.**  It is risky to change a mandatory feature to be optional on D5.0. The solution to indicate support or not of a mandatory feature can be done by introducing “disable” indication in the EHT Operation element and in the EHT OM Control. In the IEEE 802.11be, similar approach had been introduced for ER SU PPDU support.  11be Editor: please see the instructions in IEEE 802.11-24/0368r0. |

**Introduction to 11be Editor on CID 22177:**

**Text modification in Page xxx/Line xx in D5.0:**

* + - * 1. **EHT OM Control**

***TGbe editor: Change the figure below as follows (CID 22177):***

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | B0 | B1 | B2 | B3 | B4 B5 |
|  | Rx NSS  Extension | Channel Width Extension | Tx NSTS  Extension | MCS15 Disable | Reserved |
| Bits: | 1 | 1 | 1 | 1 | 2 |

**Figure 9-33a — Control Information subfield format in an EHT OM Control subfield**

***TGbe editor: Insert the paragraph below at the end of this subclause (CID 22177):***

A non-AP EHT STA sets the MCS15 Disable subfield to 1 to indicate that the reception of an EHT PPDU with EHT-MCS 15 is disabled and to 0 to indicate that the reception of an EHT PPDU with EHT-MCS 15 is enabled. If the EHT OM Control field is transmitted by an EHT AP, then the EHT-MCS 15 Disable subfield is reserved.

* + - 1. **EHT Operation element**

***TGbe editor: Change the figure below as follows (CID 22177):***

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  | B0 | B1 | B2 | B3 | B4 B5 | B6 | B7 |
|  | EHT Operation Information Present | Disabled Subchannel Bitmap Present | EHT  Default PE Duration | Group Addressed BU Indication Limit | Group Addressed BU Indication Exponent | MCS15 Disable | Reserved |
| Bits: | 1 | 1 | 1 | 1 | 2 | 1 | 1 |

**Figure 9-1001b—EHT Operation Parameters field forma****t**

***TGbe editor: Insert the paragraph below at the end of this subclause (CID 22177):***

The MCS15 Disable subfield indicates whether the reception of an EHT PPDU with EHT-MCS 15 by the AP is disabled or enabled. The MCS15 Disable subfield is set to 1 to indicate that it is disabled and set to 0 to indicate that it is enabled.

* + 1. **PPDU format selection**

…

An EHT STA 6G shall not transmit an EHT PPDU in EHT duplicate mode to a peer EHT STA if the EHT Capabilities element received from that peer EHT STA has the Support Of EHT DUP (EHT-MCS 14) In 6 GHz subfield equal to 0.

***TGbe editor: Insert the paragraph below after the 3rd paragraph of this subclause (CID 22177):***

An EHT STA shall not transmit an EHT PPDU with EHT-MCS-15 to a peer non-AP STA if the most recently received EHT OM Control field from that peer non-AP STA, if any, has the MCS15 Disable subfield equal to 1.

An EHT STA shall not transmit an EHT PPDU with EHT-MCS 15 to an AP if the most recently received EHT Operation element from that AP has the MCS15 Disable subfield equal to 1.

An EHT STA shall not transmit an EHT PPDU with EHT-MCS 15 and MRUs listed in Table 9-404n (Subfield of the EHT PHY Capabilities Information field) to a peer EHT STA if the EHT Capabilities element received from that peer EHT STA has the Support Of EHT-MCS 15 In MRU subfield equal to 0.

…