### **IEEE P802.11Wireless LANs**

|  |
| --- |
| CID 7094 |
| Date: 2024-04-16 |
| Author(s): |
| Name | Affiliation | Address | Phone | Email |
| Steve Shellhammer | Qualcomm |  |  | shellhammer@ieee.org |
| Ali Raissinia | Qualcomm |  |  | alirezar@qti.qualcomm.com |

**Abstract**

The document provides comment resolutions for CIDs: 7094.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Commenter** | **Clause** | **Page/Line** | **Comment** | **Proposed Change** | **Resolution** |
| 7094 | Kneckt, Jarkko | 27.3.20.2 | 4390/43 | Mapping between an Octet to bits, specifically which bits are LSB and MSB, is ambiguous | It would be better to add a note that clearly defines how the octet is mapped to bits and which bits are LSB and MSB. An example note would be " Note: the Octet should map to bits as follows: B7 B6 B5 B4 B3 B2 B1 B0, where B7 is the most significant bit and B0 is the least significant bit. An example of this mapping is 0xeb (Octet) = 11101011 (B7 B6 B5 B4 B3 B2 B1 B0)" | **Revised**TGme Editor makes changes as shown in IEEE 802.11-24/0697r1 |

**Discussion**

Agree with the commenter that the standard should be clear on which bits are the most significant bits and which are the least significant bits.

**Proposed Resolution**

TGme Editor make the following changes to the Draft,

The first seven pseudorandom octets (*Octet0*–*Octet6*) in the secure NDP are used for per stream phase rotations see 27.3.20.3 (Pseudorandom and deterministic per spatial stream phase rotations(11az)).

NOTE--Each octet that is used for per stream phase rotation is mapped so that B7 is the most significant bit and B0 is the least significant bit.

Starting with *Octet7*, these pseudorandom octets are used for construction of pseudorandom 64-QAM values in the secure HE-LTF sequences.