**IEEE P802.15**

**Wireless Personal Area Networks**

|  |  |  |
| --- | --- | --- |
| Project | IEEE P802.15 Working Group for Wireless Personal Area Networks (WPANs) | |
| Title | **Draft Oscillator Specification Text** | |
| Date Submitted | 30 April 2010 | |
| Source | Adrian Jennings  Time Domain | Voice: 256 759 4708 E-mail: adrian.jennings@timedomain.com |
| Re: | Draft of 802.15.4f | |
| Abstract | Recommended text for crystal oscillator specification in UWB PHY | |
| Purpose | Contribution to draft text | |
| Notice | This document has been prepared to assist the IEEE P802.15. It is offered as a basis for discussion and is not binding on the contributing individual(s) or organization(s). The material in this document is subject to change in form and content after further study. The contributor(s) reserve(s) the right to add, amend or withdraw material contained herein. | |
| Release | The contributor acknowledges and accepts that this contribution becomes the property of IEEE and may be made publicly available by P802.15. | |

**6.?? UWB RFID PHY Transmitter Specification**

The transmission time of any individual pulse shall not drift more than 10ns from its nominal transmission time over the specified operating temperature range of the device.

This is an important issue for OOK modulation since no synchronization update can be made within the receiver unless a “1” is received. For this reason, a long sequence of zeros will cause a long period between frequency drift updates and necessitate a higher quality frequency reference in the transmitter, which is generally not desirable. For this reason section ??? specifies that the modulator must insert (and the demodulator ignore) a sequence of pulses every 128th symbol after the PHR. This sync marker ensures that the timing drift requirement can be more usefully restated as:

The transmission time of any individual pulse shall not drift more than 10ns from its nominal transmission time during a 128 symbol period over the specified operating temperature range of the device.

The result of this sync marker is that the 10ns drift limit can be met using a very low cost, widely available AT-cut crystal oscillator. A wider temperature range may require a temperature compensated crystal to meet the drift requirement.