**IEEE P802.15**

**Wireless Personal Area Networks**

|  |  |
| --- | --- |
| Project | IEEE P802.15 Working Group for Wireless Personal Area Networks (WPANs) |
| Title |  UWB based Report in NBA-MMS |
| Date Submitted | July 2023 |
| Source | Mingyu Lee, Taeyoung Ha, Youngwan So, Aniruddh Rao Kabbinale, Clint Chaplin (Samsung Electronics) |
| Re: | Contribution to IEEE 802.15.4ab  |
| Abstract |  |
| Purpose | This submission proposes text to for the IEEE Std 802.15.4ab specification framework document.  |
| Notice | This document does not represent the agreed views of the IEEE 802.15 Working Group or IEEE 802.15.4ab Task Group. It represents only the views of the participants listed in the “Source(s)” field above. It is offered as a basis for discussion and is not binding on the contributing individual(s) or organization(s). The material in this document is subject to change in form and content after further study. The contributor(s) reserve(s) the right to add, amend or withdraw material contained herein. |

## Introduction

In NBA-UWB MMS [15-22-0381-05-04ab], NB 250 kbps is used as default for Report. However, if PTData field of report is long (e.g., 32 byte), it may exceed 1 ms slot duration which is generally used. Among the newly considered UWB data rates, 1.95 Mbps data rate provides enough link budget to support MMS. If UWB 1.95 Mbps is used for report instead of NB 250 kbps, air time for report can be reduced and support 1 ms slot duration easily. In this document we propose the way to provide UWB based report in NBA-UWB

## Proposal

*Revise NB PHY Config in the table of 1.6.3.2 Compressed PSDU message fields* [*15-22-0381-05-04ab*]

|  |  |  |
| --- | --- | --- |
| NB PHY Config | 8 | Sets O-QPSK PHY #1-#9 referring to [1]{#1: 250k uncoded, …, #9}Bits 0-3: NB Control PhaseBits 4-7: NB Report Phase(Bit 4-7 : 0b1111 - NB is not used, UWB for Report) |

Add at the end of the table of 1.6.3.2 Compressed PSDU message fields
[15-22-0381-05-04ab] with the references correspond to [15-23-0307-00-04ab] Table 15-7a [IEEE 802.15.4z] in the following texts.

Note : If Bits 4-7 of NB PHY Config is 0b1111, Set #1 in [15-23-0307-00-04ab] with Code index #32 in Table 15-7a [IEEE 802.15.4z] is default.