|  |  |  |
| --- | --- | --- |
| Project | **IEEE 802.16 Broadband Wireless Access Working Group <**<http://ieee802.org/16>**>** | |
| Title | **System Requirements on Interference Management for IEEE 802.16q Multi-Tier Networks** | |
| Date Submitted | **2012-09-12** | |
| Source(s) | Wooram Shin, Jaesun Cha,  Eunkyung Kim, Anseok Lee,  Kwangjae Lim  ETRI | E-mail: [w.shin@etri.re.kr](mailto:w.shin@etri.re.kr)  \*<<http://standards.ieee.org/faqs/affiliationFAQ.html>> |
| Re: | “IEEE 802.16-12-0507-02-Shet,” in response to Call for Contributions: Multi-Tier Networks IEEE 802.16 Working Group on System Requirmeent of Multi-Tier Networks | |
| Abstract | Proposal regarding System Requirements of Multi-Tier Networks | |
| Purpose | To discuss and adopt the proposed texts in the System Requirements Document (SRD) on IEEE P802.16q Multi-Tier Networks | |
| Notice | *This document does not represent the agreed views of the IEEE 802.16 Working Group or any of its subgroups*. It represents only the views of the participants listed in the “Source(s)” field above. It is offered as a basis for discussion. It is not binding on the contributor(s), who reserve(s) the right to add, amend or withdraw material contained herein. | |
| Release | The contributor grants a free, irrevocable license to the IEEE to incorporate material contained in this contribution, and any modifications thereof, in the creation of an IEEE Standards publication; to copyright in the IEEE’s name any IEEE Standards publication even though it may include portions of this contribution; and at the IEEE’s sole discretion to permit others to reproduce in whole or in part the resulting IEEE Standards publication. The contributor also acknowledges and accepts that this contribution may be made public by IEEE 802.16. | |
| Patent Policy | The contributor is familiar with the IEEE-SA Patent Policy and Procedures:  <<http://standards.ieee.org/guides/bylaws/sect6-7.html#6>> and <<http://standards.ieee.org/guides/opman/sect6.html#6.3>>.  Further information is located at <<http://standards.ieee.org/board/pat/pat-material.html>> and <<http://standards.ieee.org/board/pat>>. | |

# System Requirements on Interference Management for IEEE 802.16q Multi-Tier Networks

Wooram Shin, Jaesun Cha, Eunkyung Kim, Anseok Lee, Kwangjae Lim

ETRI

# Introduction

Recently, a multi-tier network architecture, which allows overlay deployments of several different types of cells (e.g., typically, overlay of a macro cell and several small cells(including micro, pico, femto cell)), has been vigorously studied and several standard development bodies such as IEEE 802.16 [1] have adopted this as a project item due to its potential benefits increment of areal capacity, coverage, and client quality of service (QoS) and also to decrease cost per bit. In order to accomplish those advantages, interference to/from overlaid/adjacent macro cells and adjacent small cells shall be well managed.

A 2-tier arhitecture composed of multiple small cells overlaid by a macro cell is a quite simple, but mostly considered scenario as a multi-tier network. In this architecture, mobile stations(MSs) connected to an overlaid small/macro cell may significantly suffer from interference from overlaying macro/small cell(s) in downlink. Similarly, in uplink, MSs connected to an overlaying small/macro cell may generate strong interference to overlaid macro/small cell(s). In practice, regular hexagonal deployment of base stations(BSs) may not be made, and a large number of small cells could be deployed in a hotspot area, so the effect of interference from adjacent cells becomes severer. Also, strong interference from overlaying cell(s) can degrade the performance of an overlaid cell when traffic offloading from a macro BS to a small BS even though received signal strength (RSS) from the macro BS is higher than that from the small BS. Accordingly, reliable transmission of control channels may not be guaranteed due to such interference from overlaying/adjacent cells, so there would be MSs given under coverage hole. To overcome this problem, coordinated resource(time, frequency, power) management on control channels with overlaying/adjacent BSs shall be supported. As well, in data transmission perspectives, coordinated resource management on data channels also shall be provided to enhance network capacity. It is widely accepted to take into account resource multiplexing, (soft) fractional frequency reuse (FFR), dynamic coordinated scheduling, downlink power setting/control of BSs, and uplink power control of MSs as coordinated resource management schemes for multi-tier networks, and their details are given below.

* A simple approach to discard interference is time/frequency division multiplexing (TDM/FDM), which exclusively dedicates resource(time, frequency) to a specific cell rather than reuses it among mutually overlaying/adjacet cells. It is suitable for the robust transmission such as control channels and data channels requiring high target (bit/block) error rate.
* On the other side, (soft) fractional frequency reuse (FFR) allowing more power on primary partition(s) and less power on the rest of partitions is more efficient than TDM/FDM in terms of resource reuse while permitting not-strong interference from overlaying/adjacent cells. Its gain can be improved when it is configured depending on the amount of load and the strength of interference by adapting the number of partitions, size of each partition, and (maximum) power of each partition. In the baseline standard [2], partial usage of subchannels (PUSC) is used as a sort of FFR with 3 of the number of partitions and equal partion size, but its efficacy may not be feasbile if the number of adjacent cells is larger than 3 and each cell would serve different amount of load or be exposed by different level of interference. Thus, FFR with support of varied settings on the number of partitions, size of each partition, (maximum) power of each partition is required.
* Typically, the configuration of TDM/FDM or FFR stated above statically changes without or with less consideration of small-scale channel variation, but as increase of the number of overlaying/adjacent cells, interference fluctuation becomes more dynamic due to the small-scale channel variation and unpredictable scheduling of other cells. Therefore, link reliability or transmission efficiency decreases, and then network capacity also declines. Those problems can be mitigated using dynamic coordinated scheduling jointly performed by mutually nearby BSs.
* Another approach to suppress interference to MSs connected to overlaid/adajcent cells is downlink transmit power setting/control of small BSs. For example, in downlink, small BSs can increase transmit power to exploit traffic offloading from macro BSs to them, but this may cause strong interference to MSs connected to macro BSs and located near the edge of small cells. In this case, small BSs would decrease or limit transmit power on part of resource(time, frequency) by coordination with overlaid macro BSs.
* In uplink, MSs can suppress interference to BSs in overlaid/adajcent cells by means of uplink transmit power control, by which maximum power level can be constrained not to generate significant level of interference to overlaid/adjacent BSs in a more dynamic fahsion adjusting relatively rapid channel variation.

As increase of the number of cells due to deployment of small cells, the number of cell-edges also increases, so the probability that an MS suffers from strong interference at the cell-edge can increase, which may limit or decrease client QoS. It is well known that cooperative transmission such as coordinated beamforming and collaboritve MIMO is a essential way to resolve those problems. It enhances cell-edge performance by avoiding interference from overlaying/adjacent cells or accomplishing diversity/multiplexing/array gain by joint transmission by multiple BSs.

The interference management schemes stated above can be applied not only solely but also jointly depending on how interference mutually affects or is likely to do.

Coordinated resource management and cooperative transmission can work well under good synchronization (time, frequency) conditions between MS and its overlaid/adjacent BSs as well as between MS and its serving BS. However, due to the overlaid and unstructured deployment of small BSs in multi-tier networks, the arrival time of signals from small cells and that from overlaying macro cell can be different, so it gives rise to frame misaligned. It inherently generates inter-symbol/carrier interference nontherless how well interference management work. Threrefore, synchronization between a macro BS and small BS(s) and between MSs and overlaid/adjacent BSs shall be provided to prevent from being impaired by inter-symbol/carrier interference.

In order to realize such varied interference management schemes, BSs and MSs need to determine feasibility or gain when enabling them, and some schemes necessitate knowledge of interference channel as well as desired channel. Therefore, how to measure and report interference channel from overlaying/adjacent cells or its side information shall be provided to exploit those interference management schemes.

As metioned above, most of interference management schemes require close coordination and cooperation among overlaying/adjacent cells, so it is quite significant to provide which/when/how management information is exchanged among mutually nearby BSs.

# References

1. IEEE 802.16-12-0394-05-Gdoc, PAR and Five Criteris for P802.16q on a Multi-tier Amendment to IEEE Std 802.16, July 2012.
2. IEEE Std 802.16-2012, IEEE Standard for Air Interface for Broadband Wireless Access Systems, Aug. 2012.

# Proposed Texts on Interference Management as Part of System Requirement Document (SRD) for IEEE 802.16q Multi-Tier Networks

[-------------------------------------------------------Start of Text Proposal-------------------------------------------------------]

# X. Functional Requirements

## X.1 Interference Management in Multi-tier Networks

### The 802.16q system shall support interference management by coordination and cooperation among BSs for multi-tier networks.

### X.1.1 The 802.16q system shall provide mechanisms for coordinated resource(time, frequency, power) managment to mitigate inter-cell/tier interference between macro cells, between small cells, and between macro cells and small cells.

### X.1.1.1 The 802.16q system shall provide mechanisms for resource(time, frequency) multiplexing, which limits reuse of resource by overlaying/adjacent cells and exclusively dedicates resource to a specific cell among overlaying/adjacent cells.

### X.1.1.2 The 802.16q system shall provide mechanisms for fractional frequency reuse (FFR) with support of varied settings on the number of frequency partition, size of each partition, and (maximum) power of each partition.

### X.1.1.3 The 802.16q system shall provide mechanisms for dynamic coordinated scheduling to alleviate small-scale interference variation.

### X.1.1.4 The 802.16q system shall provide mechansims for downlink transmit power setting/control of small BS to suppress interference to MSs connected to overlaid/adjacent cells.

### X.1.1.5 The 802.16q system shall provide mechansims for uplink power control of MSs to suppress interference to BSs in overlaid/adjacent cells.

### X.1.2 The 802.16q system shall provide mechansims for cooperative transmission by multiple macro BSs, by multiple small BSs, or by macro BS(s) and small BS(s) to enhance cell-edge performance and client quality of service (QoS) (e.g., coordinated beamforming, collaborative MIMO).

### X.1.3 The 802.16q system shall provide mechansims for synchronization between a macro BS and small BS(s) and between MSs and overlaid/adjacent BSs to prevent from being impaired by inter-symbol/carrier interference.

### X.1.4 The 802.16q system shall provide mechanisms for inter-cell interference channel measurement and report to support interference management by coordination and cooperation among BSs.

### X.1.5 The 802.16q system shall provide mechanisms for management information exchange among BSs to support interference management by coordination and cooperation among BSs.

[-------------------------------------------------------Start of Text Proposal-------------------------------------------------------]