IEEE P802.11  
Radio Regulatory Technical Advisory Group (RR-TAG)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| ISUS Document Mark-up | | | | |
| Date: 2022-08-01 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Rich Kennedy | Huawei Paris |  | +1 737-202-7014 | [rkennedy1000@gmail.com](mailto:rkennedy1000@gmail.com) |
| Amelia Andersdotter | Comcast | Belgium |  | amelia.ieee@andersdotter.cc |

Abstract

This document contains a marked up copy of the IEEE Standards Association (SA) position statement “Intelligent Spectrum Allocation and Management” for review.

It is based on document 18-22-0080r0



IEEE Standards Association Position Statement

Intelligent Spectrum Allocation and Management

*Approved by the*

*IEEE Standards Association Board of Governors*

5 September 2018

The IEEE Standards Association (IEEE-SA) supports the position that intelligent spectrum allocation and management is needed for both licensed and license-exempt technologies to meet the explosive growth in wireless data demand. As both consumer and business wireless data consumption increases, increased access to spectrum with commercially viable rules becomes vital to support data growth.

The IEEE-SA, through its participants, is a major contributor to the standardization of leading wireless technologies. IEEE-SA participants develop wireless standards such as the IEEE 802.111 Wireless LAN (WLAN) family of standards (inclusive of technologies known as Wi-Fi2 and WiGig3) and IEEE Standard

802.15.44 Low Rate Wireless Networks (LRWN) (inclusive of ISA1005, WiSUN6, and Zigbee7), which primarily use license-exempt spectrum. ~~The number of IEEE 802.11 WLAN enabled devices shipped exceeds 15 billion and by 2019 the number of IEEE 802.15.4 LRWN enabled devices are expected to reach 2.1 billion~~~~8~~~~.~~ This high uptake of IEEE 802 standards family of enabled wireless devices [since their conception in the 1990s] is a strong indicator of the importance of license-exempt spectrum as a driver for innovation and economic growth. [Since the first IEEE 802 technologies were developed to operate in a relatively small set of license-exempt spectrum bands, more frequency bands have been made available for unlicensed use. This highlights the important role IEEE 802 technologies play in the lives of individual people, but also in communities and for businesses.]

~~The IEEE-SA recognizes the need for more efficient use of existing and to be allocated spectrum through various spectrum sharing mechanisms. Spectrum sharing can make thousands of megahertz available~~

1 See [http://www.ieee802.org/11/.](http://www.ieee802.org/11/)

2 *Wi-Fi* is the name of a popular wireless networking technology that uses radio waves to provide wireless high- speed Internet and network connections.

3 *WiGig* is a wireless standard developed by the [Wireless Gigabit Alliance.](https://www.wi-fi.org/?utm_source=wigig&utm_medium=referral&utm_campaign=wigig-redirect) It is designed to promote significantly faster speed for wireless network connections.

4 See [http://www.ieee802.org/15/pub/TG4.html.](http://www.ieee802.org/15/pub/TG4.html)

5 See https://isa100wci.org/en-US/About-ISA100-Wireless/What-is-ISA100-Wireless.

6 See https[://w](http://www.wi-sun.org/)ww[.wi](http://www.wi-sun.org/)-[sun.org/.](http://www.wi-sun.org/)

7 See https[://w](http://www.zigbee.org/)ww[.zigbee.org](http://www.zigbee.org/)/[.](http://www.zigbee.org/)

8 See 802.11 device shipment - WiFi Alliance; 802.15.4 device forecast - Telecompetitor report.

~~more quickly and cost effectively than would occur by relocating incumbent users. Sharing can occur in bands that are currently licensed but occupied by temporally or spatially sporadic users, such as in the~~

~~3.5 GHz band in the United States, and TV white space in Colombia, Singapore, South Africa, United Kingdom, and the United States. Notably, the IEEE P802.15.4m~~~~9~~ ~~project, IEEE 802.11af~~~~10~~ ~~amendment, and IEEE 802.22~~~~11~~ ~~Wireless Regional Area Network standard are designed to access TV white space with use cases ranging from low-rate personal-area networks to high-capacity wireless regional-area networks for broadband provisioning. Sharing can also occur in license-exempt bands among devices which utilize either common air interfaces or between devices with disparate air interface technologies.~~

~~Examples of intelligent spectrum sharing techniques involve cognitive radio technologies such as Listen Before Talk utilized in IEEE 802.11 WLAN based Wi-Fi and 3~~~~rd~~ ~~Generation Partnership Project (3GPP) Long Term Evolution (LTE) based Licensed Assisted Access (LAA) systems~~~~12~~~~, the policy- based framework used by the IEEE Dynamic Spectrum Access Networks standards 1900.X~~~~13~~ ~~or spectrum sharing with primary users based on sensing, spectrum database access, and dynamic spectrum access rules used in the IEEE 802.22 TV White Space standard.~~ Cognitive radio technologies and other spectrum sharing techniques should continue to be developed and standardized to establish fair and transparent spectrum sharing among devices that avoids harmful interference. The IEEE-SA, given its history of being a neutral and collaborative standards development organization, can facilitate the development of fora where these common rules and technologies can be standardized.

In addition to intelligent spectrum utilization, the increasing demands for wireless spectrum should also be met by introducing flexibility into the use of lightly used spectrum. This includes spectrum that is being used sparsely on a geographic basis (i.e., only used in certain specific locations) or temporally. In particular, the intelligent management brought about by cognitive radio and other related technologies can assure co-existence with devices and services which currently use these spectrum bands, albeit on a sporadic basis. An example of this is in the United States where in April 2015 the Federal Communications Commission (FCC) issued a Report and Order detailing a new Citizens Broadband Radio Service (CBRS) in the 3550-3700 MHz spectrum band, which reallocated the band so that it can be shared with incumbent radar systems and fixed satellite services using rules specified by the FCC.14 Expanding on this, in 2013 IEEE 802.11 introduced access to unused TV channels with the TV White Space standard, 802.11af, now in use around the globe providing Internet access in underserved communities. Now, with basic access to the 1.2 GHz of the 6 GHz band limited to Very Low Power and Low Power Indoor use, Automatic Frequency Coordination using database determination of victim receiver locations, will enable full power use in this band.

Wireless technology will continue to benefit humanity profoundly. ~~For example, the use of wirelessly connected medical devices is expected to increase significantly in the near future.~~~~15~~ ~~As a result, medical resources can be more rapidly dispatched to where they are needed, and this will positively impact lives.~~

9 See https://standards.ieee.org/findstds/standard/802.15.4m-2014.html.

10 See https://standards.ieee.org/findstds/standard/802.11af-2013.html.

11 See [http://www.ieee802.org/22/.](http://www.ieee802.org/22/)

12 See [http://www.3gpp.org/news-events/3gpp-news/1789-laa\_update.](http://www.3gpp.org/news-events/3gpp-news/1789-laa_update)

13 See [http://grouper.ieee.org/groups/dyspan/.](http://grouper.ieee.org/groups/dyspan/)

14 See https[://w](http://www.fcc.gov/wireless/bureau-divisions/broadband-division/35-ghz-band/35-ghz-band-citizens-)ww[.fcc.gov](http://www.fcc.gov/wireless/bureau-divisions/broadband-division/35-ghz-band/35-ghz-band-citizens-)/[wireless/bureau-divisions/broadband-division/35-ghz-band/35-ghz-band-citizens-](http://www.fcc.gov/wireless/bureau-divisions/broadband-division/35-ghz-band/35-ghz-band-citizens-) broadband-radio.

15 See https[://w](http://www.medicaldesignbriefs.com/component/content/article/mdb/features/28516)ww[.medicaldesignbriefs.com](http://www.medicaldesignbriefs.com/component/content/article/mdb/features/28516)/[component/content/article/mdb/features/28516](http://www.medicaldesignbriefs.com/component/content/article/mdb/features/28516) and https://hitinfrastructure.com/news/healthcare-wireless-network-coverage-capacity-top-challenge

The IEEE-SA has an important role to play in the development of intelligent spectrum allocation and management based upon transparent, standardized rules that also account for incumbent users.

*This statement was developed by the IEEE Standards Association and represents the considered judgement of a group of IEEE standards participants with expertise in the subject field. The position taken by the IEEE Standards Association does not necessarily reflect the views of IEEE or its other Organizational Units.*

**ABOUT IEEE**

The IEEE is the world’s largest professional association advancing innovation and technological excellence for the benefit of humanity. IEEE and its members inspire a global community to innovate for a better tomorrow through its highly-cited publications, conferences, technology standards, and professional and educational activities. IEEE is the trusted “voice” for engineering, computing, and technology information around the globe.

There are more than 420,000 IEEE members in more than 160 countries. IEEE publishes a third of the world’s technical literature in electrical engineering, computer science, and electronics, and is a leading developer of international standards that underpin many of today’s telecommunications, information technology, and power generation products and services.

***ABOUT THE IEEE STANDARDS ASSOCIATION***

*The IEEE Standards Association, a globally recognized standards-setting body within IEEE, develops consensus standards through an open process that engages industry and brings together a broad stakeholder community. IEEE standards set specifications and best practices based on current scientific and technological knowledge. The IEEE-SA has a portfolio of over 1,250 active standards and over 650 tandards under development. For more information visit http://standards.ieee.org.*