|  |  |  |
| --- | --- | --- |
| Project | **IEEE 1900.7 Radio Interface for White Space Dynamic Spectrum Access Radio Systems Supporting Fixed and Mobile Operation <**http://grouper.ieee.org/groups/dyspan/7/index.htm**>** | |
| Title | PHY, MAC, Convergence sublayer within Reference Models | |
| Date Submitted | 2013-04-20 | |
| Source(s) | [Hoang Vinh Dien](http://www.nict.com.sg/hoang.htm), Hiroshi Harada  National Institute of Information and Communications Technology (NICT) | E-mail: [hvdien@nict.com.sg](mailto:hvdien@nict.com.sg); [harada@nict.go.jp](mailto:harada@nict.go.jp) |
| Re: | In response to open call for contributions IEEE 1900.7-12/0063r00 | |
| Abstract | This provides a detail explanation for PHY, MAC, convergence sublayers within reference model for 1900.7 network | |
| Purpose | To be discussed and adapted by WG for draft 1900.7 standard | |
| Notice | This document has been prepared to assist IEEE DYSPAN SC. It is offered as a basis for discussion and is not binding on the contributing individual(s) or organization(s). The material in this document is subject to change in form and content after further study. The contributor(s) reserve(s) the right to add, amend or withdraw material contained herein. | |
| Release | The contributor grants a free, irrevocable license to the IEEE to incorporate material contained in this contribution, and any modifications thereof, in the creation of an IEEE Standards publication; to copyright in the IEEE’s name any IEEE Standards publication even though it may include portions of this contribution; and at the IEEE’s sole discretion to permit others to reproduce in whole or in part the resulting IEEE Standards publication. The contributor also acknowledges and accepts that this contribution may be made public by IEEE DYSPAN SC. | |
| Patent Policy and Procedures | The contributor is familiar with the IEEE Patent Policy and Procedures <http:// ieee802.org/guides/bylaws/sb-bylaws.pdf>, including the statement "IEEE standards may include the known use of patent(s), including patent applications, provided the IEEE receives assurance from the patent holder or applicant with respect to patents essential for compliance with both mandatory and optional portions of the standard." Early disclosure to the Working Group of patent information that might be relevant to the standard is essential to reduce the possibility for delays in the development process and increase the likelihood that the draft publication will be approved for publication. Please notify the Chair <harada@nict.go.jp> as early as possible, in written or electronic form, if patented technology (or technology under patent application) might be incorporated into a draft standard being developed within IEEE DYSPAN SC. **If you have questions, contact the IEEE Patent Committee Administrator at <**[**patcom@ieee.org**](mailto:patcom@ieee.org)**>.** | |

# PHY, MAC, Convergence sublayer within Reference Models

[Hoang Vinh Dien](http://www.nict.com.sg/hoang.htm), Hiroshi Harada

NICT

# Introduction

# This contribution a detail explanation for PHY, MAC, convergence sublayers within reference model for 1900.7 network.

# Text Proposal in IEEE 1900.7 Draft

**[*Remedy 1: Replace the existing text with the following in 1900.7 Draft*]**

*[-------------------------------------------------Start of Text Proposal---------------------------------------------------]*

**5.3.1 PHY, MAC and Convergence sublayer**

The MAC CPS provides the core MAC functionality, manages the system access, including bandwidth allocation, connection management. Data from various CSs goes through MAC SAP and is channelled into various MAC connections.

The PHY includes specifications appropriate to a particular frequency range and application. The PHY specifications are discussed in section 9.

**5.3.2 Security sublayer**

The security sublayer shall guarantee the integrity of the system, shall provide authentication, secure key exchange, and encryption.

**5.3.4 Interface with TV WS database**

The white space database SAP provides the interface to TV WS database which is implementation specific.

**5.3.5 Interface with geolocation device**

This interface consists a set of functions for information exchange with the geolocation device to get the geolocation information. This interface shall follow the IEEE 1900.6a standard.

**5.3.6 Optional Interfaces**

The 1900.7 also specifies three optional interfaces to exchange the information with sensing device, external WS management and WS coexistence system.

- Interface with spectrum sensing device: TBD

- Interface with external WS management: this interface shall follow the 1900.4a standard.

- Interface with WS coexistence system: this interface shall follow the 802.19.1 standard.

*[-------------------------------------------------End of Text Proposal----------------------------------------------------]*

# References

[1] IEEE 1900.7-12/0063r00, “Open call for contributions”

[2] IEEE 1900.7-12/0041r01, “Reference Models and Management Model”

[3] IEEE 1900.7-13/008r00, "Draft 1900.7 standards"