|  |  |
| --- | --- |
| Project | **Specification of Sensor Interface for Cyber and Physical World**  <<https://sagroups.ieee.org/2888.1/> **>** |
| Title | **Syntax and semantics of sensor capability base type** |
| DCN | **2888-21-0004-01-0001** |
| Date Submitted | **Feb. 13th, 2021** |
| Source(s) | Sang-Kyun Kim, [goldmunt@gmail.com](mailto:goldmunt@gmail.com) (Myongji University)  Min Hyuk Jeong, [jmh8900@gmail.com](mailto:jmh8900@gmail.com) (Myongji University)  Hoe Yong Jin, [skydesert6410@gmail.com](mailto:skydesert6410@gmail.com) (Myongji University) |
| Re: |  |
| Abstract | This contribution illustrates the basic JSON schema structure for representing sensor capability base types and attributes in a standardized data format. The semantics and examples of the base types and attributes are presented. |
| Purpose | To start discussion on purpose of the standard |
| Notice | This document has been prepared to assist the IEEE 2888 Working Group. It is offered as a basis for discussion and is not binding on the contributing individual(s) or organization(s). The material in this document is subject to change in form and content after further study. The contributor(s) reserve(s) the right to add, amend or withdraw material contained herein. |
| Release | The contributor grants a free, irrevocable license to the IEEE to incorporate material contained in this contribution, and any modifications thereof, in the creation of an IEEE Standards publication; to copyright in the IEEE’s name any IEEE Standards publication even though it may include portions of this contribution; and at the IEEE’s sole discretion to permit others to reproduce in whole or in part the resulting IEEE Standards publication. The contributor also acknowledges and accepts that IEEE 2888 may make this contribution public. |
| Patent Policy | The contributor is familiar with IEEE patent policy, as stated in [Section 6 of the IEEE-SA Standards Board bylaws](http://standards.ieee.org/guides/opman/sect6.html#6.3) <[http://standards.ieee.org/guides/bylaws/sect6-7.html#6](http://127.0.0.1:4664/cache?event_id=757737&schema_id=1&s=5X0vID10lu_E6yrIkWkNd4Wz2H8&q=hancock)> and in *Understanding Patent Issues During IEEE Standards Development* <http://standards.ieee.org/board/pat/faq.pdf> |

# Introduction

This contribution illustrates the basic JSON schema structure for representing sensor capability base types and attributes in a standardized data format. The semantics and examples of the base types and attributes are presented.

# Data formats for sensor capability base data

## Sensor capability base data

### General

This sub-clause specifies a sensor capability base data.

### Syntax

|  |
| --- |
| "sensorCapabilityBaseData": {  "type": "object",  "properties": {  "id": {  "type": "string"  }  "sensorCapabilityBaseAttributes" : {  "$ref": "#/definitions/sensorCapabilityBaseAttributesType"  },  "accuracyType": {  "type": "object",  "properties": {  "oneOf": [  "percentAccuracy": {  "type": "number",  "minimum": 0.0,  "maximum": 1.0  },  "valueAccuracy": {  "type": "number"  }  ]  }  }  }  },  "sensorCapabilityBaseAttributesType": {  "type": "object",  "properties": {  "unit": {  "$ref": "#/definitions/unitType"  },  "maxValue": {  "type": "number"  },  "minValue": {  "type": "number"  },  "offset": {  "type": "number"  },  "numOfLevels": {  "type": number"  "minimum": 0  },  "sensitivity": {  "type": "number"  },  "snr": {  "type": "number"  },  }  } |

### Semantics

Semantics of the sensorCapabilityBaseData:

| Name | Definition |
| --- | --- |
| SensorCapabilityBaseData | SensorCapabilityBaseData provides a base type for a subset of types defined as part of the sensor device capability metadata types. |
| id | Unique identifier for identifying individual sensor capabilities. |
| sensorCapabilityBaseAttributes | Describes a group of attributes for the sensor capabilities to its actual value in sensorCapabilityBaseAttributesType. |
| accuracyType | Describes the degree of closeness of a measured quantity. Either percentAccuracy or valueAccuracy is chosen. |
| percentAccuracy | Describes the degree of closeness of a measured quantity to its actual value in a relative way using a value ranging from 0 to 1.0. 0 means 0 % accuracy and value 1.0 means 100 % accuracy. |
| valueAccuracy | Describes the degree of closeness of a measured quantity to its actual value in an absolute value of a given unit. The possible range of error as (-value, +value) of given unit. |

Semantics of the sensorCapabilityBaseAttributesType:

| Name | Definition |
| --- | --- |
| unit | Specifies the unit of the sensed value as a reference to a term that shall be using the unitType. |
| maxValue | Describes the maximum value that the sensor can perceive. The terms will be different according to the individual sensor type. |
| minValue | Describes the minimum value that the sensor can perceive. The terms will be different according to the individual sensor type. |
| offset | Describes the number of value locations added to a base value to get to a specific absolute value. |
| numOfLevels | Describes the number of value levels that the sensor can perceive in between maximum and minimum value.  EXAMPLE The value 5 means the sensor can perceive 5 steps from minValue to maxValue. |
| sensitivity | Describes the minimum magnitude of input signal required to produce a specified output signal in a given unit. |
| snr | Describes the ratio of signal power to the noise power corrupting the signal. |

### Examples

This example shows the description of a basic sensing capability with the following semantics. The sensor capability id is "CAP-011". The unit this sensor measures is in meters. "maxValue" is 1000 meters and "minValue" is 0 meters. Since "offset" is 0 and "numOfLevels" is 10, it can be measured in units of 10 meters. Since the "sensitivity" is 5, data is output when more than 5 meters is sensed. "percentAccuracy" is 0.99.

|  |
| --- |
| {  "id" : "CAP-011"  "sensorCapabilityBaseAttributes": {  "unit": "meter",  "maxValue": 1000,  "minValue": 0,  "offset": 0,  "numOfLevels": 10,  "sensitivity": 5  },  "accuracyType": [  "percentAccuracy": 0.99  ]  } |