|  |  |
| --- | --- |
| Project | **Standard for Actuator Interface for Cyber and Physical World**  <https://sagroups.ieee.org/2888/ **>** |
| Title | **Base Data of Actuator Capability** |
| DCN | **2888-21-0027-00-0002** |
| Date Submitted | **June 15, 2021** |
| Source(s) | Yegi Lee [zxcasd312@naver.com](mailto:zxcasd312@naver.com) (Konkuk University)  Shin Kim [new.xin22@gmail.com](mailto:new.xin22@gmail.com) (Konkuk University)  Eunji Choi [c950707@gmail.com](mailto:c950707@gmail.com) (Konkuk University)  Kyoungro Yoon [yoonk@konkuk.ac.kr](mailto:yoonk@konkuk.ac.kr) (Konkuk University) |
| Re: |  |
| Abstract | This contribution proposes the base data of the actuator capability |
| Purpose | To start discussion on purpose of the standard |
| Notice | This document has been prepared to assist the IEEE 2888 Working Group. It is offered as a basis for discussion and is not binding on the contributing individual(s) or organization(s). The material in this document is subject to change in form and content after further study. The contributor(s) reserve(s) the right to add, amend or withdraw material contained herein. |
| Release | The contributor grants a free, irrevocable license to the IEEE to incorporate material contained in this contribution, and any modifications thereof, in the creation of an IEEE Standards publication; to copyright in the IEEE’s name any IEEE Standards publication even though it may include portions of this contribution; and at the IEEE’s sole discretion to permit others to reproduce in whole or in part the resulting IEEE Standards publication. The contributor also acknowledges and accepts that IEEE 2888 may make this contribution public. |
| Patent Policy | The contributor is familiar with IEEE patent policy, as stated in [Section 6 of the IEEE-SA Standards Board bylaws](http://standards.ieee.org/guides/opman/sect6.html#6.3) <[http://standards.ieee.org/guides/bylaws/sect6-7.html#6](http://127.0.0.1:4664/cache?event_id=757737&schema_id=1&s=5X0vID10lu_E6yrIkWkNd4Wz2H8&q=hancock)> and in *Understanding Patent Issues During IEEE Standards Development* <http://standards.ieee.org/board/pat/faq.pdf> |

# Introduction

This contribution proposes the base data of the actuator capability. The actuator base capabilities include delaytime and locator.

Check all of the capabilities related to the actuator: https://www.jsonschemavalidator.net/s/XM3S4I3o

# Data formats for actuator capabilities

* 1. Actuator capability base data
     1. General

This sub-clause specifies a actuator capability base data.

* + 1. Syntax

|  |
| --- |
| {  "actuatorCapabilityBaseData": {  "type": "object",  "properties": {  "id": {  "type": "string"  },  "actuatorCapabilityAttributes": {  "$ref": "#/definitions/actuatorCapabilityAttributesType"  }  },  "additionalProperty": false  },  "definitions": {  "actuatorCapabilityAttributesType": {  "type": "object",  "properties": {  "zerothOrderDelayTime": {  "type": "integer",  "minimum": 0,  "default": 0  },  "firstOrderDelayTime": {  "type": "integer",  "minimum": 0,  "default": 0  },  "locater": {  "$ref": "#/definitions/locationType"/\*TBD\*/  }  },  "additionalProperty": false  }  }  } |

* + 1. Semantics

The semantics of the actuatorCapabilityBaseData:

| Name | Definition |
| --- | --- |
| actuatorCapabilityBaseData | actuatorCapabilityBaseData provides a base type for a subset of types defined as part of the actuator capability metadata types. |
| id | Unique identifier for identifying individual actuator capabilities. |
| actuatorCapabilityAttributes | Describes a group of attributes for the actuator capabilities in actuatorCapabilityAttributes. |

Semantics of the actuatorCapabilityAttributesType:

| *Name* | *Definition* |
| --- | --- |
| zerothOrderDelayTime | Describes required preparation time of a actuator to be activated since it receives a command in the unit of millisecond (ms). If the zerothOrderDelayTime is not specified, the default value is 0. |
| firstOrderDelayTime | Describes the delay time for a actuator to reach the target intensity since it receives a command and is activated in the unit of millisecond (ms). If the firstOrderDelayTime is not specified, the default value is 0. |
| locater | Describes the position of the actuator from the user’s perspective according to the x-, y-, and z-axis as a reference to a term that shall be using the locationType. |

* + 1. Examples

This example shows the description of a basic actuator capability with the following semantics. The actuator capability id is "CAP-001". This deivice requires preparation time of 1 ms to start, and 0 ms to reach target intensity, and is located at the left side.

|  |
| --- |
| {  "actuatorCapabilityBaseData": {  "id": "CAP-001",  "actuatorCapabilityAttributes": {  "zerothOrderDelayTime": 1,  "firstOrderDelayTime": 0,  "locater": "left"  }  }  } |