|  |  |
| --- | --- |
| Project | **Standard for Actuator Interface for Cyber and Physical World**<https://sagroups.ieee.org/2888.2/ **>** |
| Title | **Data Formats for Step Motor Actuator** |
| DCN | **2888-21-0061-02-0002** |
| Date Submitted | **October 12, 2021** |
| Source(s) | Yegi Lee zxcasd312@naver.com (Konkuk University)Shin Kim new.xin22@gmail.com (Konkuk University)Kyoungro Yoon yoonk@konkuk.ac.kr (Konkuk University)Gookhwan Lee ghlee@joyfun.kr (JoyFun Inc.) |
| Re: |  |
| Abstract | This contribution proposes syntaxes, semantics, and examples for representing step motor actuator information in the physical world in a standardized data format. |
| Purpose | To start discussion on purpose of the standard |
| Notice | This document has been prepared to assist the IEEE 2888 Working Group. It is offered as a basis for discussion and is not binding on the contributing individual(s) or organization(s). The material in this document is subject to change in form and content after further study. The contributor(s) reserve(s) the right to add, amend or withdraw material contained herein. |
| Release | The contributor grants a free, irrevocable license to the IEEE to incorporate material contained in this contribution, and any modifications thereof, in the creation of an IEEE Standards publication; to copyright in the IEEE’s name any IEEE Standards publication even though it may include portions of this contribution; and at the IEEE’s sole discretion to permit others to reproduce in whole or in part the resulting IEEE Standards publication. The contributor also acknowledges and accepts that IEEE 2888 may make this contribution public. |
| Patent Policy | The contributor is familiar with IEEE patent policy, as stated in [Section 6 of the IEEE-SA Standards Board bylaws](http://standards.ieee.org/guides/opman/sect6.html#6.3) <[http://standards.ieee.org/guides/bylaws/sect6-7.html#6](http://127.0.0.1:4664/cache?event_id=757737&schema_id=1&s=5X0vID10lu_E6yrIkWkNd4Wz2H8&q=hancock)> and in *Understanding Patent Issues During IEEE Standards Development* <http://standards.ieee.org/board/pat/faq.pdf> |

# Introduction

This contribution proposes actuator command types which can control step motor. It contains syntaxes, semantics, and examples for representing step motor actuator information in the physical world in a standardized data format.

2 Data formats for interfacing actuator command

* 1. **Step motor actuator**
		1. **General**

This sub-clause specifies the actuator command type which can control step motor.

* + 1. **Syntax**

|  |
| --- |
| "stepMotorCommandData": { "type": "object", "properties": { "speed": { "type": "integer", "minimum": 0, }, "steps": { "type": "integer", "minimum": 0, }, "orientation": { "type": "integer", "enum": [1, -1]  } }, "additionalProperties": false }, |

* + 1. **Semantics**

The semantics of the stepMotorCommandData:

|  |  |
| --- | --- |
| *Name* | *Definition* |
| stepMotorCommandData | Provide a structure for describing a command for a step motor actuator. |
| speed | Describes the speed that the step motor actuator shall rotate in RPM (Rotations Per Minute) unit that the specific actuator can generate. |
| steps | Describes the number of steps that the step motor actuator shall rotate through a given angle.e.g., when the fixed step angle of the step motor is 5.625 degrees and the fixed speed variation ratio is 0.015625(1/64), the number of steps for one revolution is (360/5.625)\*64=4,096.e.g., when the fixed step angle of the step motor is 5.625 degrees and the fixed speed variation ratio is 0.015625(1/64), setting steps to 2,048 means the stepper motor is commanded to perform the half revolution rotation. |
| orientation | Describes the orientation that the step motor actuator shall indicate the direction of rotation. If the orientation is 1, it means that the stepper motor rotates counterclockwise, and -1 means that it rotates clockwise. |

* + 1. **Examples**

This example shows the description of the actuator command of step motor with the following semantics. This step motor actuator is commanded to perform the 32 steps to rotate clockwise with the speed of 10 rpm.

|  |
| --- |
| { "commandInfoBaseAttributes": {}, "stepMotorCommandData": { "speed":10, "steps": 32, "orientation": -1 }} |