|  |  |
| --- | --- |
| Project | **HMD based 3D Content Motion Sickness Reducing Technology**  <<http://sites.ieee.org/sagroups-3079/> **>>** |
| Title | **Terminology in Network Aspect** |
| DCN | **21-18-000x-00-1000** |
| Date Submitted | **January 30, 2018** |
| Source(s) | **Namgi KIM** [ngkim@kgu.ac.kr](mailto:ngkim@kgu.ac.kr) **(Kyonggi University),**  **Minseok OH** [msoh@kgu.ac.kr](mailto:msoh@kgu.ac.kr) **(Kyonggi University)** |
| Re: | IEEE 3079 Session #04 in Seoul, Korea |
| Abstract | This document defines terminology used in VR in the aspect of network. |
| Purpose | Working Group Discussion and Acceptance |
| Notice | This document has been prepared to assist the IEEE 3079 Working Group. It is offered as a basis for discussion and is not binding on the contributing individual(s) or organization(s). The material in this document is subject to change in form and content after further study. The contributor(s) reserve(s) the right to add, amend or withdraw material contained herein. |
| Release | The contributor grants a free, irrevocable license to the IEEE to incorporate material contained in this contribution, and any modifications thereof, in the creation of an IEEE Standards publication; to copyright in the IEEE’s name any IEEE Standards publication even though it may include portions of this contribution; and at the IEEE’s sole discretion to permit others to reproduce in whole or in part the resulting IEEE Standards publication. The contributor also acknowledges and accepts that IEEE 3079 may make this contribution public. |
| Patent Policy | The contributor is familiar with IEEE patent policy, as stated in [Section 6 of the IEEE-SA Standards Board bylaws](http://standards.ieee.org/guides/opman/sect6.html#6.3) <[http://standards.ieee.org/guides/bylaws/sect6-7.html#6](http://127.0.0.1:4664/cache?event_id=757737&schema_id=1&s=5X0vID10lu_E6yrIkWkNd4Wz2H8&q=hancock)> and in Understanding Patent Issues During IEEE Standards Development <http://standards.ieee.org/board/pat/faq.pdf> |

# Definition

* **Virtual Reality –** This is a realization of a space similar to reality in which a space and objects according to human imagination are created. In this case, VR means a way to get a new experience getting away from a time and space constraint by using a VR HMD.
* **HMD (Head Mounted Display)** – A device that is worn like a goggle or a helmet on a person's head and through which the image displayed to the front panel can be seen by the wearer.
* **Bit Rate** – The amount of data transmitted through a certain device or a transmission link per a fixed duration. In general, bps (bit per second) is used as a unit.
* **CBR (Constant Bit Rate) encoding** – When referring to codecs, CBR encoding means that the rate at which a codec's output data should be consumed is constant.
* **VBR (Variable Bit Rate) encoding** –As opposed to CBR, VBR files vary the amount of output data per time segment. VBR allows a higher bitrate (and therefore more storage space) to be allocated to the more complex segments of media files while less space is allocated to less complex segments.
* **Frame Rate** – The amount of frames through a certain device or a transmission link per a fixed duration. In general, fps (frame per second) is used as a unit.
* **LOS** (**Line-Of-Sight) propagation** – In LOS, electro-magnetic waves travels in a straight line.
* **NLOS (Non-Line Of Sight) propagation** – Radio transmissions across a path that is partially obstructed, usually by a physical object in the innermost.
* **Jitter** – The deviation from true periodicity of a presumably periodic signal, often in relation to a reference clock signal.
* **Motion-to-photon latency** – Time delay from the HMD user’s movement and the change of view in HMD caused by the movement
* **Motion-to-audio latency** – Time delay from the HMD user’s movement and the change of sound in HMD caused by the movement
* **Multiple VR access users** – More than one user that access a VR system simultaneously at the same space.
* **Motion feedback frequency** – The frequency that an HMD sends collected data, mainly motion, to a VR server.
* **Wireless HMD access distance** – The distance from the VR content server wireless module to the HMD wireless module, and within that distance the VR HMD should display without severe interruption.
* **PER (Packet Error Rate)** – The number of incorrectly received packets divided by the total number of received packets.

