IEEE P802.11
Wireless LANs

|  |
| --- |
| Resolutions for CID 1351: Nseg |
| Date: 2011-05-04 |
| Author(s): |
| Name | Affiliation | Address | Phone | Email |
| Hongyuan Zhang | Marvell | 5488 Marvell Ln, Santa Clara, CA 95054 |  | Hongyuan@marvell.com |

Abstract

This document provides resolution for the comments listed below

Comments are from: 11-11-0276-09-00ac-tgac-d0-1-comments.xls

Comments refer to: Draft P802.11ac\_D0.1.pdf

Changes in the text refer to: Draft P802.11ac\_D0.3.pdf

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| 1351 | Zhang, Hongyuan | 22.3.7 | 91 | 28~32 | Nseg=2 only in one case: 80+80 MHz Noncontiguous frequency segments. It is not clear what "noncontiguous transmission" mean. | Revise Nseg description as: Nseg=2 for 80+80 MHz, and Nseg=1 for all the other cases. |

**Discussions: Agree in principle**

**Need to clarify the non-contiguous transmission is particularly for 80+80.**

***Editor: Please make the following changes in 22.3.7. page 110 lines1~5 in D0.3***

 represents the number of frequency segments in the transmit signal(#900), as defined in

Table 22-4 (Timing-related constants)(#351). ~~ for contiguous transmissions and ~~

~~for non-contiguous transmissions~~  for 80+80 MHz noncontiguous transmission,  for all the other cases;