IEEE P802.11
Wireless LANs

|  |
| --- |
| LB 187 Miscellaneous Comment Resolution |
| Date: 2012-05-15 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Osama Aboul-Magd | Huawei Technologies | 303 Terry Fox DriveOttawa, ONT, Canada | 613-287-1405 | Osama.aboulmagd@huawei.com |
|  |  |  |  |  |

Abstract

This submission includes proposed resolutions to CIDs 4173, 4527, 4528, 4708, and 4717.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| 4173 | 34.20 | 8.3.1.2 |  | "Otherwise the TA field is the address of the STA transmitting the RTS frame." is a duplicate of the normative rule specified on line 16. There is no need for this sentence. | Remove "Otherwise the TA field is the address of the STA transmitting the RTS frame." |

Context:

The TA field is the address of the STA transmitting the RTS frame or a bandwidth signaling TA(#5029). The

TA field is set to a bandwidth signaling TA(#5029) in an RTS frame transmitted by a VHT STA in a non-HT

or non-HT duplicate format to indicate that the scrambling sequence carries the TXVECTOR parameters

CH\_BANDWIDTH\_IN\_NON\_HT and DYN\_BANDWIDTH\_IN\_NON\_HT (see 9.3.2.5a (VHT RTS procedure)).

Otherwise the TA field is the address of the STA transmitting the RTS frame.

Discussion: Agree with the commenter. The last sentence seems redundant and doesn’t provide new information different from that provided at the beginning of the paragraph.

Proposed Resolution: Accepted.

Proposed changes

The TA field is the address of the STA transmitting the RTS frame or a bandwidth signaling TA(#5029). The

TA field is set to a bandwidth signaling TA(#5029) in an RTS frame transmitted by a VHT STA in a non-HT

or non-HT duplicate format to indicate that the scrambling sequence carries the TXVECTOR parameters

CH\_BANDWIDTH\_IN\_NON\_HT and DYN\_BANDWIDTH\_IN\_NON\_HT (see 9.3.2.5a (VHT RTS procedure)).

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| 4708 | 316.01 | C |  |  | The MIB is incomplete. For example, there's no "dot11RMNeighborReportVHTRxHighestSupportedLongGIDataRate" | Make sure the MIB is complete, using the 11n MIB as a starting point |

Proposed Resolution: Rejected. The proposed change doesn’t include sufficient detail.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| 4717 | 1.47 |  |  | Claims to be based on mb/D12.0 but isn't | For example, 118.24 has an asterisk but mb/D12.0 has a multipication sign there; 135.61 should be "reassociation"; etc. (it is impossible to give a complete list of errors, but the doubt has been sown) |

Proposed Resolution: Revised

Instruct the editor to base the next revision of the 802.11ac draft on 802.11-2012 and the appropriate versions of 802.11aa, 802.11ae and 802.11ad.

**References:**