IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Comment resolution of Active Scanning related technical comments | | | | |
| Date: 2013-03-21 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Jarkko Kneckt | Nokia Corporation | Otaniementie 19b, 02150 Espoo Finland |  | [Jarkko.Kneckt@Nokia.com](mailto:Jarkko.Kneckt@Nokia.com) |
| Yunsong Yang | Huawei | 10180 Telesis Court, STE 165  San Diego, CA 92121 |  | yangyunsong@huawei.com |

Abstract

The submission provides a resolution on the technical comments CID222, CID257 and CID281. The comments were given by few volunteers to 802.11ai D0.2 draft. All the comments are listed in the document 11-13-0036r8.

The CID222 are related to use of Reduced Neighbour Report and Neighbor Report.

The CID257 is related to name of the Comrehensive Response criteria.

The CID266, 281 is related to clause 10.1.4.3.6 and cancelling the response with Probe Response.

The text changes of the resolved CID258, CID259, CID260 and CID 283 are included to the resolutions.

**References:**

802.11iai D0.3

11-13-0036r8

Comments: CID222

CID 222:

**Comment:** NeighborReport fild is redundant because of the Reduced Neighbor Report.

**Proposed resolution by commenter:** Remove the NeighborReport field.

**Summary of the comment:**

The comments are related to use of the Neighbor Report and Reduced Neighbor Report elements. The commenters are having two conflicting proposals:

1. Add Neighbor Report element as optional element to the Beacon frame. Add more rules to the Neighbor Report element usage to support the different use cases.
2. Replace the Neighbor Report element by the Reduced Neighbor Report element, because the elements have the same content.

**Discussion:**

The target of the Neighbor Report element is to create an element that contains a minimum mandatory set of information of the network for discovery. The element is designed to be flexible; more parameters of the network and BSS may be added as subelements.

More information may be added to Neighbor Report element as well. However, the mandatory fields of the Neighbor Information element require larger payload. Also it is somewhat arguable that which information elements of neighbour APs should be provided in all scanning frames. The selection of the parameters may have device specific differences. Individually addressed Probe Requests may be applied to request more detailed parameters.

The Reduced Neighbor Report element is designed for scanning. It is already present in Beacon, Probe Response and FILS Discovery frame, while the Neighbor Report element is only present in the Probe Response frame. To simplify implementations, the standard should avoid using multiple information elements for the same operation.

**Resolution:**

The 802.11ai shall use only Reduced Neighbor Report element and delete the Neighbor Report element from Probe Response. The use of the Reduced Neighbor Report element shall be described in normative text. The resolution is implemented in the normative text and comment is pointing to above mentioned CIDs.

CID 257:

**Comment:** Is Comprehensive Response a criteria, i.e. should a STA not respond to a Probe Request if it doesn't have Neighbor's information? This field is more like a request in its nature.

**Discussion:**

The commenter is proposing to rename the Neighbor Report Request. The added information is Neighbor Report information.

**Resolution:**

Agree in Principle. Change "Comprehensive Response" to "Reduced Neighbor Report Request"

CID 266 & 281:

**These comments are discussed in 11-13-259r1**

**Proposed normative text:**

**8.3.3.10 Probe Response frame format**

Instructions to the editor: Delete the element order 71 and renumber the following fields accordingly.

**Table 8-27—Probe Response frame body**

|  |  |  |
| --- | --- | --- |
| Order | Information | Notes |
| ~~72~~ | ~~Neighbor Information~~ | ~~The Neighbor Report element is optionally present if dot11FILSActivated is true~~ |

**8.4.2.178 FILS Request Parameters element**

Instructions to the editor: Change the Comprehensive Response to Neighbor Report Request in figure Figure 8-401cx - FILS Criteria field. Change the first paragraph of below the figure as shown below:

A ~~Comprehensive Response~~ Reduced Neighbor Report Request field value of 1 indicates that the information of other BSSs are requested to be included in the Probe Response frame transmitted in response to the Probe Request. A ~~Comprehensive Response~~ Reduced Neighbor Report Request field value of 0 indicates that such BSS information is not requested.

**10.1.4.3.6 Probe response collision avoidance**

Instructions to the editor: Change the clause as shown below

If a STA with dot11FILSActivated equal to true receives two or more Probe Request frames that meet the criteria to respond as specified in 10.1.4.3.5 (Criteria to respond to probe request) and the STA has dot11OmitReplicateProbeResponses true, the responding STA may cancel the response.

~~respond with a single Beacon or Probe Response frame addressed to broadcast address. The Beacon or the broadcasted Probe Response frame shall contain all the information requested by the responded Probe Request frames.~~ ~~More details on selecting the Probe Response or Beacon frame are described below.~~

~~—~~ ~~STAs with dot11FILSActivated equal to true should respond to one or more Probe Request frames addressed to broadcast address with a Beacon frame if the criteria below is met: T~~

The STA may not respond to Probe Request frames addressed to broadcast address if the responding STA receives an acknowledged probe response addressed to the requesting STA containing the SSID of the responding STA.

The STA should not respond to Probe Request frames addressed to individual or broadcast address if the next TBTT of the responding STA is within dot11BeaconResponseDuration and is no later than any deadline of Probe Response Reception Time if the Probe Response Reception Time element is present in any Probe Request frame.

**10.1.4.3.7 Sending a response to probe request**

Instructions to the editor: Change the fifth paragraph of the clause as shown below

If the ~~Comprehensive Response~~ Reduced Neighbor Report Request field of the FILS Request Parameters element of the Probe Request is set to “1”, the Probe Response or Beacon frame may include information of other BSSs, if the criteria as defined in 10.1.4.3.5.(Criteria to respond to probe request) are met for the included BSS. The BSSs which information is included may have different primary channel as the responding STA. ~~When~~  The information of other BSSs is included~~, one~~ in Reduced Neighbor Report element of the ~~is added to~~ Probe Response or Beacon frame ~~per one reported BSS~~.