IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| LB 191 Comment Resolution – CID 8029 | | | | |
| Date: 2013-02-11 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Osama Aboul-Magd | Huawei Technologies | 303 Terry Fox Drive  Ottawa, ONT, Canada  K2K-3J1 | 613-287-1405 | osama.aboulmagd@huawei.com |
|  |  |  |  |  |

Abstract

This submission includes the proposed resolution of CID 8029.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| CID | Page | Clause | Comment | Proposed Changes | Proposed Resolution |
| 8029 | 372.32 | B.4.23.2 | Static BW operation is mandatory feature and its signaling is carried by non-HT duplicate PPDUs. This inherently suggest that transmission function of non-HT duplicate PPDUs is mandatory for a VHT STA; however, it is not clear whether a VHT STA shall support to transmit non-HT duplicate PPDUs or not. | Add a corresponding row for non-HT duplicate format to PICS (in B.4.23.2) as well as "VHTP2: VHT format". | Rejected: The non-HT duplicate format is supported by HT STAs. Since a VHT STA is also an HT STA, support of non-HT format by a VHT STA is then implied |

Discussion:

The non-HT duplicate format is supported by HT STAs. Since a VHT STA is also an HT STA, support of non-HT format by a VHT STA is then implied. No explicit reference to non-HT format in VHT is needed.**References:**