IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| TGac SB 00 Comment Resolution – Jonathan. | | | | |
| Date: 2013-05-1 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Jonathan Segev | Intel | 94 Em Hamoshavot rd. PTK, Israel | +972-54-2403587 | [jonathan.segev@intel.com](mailto:jonathan.segev@intel.com) |
|  |  |  |  |  |

Abstract

This submission included proposed resolutions to CIDs 10297, 10298, 10300.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| CID |  |  | Comment | Proposed Resolution | Resolution |
| 10297 | 129.42 | 9.7.5.6 | There has been no specification of what a "beamforming steering matrix", nor of what qualifies as such a matrix, before this requirement applying to such matrices. Need a clear definition of this concept and what does and does not qualify as such a thing. | Explicitly specify what is a "beamforming steering matrix" before this point in clause 9. | Reject:  Steering matrix is well defined in 20.3.11.11.2.  There is no requirement to have terminology defined before its usage. A Referance to section 22 may be added to section 3.2 Definitions specific to IEEE 802.11. |

**Discussion:**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| 10298 | 129.53 | 9.7.5.6 | This non-specific "Except as described below" includes the next "Except as described below" -- so, is this an exception to an exception? | On both lines 53 and 57 replace the non-specific "Except as described below" with "Except as specified in the following list of exceptions". | Proposed resolution:  Approve.  Except as described below" with "Except as ~~described below~~ specified in the following exception list". |

**Discussion:**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| 10300 | 130.37 | 9.7.6.1 | The double negative in this version of the sentence makes it non-informative. | Either describe whatever is meant in positive terms (without the double negative) or delete this NOTE. | Proposed resolution:  Aprove.  *NOTE—The rules defined in 9.7.6.2 through 9.7.6.5 apply only to control frames not carried in a A-MPDU or that are carried in a VHT single MPDU.*. |

**Discussion:**