IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Proposed resolutions towards CIDs 1006,1256,1334 and 1371 | | | | |
| Date: 2013-07-16 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Rob Sun | Huawei Canada | 300 Terry Fox Drive, Kanata | +1 613 2781948 | Rob.sun@huawei.com |
|  |  |  |  |  |

Abstract

This submission proposed resolutions towards CIDs 1006, 1255, 1334, and 1371

***Instruct the editor to modify section 3.1 as indicated:***

### 3.1 Definitions

AEAD: a cipher mode that performs authenticated encryption of a plaintext with associated data that is authenticated but not encrypted.

***Instruct the editor to modify section 4.10.3.7 as indicated:***

### 4.10.3.7 AKM operations using FILS authentication without an online trusted third party