IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Comment Resolution for CID 33 | | | | |
| Date: 2013-08-01 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Alfred Asterjadhi | Qualcomm  Inc. | 5775 Morehouse Dr  San Diego,  CA 92109 | +1-858-658-5302 | aasterja@qti.qualcomm.com |

Abstract

This document provides comment resolution for TGah Draft 0.1 Comment Collection 9 with these CIDs: 33.

Interpretation of a Motion to Adopt

A motion to approve this submission means that the editing instructions and any changed or added material are actioned in the TGah Draft. This introduction is not part of the adopted material.

***Editing instructions formatted like this are intended to be copied into the TGah Draft (i.e. they are instructions to the 802.11 editor on how to merge the text with the baseline documents).***

***TGah Editor: Editing instructions preceded by “Instruction to Editor” are instructions to the TGah editor to modify existing material in the TGah draft. As a result of adopting the changes, the TGah editor will execute the instructions rather than copy them to the TGah Draft.***

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **P.L** | **SC** | **Comment** | **Proposed Change** | **Resolution** |
| 33 | 199.34 | 24.1 | ACK Indication field in the SIG field for S1G is used to indicate Response (No, NDP, Normal, Long) rather than ACK. It is also used in the Response Indication Deferral mechanisms. For consistency, rename ACK Indication to Response indication throughout the draft. | As in comment | Revised –  TGah editor to replace “ACK Indication” with “Response Indication” throughout TGah D0.1 as the very last modification to the document to become draft 1.0. |