IEEE P802.11
Wireless LANs

|  |
| --- |
| Comment Collection 09 MAC CIDs (Comment Resolutions for CC09) |
| Date: 2013-09-16 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Shoukang ZHENG | I2R | 1 Fusionopolis Way, Connexis South Tower, Singapore 138632 |  | skzheng@i2r.a-star.edu.sg |
| Zhongding LEI | I2R |  |  | leizd@i2r.a-star.edu.sg |
|  |  |  |  |  |
|  |  |  |  |  |

Abstract

This document provides resolution for CID 856.

Interpretation of a Motion to Adopt

A motion to approve this submission means that the editing instructions and any changed or added material are actioned in the TGah Draft. This introduction is not part of the adopted material.

***Editing instructions formatted like this are intended to be copied into the TGah Draft (i.e. they are instructions to the 802.11 editor on how to merge the text with the baseline documents).***

***TGah Editor: Editing instructions preceded by “Instruction to Editor” are instructions to the TGah editor to modify existing material in the TGah draft. As a result of adopting the changes, the TGah editor will execute the instructions rather than copy them to the TGah Draft.***

Table of Contents

[0 Revision Notes 2](#_Toc350888716)

# 0 Revision Notes

R0: First draft

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Clause** | **Page** | **Line** | **Comment** | **Proposed Change** | **Resolution** |
| 856 | 9.32g.3 | 143 | 29 | It would be more efficient if STA could request/assign TWT in a DATA frame as a response to PS-poll (since DATA is an allowed response frame). | Allow DATA to be a response frame with an indication of Target Wake Time | RejectedReason: The data frame format (either normal frame or Short Data frame) does not include an indication of Target Wake Time but an A-MPDU that includes data frame and TWT frame can be response frame.  |