IEEE P802.11
Wireless LANs

|  |
| --- |
| LB 200 Comment Resolution for Clause 9.12 |
| Date: 2013-11-11 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Alfred Asterjadhi | Qualcomm Inc. | 5775 Morehouse Dr, San Diego, CA 92109 | +1-858-658-5302 | aasterja@qti.qualcomm.com |
| Amin Jafarian | Qualcomm Inc. |  |  | jafarian@qti.qualcomm.com |

Abstract

This submission proposes resolutions for comments in clause 9.12 of TGah Draft 1.0 with the following CIDs:

1725, 1726, 2457

Interpretation of a Motion to Adopt

A motion to approve this submission means that the editing instructions and any changed or added material are actioned in the TGah Draft. This introduction is not part of the adopted material.

***Editing instructions formatted like this are intended to be copied into the TGah Draft (i.e. they are instructions to the 802.11 editor on how to merge the text with the baseline documents).***

***TGah Editor: Editing instructions preceded by “TGah Editor” are instructions to the TGah editor to modify existing material in the TGah draft. As a result of adopting the changes, the TGah editor will execute the instructions rather than copy them to the TGah Draft.***

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **P.L** | **Clause** | **Comment** | **Proposed Change** | **Resolution** |
| 1725 | 164.41 | 9.12.1 | Use of "set to" not according to the Style Guide. | Replace "with multiple MPDUs with Protocol Version field in the Frame Control field set to 1," with "with multiple MPDUs whose Protocol Version subfield value is 1,". | Agree with the commenter. Revised – TGah editor to make changes shown in 11-13-1432-00-00ah under the heading for CID 1725. |
| 1726 | 164.61 | 9.12.3 | Removing "n HT STA and a DMG" from "An HT STA and a DMG STA shall not start the transmission of more than one MPDU" changes legacy 802.11 requirements. | Remove this deletion of legacy requirements. | Rejected –The deletion of “n HT STA and a DMG” is present in 802.11ac D5.0 to which the proposed changes refer to, and is not a modification proposed in D1.0 of .11ah. Hence, the comment is related to .11ac D5.0 rather than D1.0 of .11ah.  |
| 2457 | 165.11 | 9.12.3 | Why is this being reworded as being about PPDUs rather than STAs? | Follow the baseline terminology | Rejected –The rewording in 9.12.3 was already present in 802.11ac D5.0. For 11ah the only modification to D5.0 of .11ac is to append “and in 24.5 (Parameters for S1G-MCSs) for S1G PPDUs” |

**Discussion:** *Proposed changes to subclause 9.12.3 in D1.0 of 802.11ah take as baseline 802.11ac D5.0 (indicated in instructions to the editor). Comments 1726 and 2457 refer to modifications to the spec text introduced in 802.11ac D5.0 rather than modifications to the spec introduced in 802.11ah D1.0.*

* **A-MPDU contents**

**Instruction to TGah Editor:*****Modify the paragraph below as follows:***

When an A-MPDU contains multiple MPDUs whose Protocol Version field value is 1, the values of EOSP and Relayed Frame fields in the Frame Control field, and A3 Present, A4 Present subfields in the SID field shall be identical across MPDUs within the A-MPDU.