IEEE P802.11
Wireless LANs

|  |
| --- |
| LB 200 BSS-Max-Idle-Period-Management comment resolution |
| Date: 2013-xx-xx |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Haiguang Wang  | I2R |  |  | hwang@i2r.a-star.edu.sg  |
| Zander Lei | I2R |  |  | leizd@i2r.a-star.edu.sg  |

Abstract

This submission proposes resolution for the comment with CID 2485 on clause 10.24.13

Interpretation of a Motion to Adopt

A motion to approve this submission means that the editing instructions and any changed or added material are actioned in the TGah Draft. This introduction is not part of the adopted material.

***Editing instructions formatted like this are intended to be copied into the TGah Draft (i.e. they are instructions to the 802.11 editor on how to merge the text with the baseline documents).***

***TGah Editor: Editing instructions preceded by “TGah Editor” are instructions to the TGah editor to modify existing material in the TGah draft. As a result of adopting the changes, the TGah editor will execute the instructions rather than copy them to the TGah Draft.***

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Page** | **Clause** | **Comment** | **Proposed Change** | **Resolution** |
| 2485 | 226.08 | 10.24.13 | The changes indicated suggest the baseline is "If dot11MaxIdlePeriod is a nonzero is true". This can't be right | Make sure the change tracking is accurate. Otherwise the reviewing won't be accurate either | Agreed with the commenter. Revised – Change as suggested; underline the words “is true”. |

***TGah editor: Underline “is true” (highlighted phrase only) in the sub-clause 10.24.13 as the following:***

**10.24.13 BSS Max idle period management**

If the value of dot11MaxIdlePeriod at a STA is ~~a~~ nonzero or dot11S1GOptionImplemented is true, the STA shall include the BSS Max Idle Period element in transmitted the Association Response ~~frame or the~~ and Reassociation Response frames. Otherwise, the STA shall not include the BSS Max Idle Period element in ~~the~~ transmitted Association Response ~~frame or~~ and ~~the~~ Reassociation Response frames. ~~A STA may send security protocol protected or unprotected keep-alive frames, as indicated in the Idle Options field.~~