IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Some 11ak EtherType Frame Encoding Text | | | | |
| Date: 2014-03-20 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | Email |
| Donald Eastlake | Huawei Technologies | 155 Beaver Street, Milford, MA 01757, USA | +1-508-333-2270 | d3e3e3@gmail.com |
|  |  |  |  |  |

Abstract

This document provides some tentative text concerning recognizing General Link (GLK) STAs, basic properties of GLK STAs, their use of EtherType frame encoding (EPD, etc., for a P802.11ak draft. It uses Draft P802.11REVmc\_D2.4 as its base document.

**Editor’s notes**

The editor’s notes do not form a part of this standard. They will be removed before publication. Please do not comment on editor’s notes in any ballot on the draft, as these comments would have no effect on the published standard.

***Editor’s Note: Editor’s Notes in the body of the standard appear like this. They will be removed before*** ***publication. They indicate some item of work or comment that will be addressed prior to publication.***

***This text is based on 802.11REV-mc D2.3 and will need to be revised in light of 802.11 amendments not incorporated in that draft and adopted after that draft but before P802.11ak.***

**Table of Contents**

Introduction 7

1 Overview 7

1.1 Scope 7

1.2 Purpose 7

1.3 Supplementary Information on Purpose 7

1.4 Word Usage 7

1.5 Mathematical Usage 7

2 Normative references 7

3 Definitions, acronyms, and abbreviations 8

3.1 Definitions 8

3.2 Definitions specific to IEEE 802.11 8

3.3 Abbreviations and acronyms 8

4 General Description 8

4.1 General description of the architecture 8

4.2 How wireless local area networks (WLANs) are different 8

4.2.1 Introduction 8

4.2.2 Wireless station (STA) 8

4.2.3 Media impact on design and performance 9

4.2.4 The impact of handling mobile STAs 9

4.2.5 Interaction with other IEEE 802® layers 9

4.2.6 Interaction with non-IEEE-802 protocols 9

4.3 Components of the IEEE Std 802.11 architecture 9

4.3.1 General 9

4.3.2 The independent BSS 9

4.3.3 The personal BSS 9

4.3.4 STA membership in a BSS is dynamic 9

4.3.5 Distribution system (DS) concepts 9

4.3.5.1 Overview 9

4.3.5.2 Extended service set (ESS): The large coverage network 9

4.3.5.3 Robust security network association (RSNA) 9

4.3.5.4 Centralized coordination service set (CCSS) and extended centralized AP or PCP cluster (ECAPC) within the DMG 9

4.3.6 Area conepts 10

4.3.7 Integration with wired LANs 10

4.3.8 QoS BSS 10

4.3.9 Wireless LAN Radio Measurements 10

4.3.10 Operation in licensed frequency bands 10

4.3.11 High throughput (HT) STA 10

4.3.12 Very high throughput (VHT) STA 10

4.3.13 STA transmission of Data frames outside the context of a BSS 10

4.3.14 Tunneled direct-link setup 10

4.3.15 Wireless network management 10

4.3.16 Subscription service provider network (SSPN) interface 10

4.3.17 Mesh BSS: IEEE Std 802.11 wireless mesh network 10

4.3.18 DMG STA 10

4.3.19 DMG Relay 10

4.3.20 Robust audio video (AV) streaming 10

4.3.21 General Link (GLK) concepts 10

4.3.21.1 General 10

4.3.21.2 GLK MSDU Encoding 11

4.3.21.3 GLK SSes 11

4.4 Logical service interfaces 14

4.4.1 General 14

4.4.2 SS 15

4.4.3 PBSS control point service (PCPS) 15

4.4.4 DSS 15

4.5 Overview of the services 15

4.6 Multiple logical address spaces 15

4.7 Differences among ESS, PBSS, and IBSS LANs 15

4.8 Differences between ESS and MBSS LANs 15

4.9 Reference model 15

4.10 IEEE Std 802.11 and IEEE Std 802.1X-2010 15

4.11 Generic advertisement service (GAS) 15

5 MAC service definition 15

5.1 Overview of MAC services 15

5.1.1 Data service 15

5.1.1.2 Determination of UP 15

5.1.2 Security services 16

5.1.3 MSDU ordering 16

5.1.4 MSDU format 16

5.1.5 MAC data service architecture 16

5.2 MAC data service specification 16

5.2.1 General 17

5.2.2 MA-UNITDATA.request 17

5.2.2.2 Semantics of the service primitive 17

5.2.3 MA-UNITDATA.indication 17

5.2.3.2 Semantics of the service primitive 17

5.2.4 MA-UNITDATA-STATUS.indication 17

5.2.4.2 Semantics of the service primitive 17

6 Layer management 18

6.1 Overview of management model 18

6.2 Generic management primitives 18

6.3 MLME SAP interface 18

6.3.3 Scan 18

6.3.3.2.2 Semantics of the service primitive 18

6.4 MAC state generic convergence function (MSGCF) 20

6.5 PLME SAP interface 20

7 PHY service specification 20

8 Frame formats 20

8.1 General requirements 20

8.2 MAC frame formats 20

8.3 Format of individual frame types 20

8.3.1 Control frames 20

8.3.2 Data frames 20

8.3.3 Management frames 20

8.3.4 Extension frames 20

8.4 Management and Extension frame body components 20

8.4.1 Fields that are not elements 20

8.4.1.4 Capability Information field 20

8.4.2 Elements 21

8.4.2.3 Supported Rates element 21

8.4.2.30 TCLAS Element 21

8.4.2.127.2 DMG STA Capability Information field 22

8.4.2.147 Relay Capabilities element 23

8.4.3 Information Subelements 23

8.4.4 Access network query protocol (ANQP) elements 23

8.5 Fields used in Management and Extension frame bodies and Control frames 23

8.6 Action frame format details 23

8.7 Aggregate MPDU (A-MPDU) 23

9 MAC sublayer functional description 23

9.1 Introduction 23

9.2 MAC architecture 23

9.2.1 General 23

9.2.2 DCF 23

9.2.3 PCF 23

9.2.4 Hybrid coordination function (HCF) 23

9.2.4.2 HCF contention based channel access (EDCA) 23

9.2.5 Mesh coordination function (MCF) 24

9.2.6 Combined use of DCF, PCF, and HCF 24

9.2.7 Fragmentation/defragmentation overview 24

9.2.8 MAC data service 24

9.3 DCF 25

9.4 PCF 25

9.5 Fragmentation 25

9.6 Defragmentation 25

9.7 Multirate support 25

9.8 MSDU transmission restrictions 25

9.9 HT Control field operation 25

9.10 Control Wrapper operation 25

9.11 A-MSDU operation 25

9.12 A-MPDU operation 25

9.13 PPDU duration constraint 25

9.14 DMG A-PPDU operation 25

9.15 LDPC operation 25

9.16 STBC operation 25

9.17 Short GI operation 25

9.18 Greenfield operation 25

9.19 Group ID and partial AID in VHT PPDUs 25

9.20 Operation across regulatory domains 25

9.21 HCF 25

9.22 Mesh coordination function (MCF) 25

9.23 Block acknowledgement (block ack) 25

9.24 No Acknowledgement (No Ack) 26

9.25 Protection mechanisms 26

9.26 MAC frame processing 26

9.27 Reverse direction protocol 26

9.28 PSMP Operation 26

9.29 Sounding PPDUs 26

9.30 Link adaptation 26

9.31 Transmit beamforming 26

9.32 Antenna selection (ASEL) 26

9.33 Null data packet (NDP) sounding 26

9.34 Mesh forwarding framework 26

9.35 DMG channel access 26

9.36 DMG AP or PCP clustering 26

9.37 DMG beamforming 26

9.38 DMG block ack with flow control 26

9.39 DMG link adaptation 26

9.40 DMG dynamic tone pairing (DTP) 26

9.41 DMG relay operation 26

9.42 GLK operation 26

10 MLME 27

11 Security 27

12 Fast BSS transition 27

13 MLME Mesh procedures 27

13.1 Mesh STA dependencies 27

13.2 Mesh discovery 27

13.3 Mesh peering management (MPM) 27

13.4 Mesh peering management finite state machine (MPM FSM) 27

13.5 Authenticated mesh peering exchange (AMPE) 27

13.6 Mesh group key handshake 27

13.7 Mesh security 27

13.8 Mesh path selection and metric framework 27

13.9 Airtime link metric 27

13.10 Hybrid wireless mesh protocol (HWMP) 27

13.11 Interworking with the DS 27

13.11.1 Overview of interworking between a mesh BSS and a DS 27

13.11.2 Gate announcement (GANN) 28

13.11.3 Data forwarding at proxy mesh gates 28

13.11.4 Proxy information and proxy update 28

13.11.5 Mesh STA collocation 28

13.12 Intra-mesh congestion control 28

13.13 Synchronization and beaconing in MBSSs 28

13.14 Power save in mesh BSS 28

14 Frequency-Hopping spread spectrum (FHSS) PHY specification for the 2.4 GHz industrial, scientific, and medical (ISM) band 28

15 Infrared (IR) PHY specification 28

16 DSSS PHY specification for the 2.4 GHz band designated for ISM applications 28

17 High rate direct sequence spread spectrum (HR/DSSS) PHY specification 28

18 Orthogonal frequency division multiplexing (OFDM) PHY specification 28

19 Extended Rat PHY (ERP) specification 29

20 High Throughput (HT) PHY specification 29

21 Directional multi-gigabit (DMG) PHY specification 29

22 Very High Throughput IVHT) PHY 29

Annex A, Bibliography 29

Annex B, Protocol Implementation Conformance Statement (PICS) 29

Annex C, ASN.1 encoding of the MAC and PHY MIB 29

… 29

Annex P, Integration Function 29

P.1 Introduction 29

P.2 Ethernet V2.0/IEEE Std 802.3 LAN integration function 30

P.3 Example 30

P.4 Integration service versus bridging 30

… 30

Annex V, Interworking with external networks 30

V.1 General 30

V.2 Network discovery and selection 30

V.3 QoS mapping guidelines for interworking with external networks 30

V.3.3 Example of QoS mapping from different networks 30

V.4 Interworking and SSPN interface support 31

V.5 Interworking with external networks and emergency call support 31

V.6 Peer information 31

… 31

NOTE — The editing instructions contained in this amendment define how to merge the material contained therein into the existing base standard and its amendments to form the comprehensive standard.

The editing instructions are shown in ***bold italic***. Four editing instructions are used: ***change***, ***delete***, ***insert***, and ***replace***. Change is used to make corrections in existing text or tables. The editing instructions specify the location of the change and describe what is being changed by using ~~strike through~~ (to remove old material) and underscore (to add new material). ***Delete*** removes existing material. ***Insert*** adds new material without disturbing the existing material. Insertions may require renumbering. If so, renumbering instructions are given in the editing instruction. ***Replace*** is used to make changes in figures or equations by removing the existing figure or equation and replacing it with a new one. Editorial notes will not be carried over into future editions because the changes will be incorporated into the base standard.

# Introduction

This section will not be included when P802.11ak is rolled into the base standard.

IEEE Std 802.11 was originally designed with the assumption that non-AP non-mesh STAs would be leaf nodes of the network. This amendment optionally extends the 802.11 standard so that communication between STAs are usable as a transit link inside a general network conformant to IEEE Std 802.1Q.

# Overview

## Scope

## Purpose

## Supplementary Information on Purpose

***Add the following at the end of Clause 1.3:\***

* Define the mechanisms for using IEEE 802.11 media as transit links in a bridged LAN.

## Word Usage

## Mathematical Usage

# Normative references

***Insert the following references (maintaining alphabetic order):***

IEEE Std 802.1AC-20XX, “Media Access Control (MAC) Service Definition”

IEEE Std 802.1Qbz™-20XX, “Virtual Bridged Local Area Networks — Amendment: Enhancements to Bridging of 802.11 Media”

# Definitions, acronyms, and abbreviations

## Definitions

***Insert the following definitions (maintaining alphabetical order):***

EtherType Protocol Discrimination (EPD): A frame format that uses an EtherType to identify the protocol of the following information.

**LLC Protocol Discrimination (LPD):** A frame format that uses a destination LSAP, a source LSAP, and a Control octet (LLC) to identify the protocol of the following information.

## Definitions specific to IEEE 802.11

***Insert the following definition (maintaining alphabetical order):***

**General link (GLK):** Communication between two stations (STAs) over the wireless medium suitable for use as a link in the middle of an IEEE Std. 802.1Q conformant network.

## Abbreviations and acronyms

***Insert the following acronyms (maintaining alphabetical order):***

EPD EtherType Protocol Discrimination

GLK General Link

LPD LLC Protocol Discrimination

MSAP MAC Service Access Point

# General Description

## General description of the architecture

## How wireless local area networks (WLANs) are different

### Introduction

### Wireless station (STA)

***Change the first paragraph as follows:***

~~In the design of wired LANs it is implicitly assumed that an address is equivalent to a physical location. In wireless networks, this is not always the case.~~ In IEEE Std 802.11, the addressable unit is a station (STA). The term implies no more than the origin or/and destination of a message. Physical and operational characteristics are defined by modifiers that are placed in front of the term STA. For example, in the case of location and mobility, the addressable units are the fixed STA, the portable STA, and the mobile STA. The STA is a message destination, but not (in general) a fixed location.

### Media impact on design and performance

### The impact of handling mobile STAs

### Interaction with other IEEE 802® layers

### Interaction with non-IEEE-802 protocols

## Components of the IEEE Std 802.11 architecture

### General

### The independent BSS

### The personal BSS

### STA membership in a BSS is dynamic

### Distribution system (DS) concepts

#### Overview

***Change text as follows:***

PHY limitations determine the direction station-to-station distance that may be supported. For some networks this distance is sufficient; for other networks, increased coverage is required. Clause 4.3.5 discusses the DS and ESS as one means of expanded range and the ESS Portal as one means of connectivity to non-802.11 networks in the context of STAs that are not General Link (GLK) STAs. Clause 4.3.21 discusses the GLK STA alternative means to accomplish these goals.

#### Extended service set (ESS): The large coverage network

#### Robust security network association (RSNA)

#### Centralized coordination service set (CCSS) and extended centralized AP or PCP cluster (ECAPC) within the DMG

### Area concepts

### Integration with wired LANs

To integrate the IEEE Std 802.11 non-GLK architecture with a non-IEEE Std 802.11 LAN, including a traditional wired LAN, a final *logical* architectural component is introduced—a *portal*. A portal is not used in the GLK 802.11 architecture (see 4.3.21).

### QoS BSS

### Wireless LAN Radio Measurements

### Operation in licensed frequency bands

### High throughput (HT) STA

### Very high throughput (VHT) STA

### STA transmission of Data frames outside the context of a BSS

Note: I am told that users of this service are anxious to save every bit they can. Thus it is possible they will want to use 802.11ak (EtherType) formatted data frames.

### Tunnelled direct-link setup

### Wireless network management

### Subscription service provider network (SSPN) interface

### Mesh BSS: IEEE Std 802.11 wireless mesh network

### DMG STA

### DMG Relay

### Robust audio video (AV) streaming

Insert a new sub-Clause at the end of Clause 4.3 as follows:

### General Link (GLK) concepts

#### General

GLK STAs are extended non-GLK STAs such that a link between GLK STAs is suitable, insofar as the capabilities of 802.11 wireless permit, to be used as a transit link in the interior of an IEEE Std 802.1Q conformant network.

Every STA is either a GLK STA or a non-GLK STA. A GLK STA is also an HT STA and a QoS STA. GLK STAs advertise themselves as such through the use of the GLK bit in the Capability Information field (see 8.4.1.4) or the GLK bit in the DMG Capabilities Information field (see 8.4.2.127.2). For a GLK STA, dot11GeneralLink is true. For a non-GLK station, dot11GeneralLink is false or absent.

A GLK STA does not attempt to form an infrastructure, IBSS, or PBSS association or mesh peering with any non-GLK STA. If a non-GLK STA attempts to associate with a GLK AP, the GLK AP will refuse the association. If a non-GLK mesh STA attempts to peer with a GLK mesh STA, the GLK STA will refuse the peering.

#### GLK MSDU Encoding

IEEE Std 802.1Q requires EPD MSDU encoding. Thus a transit IEEE Std 802.11 link using the LPD required in previous 802.11 standards would have to convert from EPD to LPD on entry to the 802.11 link and from LPD to EPD on exit. Especially as such links may be in the interior of complex networks, it is anticipated that the MSDUs will sometimes include multiple tags, includes new tags to be defined in the future. However, conversion between EPD and LPD formats in either direction requires knowledge of at least the lengths of all tags that might be encountered within the MSDUs being converted, which would be impossible in general.

Thus, while all non-GLK STAs use LPD and interpret Priority Code Points according to IEEE Std 802.1D, all GLK STAs use EPD and interpret Priority Code Points according to IEEE Std 802.1Q.

#### GLK SSes

##### Provision of the MAC service

To provide transit service suitable for use within an 802.1Q conformant network, it is essential that the 802.1AC MAC service be provided at the interface to such transit service. The exact service provided at the ends of an 802.11 association, for example from a non-AP STA to an AP, has not been precisely specified in pervious revisions of 802.11; the point of convergence between non-GLK 802.11 and other network types is the integration service and it was not assumed that any other points within 802.11 networks would interconnect with non-802.11 networks.

GLK STAs provide access to the WM via one or more MSAPs.

In all figures in 4.3.21.3, items labelled “802.1Q Bridge” can actually by anything offering the services of an 802.1Q conformant network, such as an 802.1Q bridged LAN.

##### GLK IBSS and PBSS

Figure 4-12A shows a GLK IBSS involving two GLK STAs. Each participating STA provides the MAC service via an MSAP. For example, each of the STAs shown could be part of a laptop computer with the STA providing, via the MSAP, access to the link to the other STA and thence to the other laptop. A difference from non-GLK 802.11 is that either or both of the MSAPs could be connected to an 802.1Q bridge or network providing 802.1Q conformant service that, in turn could be connected to one or more end stations. The two MSAPs shown could even be safely connected to the same 802.1Q conformant network since one service provided by such a network is protection from loops.

**Figure 4-12A—GLK IBSS**

GLK

STA

GLK

STA

(MSAP)

(MSAP)

A GLK PBSS similarly provides two linked instances of the MAC service.


##### GLK infrastructure BSS

An example GLK infrastructure BSS is show in Figure 4-12B. The MAC service is provided via the MSAPs shown. These multiple GLK AP MSAPs may be logical entities implemented as a single interface that accepts a vector of destinations as a parameter.


Although transmissions by an AP are typically received by all STAs associated with that AP, the service provided by a GLK infrastructure BSS is intended to be equivalent, insofar as practical, to separate point-to-point links between the GLK AP and each associated GLK STA. Provision of such apparent point-to-point links is natural for MSDUs that are unicast. To provide such apparent point-to-point links for multi-destination MSDUs requires that the GLK AP be able to transmit them so that they are accepted by an arbitrary subset of the associated GLK STAs. Such selective transmission is provided through the CBA-MSDU facility (see 8.3.2.3).

Reasons for such selective transmission include the MAC service requirement that, when an MSDU is transmitted, it is not returned to the transmitting end station. When a non-AP STA associated with a GLK AP sends a group addressed MSDU to that AP, the AP retransmits it but can use the selective transmission facility to stop the originating GLK non-AP STA from accepting it. Also, since the AP MSAPs may connect to an 802.1Q Bridge, loop prevention can require blocking traffic to one or more of the associated GLK non-AP STAs. Such blocking can be implemented by the selective transmission facility.

**Figure 4-12B—GLK infrastructure BSS**



A GLK ESS can be constructed from GLK BSSes, for example as shown in the middle of Figure 4-12C. There is no portal in a GLK ESS. The concept of the DS is roughly replaced, for a GLK ESS, by an 802.1Q conformant network; however, the GLK ESS topology is more general. For example, as shown in Figure 4-12C, a GLK ESS can be formed of GLK BSSes connected by 802.1Q Bridged LANs connected in some cases to an MSAP provided by a GLK AP and in other cases provided by a GLK non-AP STA.



**Figure 4-12C—GLK ESS**

## Logical service interfaces

### General

***Change text as follows:***

A DS may be created from many different technologies or combinations of technologies including ~~current~~ IEEE 802.1Q bridging ~~wired LANs~~ or IETF IP routing. IEEE Std 802.11 does not constrain the DS to be either data link or network layer based. Nor does IEEE Std 802.11 constrain a DS to be either centralized or distributed in nature.

### SS

### PBSS control point service (PCPS)

### DSS

## Overview of the services

### General

### Distribution of messages with a DS

#### Distribution

***Change text as follows:***

This is the primary service used by IEEE Std 802.11 non-GLK STAs. It is conceptually invoked by every data message to or from an IEEE Std 802.11 non-GLK STA operating in an ESS (when the frame is sent via the DS). Distribution is via the DSS.

***Change to name of 4.5.3 as follows:***

### Services that support the ~~distribution service~~ DS, GLK ESSes, and PCP service

#### General

#### Mobility Types

#### Association

***Change text as follows:***

In the non-GLK case, to deliver a message within a DS, the distribution service needs to know which AP to access for the given IEEE Std 802.11 STA. This information is provided to the DS by the concept of association. Association is necessary, but not sufficient, to support BSS-transition mobility. Association is sufficient to support no-transition mobility. Association is one of the services in the DSS.

Before a STA is allowed to send a data message via an AP, it first becomes associated with the AP. The act of becoming associated invokes the association service, which provides the STA to AP mapping to the DS in the non-GLK case or creates or enables a corresponding MSAP on the GLK AP in the GLK case. The DS uses this information to accomplish its message distribution service. How the information provided by the association service is stored and managed within the DS is not specified by this standard.

#### Reassociation

***Change text as follows:***

Association is sufficient for no-transition message delivery between IEEE Std 802.11 STAs. Additional functionality is needed to support BSS-transition mobility. The additional required functionality is provided by the reassociation service. In the non-GLK case, reassociation is one of the services in the DSS.

The reassociation service is invoked to “move” a current association from one AP to another. In the non-GLK case, this keeps the DS informed of the current mapping between AP and STA as the STA moves from BSS to BSS within an ESS. In the GLK case, such a BSS-transition results in the removal or disablement of the corresponding MSAP provided by the from GLK AP and the creation or enablement of a corresponding MSAP provided by the to GLK AP. Reassociation also enables changing association attributes of an established association while the STA remains associated with the same AP. Reassociation is always initiated by the non-AP STA.

#### Disassociation

***Change text as follows:***

The disassociation service is invoked when an existing association is to be terminated. In the non-GLK case, disassociation is one of the services in the DSS.

In an non-GLK ESS, this tells the DS to void existing association information. Attempts to send messages via the DS to a disassociated STA will be unsuccessful. For a GLK AP, disassociation removes or disables the corresponding MSAP being provided by that GLK AP.

### Access control and data confidentiality services

### Spectrum Management services

### Traffice differentiation and QoS support

### Support for higher layer timer synchronization

### Radio measurement service

### Interworking with external networks

## Multiple logical address spaces

***Change text as follows:***

The IEEE Std 802.11 choice of address space implies that for many instantiations of the IEEE

Std 802.11 architecture, the wired LAN MAC address space and the IEEE Std 802.11 MAC

address space might be the same. In those situations where a DS that uses MAC level IEEE 802

addressing is appropriate, all three of the logical address spaces used within a system could be identical. While this is a common case, it is not the only combination allowed by the architecture. The IEEE Std 802.11 architecture allows for all three logical address spaces to be distinct. However, in the GLK case, all three address spaces are the IEEE 802 48-bit address space.

## Differences among ESS, PBSS, and IBSS LANs

## Differences between ESS and MBSS LANs

## Reference model

## IEEE Std 802.11 and IEEE Std 802.1X-2010

## Generic advertisement service (GAS)

# MAC service definition

## Overview of MAC services

### Data service

#### 5.1.1.2 Determination of UP

Change text as follows:

The QoS facility supports eight priority values, referred to as UPs. The values a UP may take are the integer values from 0 to 7 and are identical to the IEEE Std 802.1D priority ~~tags~~ values for non-GLK STAs and to the IEEE Std 802.1Q priority values for GLK STAs. An MSDU with a particular UP is said to belong to a traffic category (TC) with that UP. The UP is provided with each MSDU at the medium access control service access point (MAC\_SAP) either directly, in the UP parameter, or indirectly, in a TSPEC or SCS Descriptor element designated by the UP parameter.

### Security services

### MSDU ordering

### MSDU format

***Change Clause 5.1.4 as follows:***

~~This standard is part of the IEEE 802 family of LAN standards, and as such~~ All ~~all~~ MSDUs sent by non-GLK STAs use LPD ~~are LLC PDUs~~ as defined in IEEE Std 802.1Qbz~~ISO/IEC 8802-2: 1998~~. In order to achieve interoperability between non-GLK STAs and networks using EPD, implementers are recommended to apply the procedures described in ISO/IEC Technical Report 11802-5:1997(E) (previously known as IEEE Std 802.1H-1997 [B21]), along with a selective translation table (STT) that handles a few specific network protocols, with specific attention to the operations required when passing MSDUs to or from LANs or operating system components that use EPD ~~the Ethernet frame format~~. Note that such translations might be required in a STA.

All GLK STA MSDUs use EPD as specified in IEEE Std 802.1Qbz.

### MAC data service architecture

***Change text as follows:***

During reception, a received Data frame goes through processes of possible A-MPDU deaggregation, MPDU header and cyclic redundancy code (CRC) validation, duplicate removal, possible reordering if the block ack mechanism is used, decryption, defragmentation, integrity checking, and replay detection. After replay detection (or defragmentation if security is not used), possible A-MSDU deaggregation, and possible MSDU rate limiting, one or more MSDUs are, delivered to the MAC\_SAP or to the DS. When transparent FST is used, MSDUs originating from different PHY-SAPs go through an additional transparent FST entity that contains a multiplexing process before forwarding the MSDU to the MSDU rate limiting process. The IEEE 802.1X Controlled~~/Uncontrolled~~ Port~~s~~ discards any received MSDU if the Controlled Port is not enabled. The Uncontrolled Port admits the frame for use if it is ~~and if the MSDU does not represent~~ an IEEE Std 802.1X frame and optionally for other protocols that use the Uncontrolled Port. Frame order enforcement provided by the enhanced data cryptographic encapsulation mechanisms occurs after decryption, but prior to MSDU defragmentation; therefore, defragmentation fails if MPDUs arrive out of order.

## MAC data service specification

# Layer management

## Overview of management model

## Generic management primitives

## MLME SAP interface

### 6.3.3 Scan

#### 6.3.3.2.2 Semantics of the service primitive

***Change text as follows:***

MLME-SCAN.request(

BSSType,

BSSID,

SSID,

ScanType,

ProbeDelay,

ChannelList,

MinChannelTime,

MaxChannelTime,

RequestInformation,

SSID List,

ChannelUsage,

AccessNetworkType,

HESSID,

MeshID,

DiscoveryMode,

GeneralLinkType,

VendorSpecifInfo

)

***Change the MLME-SCAN.request parameter table by adding the following as the next to last entry:***

|  |  |  |  |
| --- | --- | --- | --- |
| GeneralLinkType | Integer | 0-2 | If 0, only a non-GLK BSS is desired. If 1, only a GLK BSS is desired. If 2, the GLK nature of the BSS is ignored. |

Note:

* No change is needed in the BSSDescription for MLME-SCAN.confirm because it already includes BSSMembershipSelectorSet that indicates a GLK BSS as described in 8.4.2.3.
* No change is needed in the parameters to MLME-JOIN.request because it already includes the Capability Information field, which includes a GLK bit as described in 8.4.1.4.
* No change is needed in the parameters to MLME-ASSOCIATE.request because it already includes the Capability Information field, which includes a GLK bit as described in 8.4.1.4.
* No change is needed in the parameters to MLME-ASSOCIATE.confirm because it already includes the Capability Information field, which includes a GLK bit as described in 8.4.1.4, and ResultCode includes the possible value REFUSED\_CAPABILITIES\_MISMATCH.
* No change is needed in the parameters to MLME-ASSOCIATE.indication because it already includes the Capability Information field, which includes a GLK bit as described in 8.4.1.4.
* No change is needed in the parameters to MLME-ASSOCIATE.response because it already includes the Capability Information field, which includes a GLK bit as described in 8.4.1.4, and ResultCode includes the possible value REFUSED\_CAPABILITIES\_MISMATCH.
* No change is needed in the parameters to MLME-REASSOCIATE.request because it already includes the Capability Information field, which includes a GLK bit as described in 8.4.1.4.
* No change is needed in the parameters to MLME-REASSOCIATE.confirm because it already includes the Capability Information field, which includes a GLK bit as described in 8.4.1.4, and ResultCode includes the possible value REFUSED\_CAPABILITIES\_MISMATCH.
* No change is needed in the parameters to MLME-REASSOCIATE.indication because it already includes the Capability Information field, which includes a GLK bit as described in 8.4.1.4.
* No change is needed in the parameters to MLME-REASSOCIATE.response because it already includes the Capability Information field, which includes a GLK bit as described in 8.4.1.4, and ResultCode includes the possible value REFUSED\_CAPABILITIES\_MISMATCH.
* No change is needed in the parameters to MLME-START.request because it already includes the Capability Information field, which includes a GLK bit as described in 8.4.1.4.
* No change is needed in the parameters to MLME-MESHPEERINGMANAGEMENT.request or MLME-MESHPEERINGMANAGEMENT.indication because the relevant MeshPeeringMgmtFrameContent values (Mesh Peering Open (8.6.16.2) and Mesh Peering Confirm (8.6.16.3)) already includes the Capability Information field, which includes a GLK bit as described in 8.4.1.4.
* No change is needed to the set of MLME-RELAYSearch.\* or set of MLME-RLS.\* because the Relay Capabilities Information field includes a GLK bit as described in 8.4.2.147.

## MAC state generic convergence function (MSGCF)

## PLME SAP interface

# PHY service specification

# Frame formats

## General requirements

## MAC frame formats

## Format of individual frame types

### Control frames

### Data frames

### Management frames

### Extension frames

## Management and Extension frame body components

### Fields that are not elements

#### 8.4.1.4 Capability Information field

Note: Add B13 as General link bit. This is pending ANA assignment of that bit to GLK.

***Change Figure 8-65—Capability Information field (non-DMG STA) and Figure 8-66—Capability Information field (DMG STA) as follows:***

ESS

B0 B1 B2 B3 B4 B5 B6 B7

**Figure 8-65—Capability Information field (non-DMG STA)**

CF Pollable

CF-Poll Request

Short Preamble

Reserved

IBSS

Privacy

Reserved

Spectrum Management

B8 B9 B10 B11 B12 B13 B14 B15

QoS

Radio Measurement

GLK

APSD

Delayed Block Ack

Short Slot Time

Immediate Block Ack

DMG Parameters

B0 B7 B8 B9 B11 B12 B13 B14 B15

Reserved

GLK

Reserved

Spectrum Management

Radio Measurement

**Figure 8-66—Capability Information field (DMG STA)**

***Add the following as the 2nd to last paragraph of Clause 8.4.1.4:***

A STA sets the GLK sub-field in the Capabilities Information field to 1 when do11GeneralLink is true and sets it to 0 otherwise.

### Elements

#### 8.4.2.3 Supported Rates element

***Add a row at the end of Table 8-75—BSS membership selector value encoding:***

|  |  |  |
| --- | --- | --- |
| 125 | GLK | Support for the features of Clause 9.42 (GLK operation) is required in order to join the BSS that was the source of the Supported Rates element or Extended Supported Rates element containing this value. |

#### 8.4.2.30 TCLAS Element

Note: PCP used below and in 802.1 means Priority Code Point but in 802.11 it means PBSS Control Point. I have expanded or dropped PCP to avoid this conflict.

***Change text in Clause 8.4.2.30 as follows:***

For Classifier Type 5, the classifier parameters are the following parameters in an IEEE Std 802.1D/Q~~-2003~~ [B22] tag header: Priority Code Point (~~PCP;~~ equivalent to IEEE Std 802.1D/Q~~-2004~~ [B20] User Priority), ~~Canonical Format Indicator (CFI)~~ Drop Eligibility Indicator (DEI), and VLAN ID (VID).

***Change Figure 8-238 as follows:***

Classifier Type (5)

Octets: 1 1 1 1 1

**Figure 8-238—Frame Classifier field of Classifier Type 5**

Classifier Mask

802.1Q ~~PCP~~ Priority   
Code Point

802.1Q

~~CFI~~ DEI

802.1Q VID

***Change text in Clause 8.4.2.30 as follows:***

The ~~PCP~~ Priority Code Point subfield contains the value in the 4 LSBs; the 4 MSBs are reserved.

The ~~CFI~~ DEI subfield contains the value in the LSB; the 7 MSBs are reserved.

#### 8.4.2.127.2 DMG STA Capability Information field

***Change Figures 8-481 as follows:***

Reverse Direction

B0 B1 B2 B3 B4 B5 B6 B7 B13

**Figure 8-481—DMG STA Capability Information field format**

TPC

SPSH and Interference Mitigation

Fast Link Adaptation

Total Number of Sectors

Higher Layer Timer Synchronization

Number of RX DMG Antennas

RXSS Length

B14 B19 B20 B21 B26 B27 B28 B51 B52 B53

DMG Antenna Reciprocity

Supported MCS Set

BA with Flow Control

DTP Supported

A-MPDU Parameters

A-PPDU Supported

B54 B55 B56 B57 B59 B60 B61 B62 B63

Heartbeat

Antenna Pattern Reciprocity

GLK

Supports Other\_AID

Heartbeat Elapsed Indication

RXSSTx- Rate Supported

Bit: 1 1 1 1 2 1 7

Bit: 6 1 6 1 24 1 1

Grant Ack Supported

Reserved

Bit: 1 1 1 3 1 1 1 1

***Add to the end of Clause 8.4.2.127.2:***

A DMG STA sets the GLK sub-field in the DMG Capabilities Information field to 1 when do11GeneralLink is true and sets it to 0 otherwise.

#### 8.4.2.147 Relay Capabilities element

***Change Figure 8-519 as follows:***

Relay Supportability

Bits: 1 1 1 1 1 1 1 1 1

**Figure 8-519—Relay Capability Information field format**

Relay Usability

A/C Power

Cooperation

Reserved

B0 B1 B2 B3 B4 B5 B6 B7 B8 B9 B15

Relay Permission

Relay Preference

Duplex

GLK

***Add the following text at the end of Clause 8.4.2.147:***

A DMG STA sets the GLK sub-field in the Relay Capabilities Information field to 1 when do11GeneralLink is true and sets it to 0 otherwise.

### Information Subelements

### Access network query protocol (ANQP) elements

## Fields used in Management and Extension frame bodies and Control frames

## Action frame format details

## Aggregate MPDU (A-MPDU)

# MAC sublayer functional description

## Introduction

## MAC architecture

### General

### DCF

### PCF

### Hybrid coordination function (HCF)

#### 9.2.4.2 HCF contention based channel access (EDCA)

***Change the first paragraph in 9.2.4.2 as follows:***

The EDCA mechanism provides differentiated, distributed access to the WM for STAs using eight different UPs. The EDCA mechanism defines four access categories (ACs) that provide support for the delivery of traffic with UPs at the STAs. Six transmit queues are defined when dot11AlternateEDCAActivated is true, and four transmit queues otherwise. The transmit queue and AC are derived from the UPs as shown in Table 9-1 (UP-to-AC mappings) for non-GLK STAs. For GLK STAs, Table 9-1 gives the default mapping of Ups to AC but other mappings are configurable.

Table 9-1 is changed as shown below by adding a column on the left and adding a second section to the table for the GLK case.

***Replace Table 9-1 with the following:***

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Type | Priority | UP | 802.1 | AC | Transmit queue | Transmit queue | Designation (informative) |
| Non-GLK (802.1D UP) | Lowest     Highest | 1 | BK | AC\_BK | BK | BK | Background |
| 2 | — | AC\_BK | BK | BK | Background |
| 0 | BE | AC\_BE | BE | BE | Best Effort |
| 3 | EE | AC\_BE | BE | BE | Best Effort |
| 4 | CL | AC\_VI | VI | A\_VI | Video (alternate) |
| 5 | VI | AC\_VI | VI | VI | Video |
| 6 | VO | AC\_VO | VO | VO | Voice |
| 7 | NC | AC\_VO | VO | A\_VO | Voice (alternate) |
| GLK (802.1Q UP) | Lowest     Highest | 1 | BK | AC\_BK | BK | BK | Background |
| 0 | BE | AC\_BE | BE | BE | Best Effort |
| 2 | EE | AC\_BE | BE | BE | Best Effort |
| 3 | CA | AC\_VI | VI | A\_VI | Video (alternate) |
| 4 | VI | AC\_VI | VI | VI | Video |
| 5 | VO | AC\_VO | VO | VO | Voice |
| 6 | IC | AC\_VO | VO | VO | Voice |
| 7 | NC | AC\_VO | VO | A\_VO | Voice (alternate) |

### Mesh coordination function (MCF)

### Combined use of DCF, PCF, and HCF

### Fragmentation/defragmentation overview

### MAC data service

## DCF

## PCF

## Fragmentation

## Defragmentation

## Multirate support

## MSDU transmission restrictions

## HT Control field operation

## Control Wrapper operation

## A-MSDU operation

## A-MPDU operation

## PPDU duration constraint

## DMG A-PPDU operation

## LDPC operation

## STBC operation

## Short GI operation

## Greenfield operation

## Group ID and partial AID in VHT PPDUs

## Operation across regulatory domains

## HCF

## Mesh coordination function (MCF)

## Block acknowledgement (block ack)

## No Acknowledgement (No Ack)

## Protection mechanisms

## MAC frame processing

## Reverse direction protocol

## PSMP Operation

## Sounding PPDUs

## Link adaptation

## Transmit beamforming

## Antenna selection (ASEL)

## Null data packet (NDP) sounding

## Mesh forwarding framework

## DMG channel access

## DMG AP or PCP clustering

## DMG beamforming

## DMG block ack with flow control

## DMG link adaptation

## DMG dynamic tone pairing (DTP)

## DMG relay operation

***Add new Clause 9.42:***

## GLK operation

All MSDUs transmitted by a GLK STA shall use EPD.

A GLK STA shall set dot11GeneralLink to true.

# MLME

# Security

# Fast BSS transition

# MLME Mesh procedures

## Mesh STA dependencies

## Mesh discovery

## Mesh peering management (MPM)

## Mesh peering management finite state machine (MPM FSM)

## Authenticated mesh peering exchange (AMPE)

## Mesh group key handshake

## Mesh security

## Mesh path selection and metric framework

## Airtime link metric

## Hybrid wireless mesh protocol (HWMP)

## Interworking with the DS

### Overview of interworking between a mesh BSS and a DS

***Change first paragraph as follows:***

A mesh STA that has access to a DS is called a mesh gate. Mesh STAs in an MBSS access the DS via the mesh gate. An MBSS functions like an IEEE 802 LAN segment that is compatible with IEEE Std 802.1D if the MBSS is composed of non-GLK mesh STAs and compatible with IEEE Std 802.1Q if the MBSS is composed of GLK mesh STAs. The MBSS appears as a single access domain.

### Gate announcement (GANN)

### Data forwarding at proxy mesh gates

### Proxy information and proxy update

### Mesh STA collocation

## Intra-mesh congestion control

## Synchronization and beaconing in MBSSs

## Power save in mesh BSS

# Frequency-Hopping spread spectrum (FHSS) PHY specification for the 2.4 GHz industrial, scientific, and medical (ISM) band

# Infrared (IR) PHY specification

# DSSS PHY specification for the 2.4 GHz band designated for ISM applications

# High rate direct sequence spread spectrum (HR/DSSS) PHY specification

# Orthogonal frequency division multiplexing (OFDM) PHY specification

# Extended Rat PHY (ERP) specification

# High Throughput (HT) PHY specification

# Directional multi-gigabit (DMG) PHY specification

# Very High Throughput IVHT) PHY

# Annex A, Bibliography

# Annex B, Protocol Implementation Conformance Statement (PICS)

Need to do something about the PICS.

# Annex C, ASN.1 encoding of the MAC and PHY MIB

Need to add more for configuration of UP to AC mapping for GLK STAs.

***Add the following entry at the end of the* dot11StationConfigEntry SEQUENCE*:***

dot11GeneralLink TruthValue

# …

# Annex P, Integration Function

Note: More extensive changes in Annex P may be required.

## P.1 Introduction

***Replace the contents of P.1 with the following:***

The purpose of this annex is to guide the implementer of a non-GLK WLAN system that includes a portal that integrates the WLAN systems with a wired LAN. This annex does not apply to GLK WLAN systems.

## P.2 Ethernet V2.0/IEEE Std 802.3 LAN integration function

## P.3 Example

***Change the second paragraph as follows:***

In the tables below the rows that have a 81-00 Type/Length field value represent bridging between an Ethernet/IEEE Std 802.3 LAN and an IEEE Std 802.11 LAN. Both LANs are carrying VLAN-tagged MSDUs (User Priority=4, ~~CFI-~~DEI=0, VLAN ID=1893).

## P.4 Integration service versus bridging

# …

# Annex V, Interworking with external networks

## V.1 General

## V.2 Network discovery and selection

## V.3 QoS mapping guidelines for interworking with external networks

### V.3.3 Example of QoS mapping from different networks

***Change the first sentence of Clause V.3.3 as follows:***

IEEE Std 802.1D/Q UPs map to EDCA ACs, as described in Table 9-1 (UP-to-AC mappings).

Table V-1 is changed below by adding a new column on the right and changing the headings of the two rightmost columns.

***Change Table V-1 to the following:***

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 3GPP QoS Information | | DiffServ PHB | DSCP | QoS Requirement on GPRS Roaming Exchange | | | | EDCA Access Category | UP (non-GLK 802.1D) | UP (GLK 802.1Q) |
| Traffic Class | THP |  |  | Max Delay | Max Jitter | MSDU Loss | MSDU Error Rate |  |  |  |
| Conversational | N/A | EF | 101110 | 20 ms | 5 ms | 0.5% | 1.0E-05 | AC\_VO | 7, 6 | 7, 6, 5 |
| Streaming | N/A | AF41 | 100010 | 40 ms | 5 ms | 0.5% | 1.0E-05 | AC\_VI | 5, 4 | 4, 3 |
| Interactive | 1 | AF31 | 011010 | 250 ms | N/A | 0.1% | 1.0E-07 | AC\_BE | 3 | 2 |
|  | 2 | AF21 | 010010 | 300 ms | N/A | 0.1% | 1.0E-07 | AC\_BE | 3 | 2 |
|  | 3 | AF11 | 001010 | 350 ms | N/A | 0.1% | 1.0E-07 | AC\_BE | 0 | 0 |
| Background | N/A | BE | 000000 | 400 ms | N/A | 0.1% | 1.0E-07 | AC\_BK | 2, 1 | 1 |

## V.4 Interworking and SSPN interface support

## V.5 Interworking with external networks and emergency call support

## V.6 Peer information

# …