IEEE P802.11
Wireless LANs

|  |
| --- |
| LB 202 Comment Resolution for CID 3043 and 3045 |
| Date: 2014-07-13 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Bo Sun | ZTE Corp. | #9 Wuxing Seg. Chang’an District, Xi’an, China | +86 29 68700941 | Sun.bo1@zte.com.cn |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

Abstract

This submission proposes resolutions for comments CID 3043 and 3045 in LB 202 for TGRevmc Draft 3.0.

Interpretation of a Motion to Adopt

A motion to approve this submission means that the editing instructions and any changed or added material are actioned in the TGah Draft. This introduction is not part of the adopted material.

***Editing instructions formatted like this are intended to be copied into the TGRevmc Draft (i.e. they are instructions to the 802.11 editor on how to merge the text with the baseline documents).***

***TGRevmc Editor: Editing instructions preceded by “TGRevmc Editor” are instructions to the TGRevmc editor to modify existing material in the TGRevmc draft. As a result of adopting the changes, the TGRevmc editor will execute the instructions rather than copy them to the TGRevmc Draft.***

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **P.L** | **Clause** | **Comment** | **Proposed Change** | **Resolution** |
| 3043 | 2442.32 | 22.2.2 | "Indicates whether a VHT AP allows non-AP VHT STAs in TXOP power save mode to enter Doze state during the TXOP.0 indicates that the VHT AP allows non-AP VHT STAs to enter doze mode during a TXOP." -- What is the difference between "Doze state" and "doze mode"? | Use only one term | Revised.TGRevmc Editor: replace “doze mode” with “Doze state” in pg2442/ln36 in Revmc D3.0 draft. |
| 3045 | 2519.60 | 22.3.15 | "The transmitter RF delay is defined in 18.3.8.6" -- no it's not. That subclause has been deleted.Ditto at 2639.57. | Delete 22.3.15 and any references to it.Likewise 23.3.15. | Revised.TGRevmc Editor: remove clause 22.3.15 at pg2519/ln58 and remove clause 23.3.15 at pg2600/ln52 in Revmc D3.0 draft. |
|  |  |  |  |  |  |
|  |  |  |  |  |  |

**Discussion:**

CID 3043: agreed with the commentor. As defined in Clause 10.2.2.2, a STA may in one of two different power states: Awake and Doze. Therefore the description should be unified to “Doze state”.

CID 3045: agreed with the commentor. Clause 18.3.8.6 has been removed from Revmc draft D1.0.