IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| LB202 Assigned comments | | | | |
| Date: 2014-07-15 | | | | |
| Author(s): | | | | |
| Name | Company | Address | Phone | email |
| Dorothy Stanley | Aruba Networks | 1322 Crossman Ave Sunnyvale, CA 94089 | +1 630-363-1389 | [dstanley@arubanetworks.com](mailto:dstanley@arubanetworks.com) |
|  |  |  |  |  |

Abstract

This submission contains proposed comment resolutions for CIDs

3072, 3093, 3096, 3085, 3059,

3312, 3609, 3615

# CID 3072

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| 3072 | 721.09 | 8.4.2.14 |  |  | Should the reference to 10.8.3 be 10.8.4?    Ditto at line 15. | Determine whether to change reference to 10.8.4. |

**Discussion:**

The cited text is below:



The proposed reference change is to 10.8.4 “**10.8.4 Interpretation of transmit power capability”.**

Yes, 10.8.4 is a better reference.

**Proposed resolution: Revised**

At 721.09 and 721.15, change from “10.8.3” to “10.8.4”.

**CID 3093**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| 3093 | 1012.19 | 8.4.2.66.2 |  |  | What is the meaning of the "Order" column in table 8-177? No semantics are defined for it. | Remove the "Order" column in Table 8-177. |

**Discussion:**

The cited text is below:



The subelements are used independently, for example

****

**Proposed resolution: Accepted**

**CID 3096**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| 3096 | 643.12 | 8.4.1.6 |  |  | "An AP may use the Listen Interval information in determining the lifetime of frames that it buffers for a STA." - normative verb in clause 8 | "may" -> "might" at cited location |

**Discussion:**

**The cited text is below:**

****

**Proposed resolution: Revised**

**Change from “may use” to “uses”**

**CID 3085**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| 3085 | 1012.12 | 8.4.2.138 |  |  | "The ADDBA Request frame, ADDBA Response frame, or both can contain the element." -- This says nothing over and above the previous sentence. | Delete cited sentence. |

**Discussion:**

**The cited text is below:**

****

**Proposed resolution: Accepted**

**CID 3059**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| 3059 | 53.50 | 3.4 |  |  | Similar definitions for GCMP were added by .11ad and .11ac. | Delete the shorter definition at line 50. |

**Discussion:**

The cited text is below:



**Proposed resolution: Accepted**

**CID 3312**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| 3312 | 18.46 | 3.1 |  |  | STBC/SM is defined but not described anywhere | Delete the definition |

**Discussion:**

The cited text is below:



This is the only reference, so agree to delete.

**Proposed resolution: Accepted**

**CID 3609**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| 3609 | 75.35 | 4.3.10.4 |  |  | "if a secondary licensee causes inference to a primary licensee, the licensee is obliged to resolve complaints that result from interference caused by any STA under its control": just which licensee is so obliged? Presumably it's the secondary licensee, but this description does not say that. | Replace "the licensee is obliged" with "the secondary licensee is obliged". |

Discussion:

The cited text is below:



**Proposed resolution: Accepted**

**CID 3615**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| 3615 | 79.04 | 4.3. |  |  | "this standard also allows a STA that is not a member of a BSS to transmit Data frames.": another example of a normative statement in an informative clause. | Replace "allows" with "defines a mechanism by which" and replace "to transmit" with "can transmit". |

**Discussion:**

**The cited text is below:**

****

**The commenter proposed to change as follows:**

In addition to defining procedures for STA communication within a BSS, this standard also defines a mechanism by which a STA that is not a member of a BSS can transmit Data frames. Such Data frames are defined as being transmitted outside the context of a BSS. A STA transmits a Data frame outside the context of a BSS only if dot11OCBActivated is true.

**Proposed resolution: Accepted**