IEEE P802.11
Wireless LANs

|  |
| --- |
| Reference change from 3GPP TS 24.234 to TS 24.302 |
| Date: 2014-11-03 |
| Author(s): |
| Name | Company | Address | Phone | email |
| Stephen McCann | BlackBerry Ltd | 200 Bath Road, Slough, Berkshire, SL1 3XE, UK | +44 1753 667099 | smccann@blackberry.com |

Abstract

This document proposes to update the document reference from 3GPP TS 24.234 to TS 24.302 as described in the liaison received from 3GPP, document 11-14-1411-00-0000-liaison-3gpp-document-reference.docx

This uses Draft P802.11REVmc\_D3.2.pdf as a baseline.

***Modify the text in the following clauses:***

***2.* Normative References**

 (11u)

3GPP TS 24.302, Access to the 3GPP Evolved Packet Core (EPC) via non-3GPP access networks; Stage 3.1

**8.4.4.11 3GPP Cellular Network ANQP-element**

…

The Payload field is a variable-length field and is a generic container. An example of the format and content is defined in Annex H of 3GPP TS 24.302.