### IEEE P802.11 Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| LB 205 Comment Resolution for Synchronization (Sync) Frame Operation | | | | |
| Date: 2014-12-01 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Po-Kai Huang | Intel Corporation | 2200 Mission College Blvd, Santa Clara, CA 950542200 | 408 765 7766 | po-kai.huang@intel.com |
| Chittabrata Ghosh | Intel Corporation | 2200 Mission College Blvd, Santa Clara, CA 95054 |  | chittabrata.ghosh@intel.com |

Abstract

This submission proposes resolutions for comments in clause 9.46.1 of TGah Draft 3.1 with the following CID:

* 5368

Revisions:

* Rev 0: Initial version of the document.

Interpretation of a Motion to Adopt

A motion to approve this submission means that the editing instructions and any changed or added material are actioned in the TGah Draft. This introduction is not part of the adopted material.

***Editing instructions formatted like this are intended to be copied into the TGah Draft (i.e. they are instructions to the 802.11 editor on how to merge the text with the baseline documents).***

***TGah Editor: Editing instructions preceded by “TGah Editor” are instructions to the TGah editor to modify existing material in the TGah draft. As a result of adopting the changes, the TGah editor will execute the instructions rather than copy them to the TGah Draft.***

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **P.L** | **Clause** | **Comment** | **Proposed Change** | **Resolution** |
| 5368 | 300.25 | 9.46.1 | To make it easier to read, add "," and change "TWT time" to "a time of TWT". | Add "," after "RAW" and change to "a time of TWT" as "When an AP ... to 1, the AP shall protect a time slot that is assigned for the STA in a RAW, or a time of TWT, or a TXOP duration after the expiration of a wakeup timer of the STA with NAV-setting frame exchanges." | Revised –  Agree in principle with the commenter.  Add “,” will indeed improve the readability.  As for the revision of “a TWT time,” the following description “a time duration at a TWT” is used in 300.16. Hence, for clarity, propose to use the same description in 300.16.  TGah editor to make the changes shown in 14/1573r0 under all headings that contain CID 5368. |

**Discussion:** *None.*

**Propose:**

* Revised for CID 5368, per discussion and editing instructions in 11-14/1573r0.

***TGah editor: Change this subclause (9.46.1) as follows:*** *(CID 5368)*

When an AP receives a Sync Control frame froma STA with the Time Slot Protection Request

field equal to 1, the AP shall protect a time slot that is assigned for the STA in a RAW, or a time duration that is assigned for the STA at a TWT, or a TXOP duration after the expiration of a wakeup timer of the STA with NAV-setting frame exchanges.