IEEE P802.11
Wireless LANs

|  |
| --- |
| Resolutions for CID 6057 |
| Date: 2014-11-06 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Santosh Abraham Jouni MalinenGeorge CherianAbhishek Patil | Qualcomm | 5775 Morehouse Dr., San Diego, CA 92121 | +1 858 651 6645 | sabraham@qti.qualcomm.com |
|  |  |  |  |  |

Abstract

This document provides proposed resolution for CIDs 6057

Note: All page and line numbers indicated here are with respect to Draft 3.0



***Resolution to CID 6057***

**8. Frame formats**

**8.6 Action frame format details**

**8.6.8 Public Action details**

**8.6.8.38 FILS Discovery frame format**

***Modify Figure 8-662a as follows***

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |
|  | FILS Discovery frameControl | Timestamp | BeaconInterval |  SSID/Compressed SSID | FD Capability(conditional) |
| Octets: | 2 | 8 | 2 | 1-32 | 0 or 2 |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |  |
|  | AP’s NextTBTT Offset(ANTO)(conditional) | AP ConfigurationSequenceNumber(APCSN)(conditional) | Access NetworkOptions(ANO)(conditional) |  PrimaryChannel(conditional) | Channel CenterFrequencySegment 1(conditional) | RSN Information(conditional) |
| Octets: | 0 or 1 | 0 or 1 | 0 or 1 | 0 or 1  | 0 or 1 | 0 or 4 |

***Modify Figure 8-662b as follows***

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | B0 B4 | B5 | B6 | B7 |
|  | SSID Info rmation | Capability Presence Indicator | ANTO Presence Indicator |  AP-CSN Presence Indicator |
| Bits: |  5 | 1 | 1 | 1 |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  | B8 | B9 | B10 | B11 | B12 | B13 B15 |
|  | ANO Presence Indicator | CCFS-1 Presence Indicator | Primary Channel Presence Indicator | RSN InfoPresenceIndicator | SSID Type Indicator | Reserved 3 bits |
| Bits | 1 | 1 | 1 |  | 1 | 4 |

**Figure 8-662b—FILS Discovery frame Control field format**

***Insert the following Table next to Figure 8-662b***

|  |  |  |
| --- | --- | --- |
| SSID Type Indicator | Description | SSID Information field |
| 0 | Full SSID Present | B0 – B4: Set to length in octets of the SSID field in the FILS Discovery frame |
| 1 | Other SSID Type | B0 = 0: Short SSIDB0 = 1: ReservedB1-B4: Reserved |

**Table 8-11ai-1: SSID Type Indicator and SSID Information field**

***Replace the paragraph on lines 27-29 of Page 69 with the following***

The SSID Information field is set as shown in Table 8-11ai-1. The Short SSID field is 4 octets long and is present if the SSID Type Indicator field is set to 1. The Short SSID field indicates a 32-bit CRC calculated as defined in 8.2.4.8 FCS field, wherein the calculation field is the SSID field in the SSID element of the Beacon frame.