IEEE P802.11
Wireless LANs

|  |
| --- |
| LB 205 Comment Resolution for 9.42i |
| Date: 2015-1-6 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Betty Zhao | Huawei Technologies | Beijing, China |  | betty.zhao@huawei.com |

Abstract

This submission proposes resolutions for comments in clause 9.42i of TGah Draft 3.0 with the following CIDs:

* 5141, 5324, 5325, 5326, 5327, 5328

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **P.L** | **Clause** | **Comment** | **Proposed Change** | **Resolution** |
| 5141 | 325.30 | 9.42i | Change title of 9.42i to spell out the acronym and improve readability. I know its in the 3.2 definitions section, but its too easy to lose context when reading this spec | Chagge "Multicast AID" to "Multicast Paged Association Identifiers (Multicast AID)" | Rejected -The abbreviation of “AID” is in the subclause 3.3 of IEEE Std 802.11-2012. And with that, “Multicast AID” as a title is self-explanatory. |
| 5324 | 325.34 | 9.42i | This sentence is a little bit repetitive. | Remove ", which follows the rules of the implementation of traffic using AID" | Accepted –As proposed change |
| 5325 | 325.37 | 9.42i | Some suggestions in the proposed change to make this paragraph clearer and fix some grammatical errors. | Replace "that represents" with "that is assigned by an S1G AP to identify" in P325L37.Replace "is the same signalling" with "using the same signalling". | Accepted –As proposed change |
| 5326 | 325.55 | 9.42i | Need to clarify that the multicast listen interval starts from the moment that the AID Switch Count in the AID Switch Response has expired. | Clarify that the multicast listen interval starts at the T(S)BTT where the AID Switch Count value in the AID Switch Response for this particular multicast AID has expired (making sure the description is inline with 10.44a). Clarify the behavior for both AP and non-AP STA. | Revised –Brief explanation of the proposed resolution.TGah editor to make the changes shown in 11-15/0127r0 under all headings that include CID 5326. |
| 5327 | 325.63 | 9.42i | page slice is the name of the element so it should take capital letters. Replace "page slice" with "Page Slice". | As in comment. | Accepted –As proposed change |
| 5328 | 326.12 | 9.42i | The STA shall discard only those frame that contain the group MAC address that corresponds to that multicast AID. | Replace "the group" with "that group". | Accepted –As proposed change |

***TGah Editor: Change the clause 9.42i as follows (11-15-0127-00-00ah-LB205-MAC-Resolution-9.42i):***

**9.42i Multicast AID**

The S1G AP shall indicate the presence of group addressed BUs corresponding to a multicast AID in the TIM included in the S1G Beacon frame that is sent every multicast listen interval, following the expiration of a counter that corresponds to the AID Switch Count included in the AID Response element containing the multicast AID and which started upon transmission of that element. The S1G STA that has negotiated multicast AID operation shall wake up every multicast listen interval to receive the S1G Beacon frame, starting from the T(S)BTT that follows the expiration of a counter that corresponds to the AID Switch Count included in the AID Response element containing the multicast AID and which started upon receipt of that element.