IEEE P802.11
Wireless LANs

|  |
| --- |
| LB 205 MAC Comment Resolution for Clause 8.6.23a.2 and 8.6.23a.3 |
| Date: 2015-01-12 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Jae Seung Lee | ETRI | 161 Gajeong-dong,Yuseong-gu, Daejeon, Korea | +82 42 860 1326 | jasonlee@etri.re.kr  |
| Jaewoo Park | ETRI | 161 Gajeong-dong, Yuseong-gu, Daejeon, Korea | +82 42 860 5635 | parkjw@etri.re.kr |
| Yu Ro Lee | ETRI | 161 Gajeong-dong, Yuseong-gu, Daejeon, Korea | +82 42 860 5693 | yurolee@etri.re.kr |
| Jeeyon Choi | ETRI | 161 Gajeong-dong, Yuseong-gu, Daejeon, Korea | +82 42 860 5247 | jychoi@etri.re.kr |
| Il Gyu Kim | ETRI | 161 Gajeong-dong, Yuseong-gu, Daejeon, Korea | +82 42 860 5490 |  igkim@etri.re.kr |

Abstract

This submission proposes comment resolutions for Clause 8.6.23a.2 and 8.6.23a.3

* CIDs: 5275 and 5276 (2 CIDs)

Changes in the text refer to: Draft P802.11ah/D3.1

Interpretation of a Motion to Adopt

A motion to approve this submission means that the editing instructions and any changed or added material are actioned in the TGah Draft. This introduction is not part of the adopted material.

***Editing instructions formatted like this are intended to be copied into the TGah Draft (i.e. they are instructions to the 802.11 editor on how to merge the text with the baseline documents).***

***TGah Editor: Editing instructions preceded by “TGah Editor” are instructions to the TGah editor to modify existing material in the TGah draft. As a result of adopting the changes, the TGah editor will execute the instructions rather than copy them to the TGah Draft.***

**CID 5275 and 5276**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Clause** | **Page** | **Line** | **Comment** | **Proposed Change** | **Proposed****Resolution** |
| 5275 | 8.6.23a.2 | 187 | 46 | There is no "Multicast ID". Replace it with "multicast AID" (check that the terminology is the same throughout the draft). | As in comment. | Accepted –Only one occurrence of “Multicast ID” is found throughout the draft. (only in the indicated subcluase pointed by the commenter)Editor to change “Multicast ID” to “multicast AID” in 8.6.25.2 AID Switch Request frame format of D3.0 |
| 5276 | 8.6.23a.3 | 188 | 51 | The name of the field does not need the "element" identifier as noted by the Editor's note. Remove the first occurrence of "element" in this sentence. Idem from the 4th row of Table 8-406a3 in P188L32. Perform similar changes throughout all subclauses of 8.6.23a (S1G Action frame details). In addition, ensure that the names of fields/subfields throughout these subclauses start with a capital letter. For example "Category" "S1G Action" etc. | As in comment. | Revised – Agree with the commenter.TGah Editor to make changes shown in 15/0139 |

**Proposed Remedy on CID 5276:**

***Instructions to TGah Editor: Modify the followings in Subclauses under 8.6.25 S1G Action frame details of D3.1 as follows:***

8.6.25.3 AID Switch Response frame format

….

|  |  |  |  |
| --- | --- | --- | --- |
|

|  |
| --- |
| **Order** |

 |

|  |
| --- |
| **Information** |

 |
|  |  |
|  |  |
|  |  |
|

|  |
| --- |
| 4 |

 |

|  |
| --- |
| AID Response ~~element~~ (see 8.4.2.191 (AID Response element)) |

 |

…

The AID Response ~~element~~ field contains an AID Response element as specified in 8.4.2.191 (AID Response element).

8.6.25.5 STA Information Announcement frame format

….

|  |  |  |  |
| --- | --- | --- | --- |
|

|  |
| --- |
| **Order** |

 |

|  |
| --- |
| **Information** |

 |
|  |  |
|  |  |
|

|  |
| --- |
| 3 |

 |

|  |  |
| --- | --- |
|

|  |
| --- |
| AID Announcement ~~element~~ (8.4.2.205 (AID Announcement element)) |

 |

 |

…

The AID Announcement ~~element~~ field contains an AID Announcement element as specified in 8.4.2.205 (AID Announcement element).

8.6.25.6 EDCA Parameter Set frame format

…..

The EDCA Parameter Set ~~element~~ field contains an EDCA Parameter Set element as specified in 8.4.2.28 (EDCA Parameter Set element).

8.6.25.7 Activity Specification frame format

…

|  |  |  |  |
| --- | --- | --- | --- |
|

|  |
| --- |
| **Order** |

 |

|  |
| --- |
| **Information** |

 |
|  |  |
|  |  |
|

|  |
| --- |
| 3 |

 |

|  |  |  |
| --- | --- | --- |
|

|  |  |
| --- | --- |
|

|  |
| --- |
| Activity Specification ~~element~~ (8.4.2.207 (Activity Specifica­tion element)) |

 |

 |

 |

…

The Activity Specification ~~element~~ field contains an Activity Specification element as specified in 8.4.2.207 (Activity Specification element).

8.6.25.8 TWT Setup frame format

The ~~c~~Category field is set to the value for S1G specified in Table 8-54 (Category values).

|  |  |  |  |
| --- | --- | --- | --- |
|

|  |
| --- |
| **Order** |

 |

|  |
| --- |
| **Information** |

 |
|  |  |
|  |  |
|  |  |
|

|  |
| --- |
| 4 |

 |

|  |  |
| --- | --- |
|

|  |
| --- |
| TWT ~~element~~ (8.4.2.196 (TWT element)) |

 |

 |

…

8.6.25.9 TWT Teardown frame format

…..

The ~~c~~Category field is set to the value for S1G specified in Table 8-54 (Category values).

8.6.25.10 Sectorized Group ID List frame format

…

|  |  |  |  |
| --- | --- | --- | --- |
|

|  |
| --- |
| **Order** |

 |

|  |
| --- |
| **Information** |

 |
|  |  |
|  |  |
|

|  |
| --- |
| 3 |

 |

|  |  |  |  |
| --- | --- | --- | --- |
|

|  |  |  |
| --- | --- | --- |
|

|  |  |
| --- | --- |
|

|  |
| --- |
| Sectorized Group ID List ~~element~~ (8.4.2.208 (Sectorized Group ID List element)) |

 |

 |

 |

 |

…

The Sectorized Group ID List ~~element~~ field contains a Sectorized Group ID List as specified in 8.4.2.208 (Sectorized Group ID List element).

8.6.25.11 Sector ID Feedback frame format

…

The S1G ~~a~~Action field is set to the value for Sector ID Feedback, specified in Table 8-406a1 (S1G Action field values).

8.6.25.12 Header Compression frame format

…..

|  |  |  |  |
| --- | --- | --- | --- |
|

|  |
| --- |
| **Order** |

 |

|  |
| --- |
| **Information** |

 |
|  |  |
|  |  |
|  |  |
|

|  |
| --- |
| 4 |

 |

|  |  |  |
| --- | --- | --- |
|

|  |  |
| --- | --- |
|

|  |
| --- |
| Header Compression ~~element~~ (see 8.4.2.210 (Header Compres­sion element)) |

 |

 |

 |

…

The Header Compression ~~element~~ field contains a Header Compression element as specified in 8.4.2.210 (Header Compression element).

8.6.25.13 TWT Information frame format

…..

The ~~c~~Category field is set to the value for S1G specified in Table 8-54 (Category values).