IEEE P802.11
Wireless LANs

|  |
| --- |
| LB207 MAC Resolution to Comments in D4.0 Subclauses 10.3.8.1 and 8.4.2.1 |
| Date: 2015-02-23 |
| Author(s): |
| Name | Affiliation | Address | Phone | Email |
| Zander Lei | I2R | 1 Fusionopolis Way #21-01 Connexis, Singapore | +65 6408 2436 | leizd@i2r.a-star.edu.sg |
| Shoukang Zheng | +65 6408 2252 | skzheng@i2r.a-star.edu.sg |
| Yuan Zhou | +65 6408 2472 | yzhou@i2r.a-star.edu.sg |

Abstract

This submission proposes resolution to comments in D4.0 subclauses 10.3.8.1 and 8.4.2.1. There are 3 CIDs addressed: 6019, 6052, and 6192.

Revision History:

**Interpretation of a Motion to Adopt:** A motion to approve this submission means that the editing instructions and any changed or added material are actioned in the TGah Draft. This introduction is not part of the adopted material.

***Editing instructions formatted like this are intended to be copied into the TGah Draft (i.e. they are instructions to the 802.11 editor on how to merge the text with the baseline documents).***

***TGah Editor: Editing instructions preceded by “TGah Editor” are instructions to the TGah editor to modify existing material in the TGah draft. As a result of adopting the changes, the TGah editor will execute the instructions rather than copy them to the TGah Draft.***

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| 6019 | 353.50 | 10.3.8.1 | A CCA STA sets dot11S1GCentralizedAuthenticationControlActivated to true. -- The mit variable dot11S1GCentralizedAuthenticationControlActivated is (already) set to true in order to make a STA a CCA STA. Since it cannot (re)set the mib variable to ture. | Delete "sets dot11S1GCentralizedAuthenticationControlActivated to true and"Per definition, a CCA STA is well defined havig dot11S1GCentralizedAuthenticationControlActivated set to true. No need to say this again here. | Accept. Instruction to TGah editor: Please remove the phrase "sets dot11S1GCentralizedAuthenticationControlActivated to true and" at page.line=353.50 according to the proposed resolution.  |
| 6052 | 353.23 | 10.3.8.1 | The sentence starting with "An S1G STA with ..." provides redundant and unecessary information as the definition of CCA STA and CCA AP provides exactly this information | Delete sentence starting from "An SIG STA with ..." | Accept. Instruction to TGah editor: Please remove the last sentence (in lines 23-25, page 353) of the 1st paragraph of 10.3.8.1, as suggested by the commenter.  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| 6160 | 113.09 | 8.4.2.1 | This amendment is creating a huge number of new elements. Are all these elements truly used independently? That is, not just carrying independent semantics, but must appear in different contexts? If some of these are always used in the same contexts (carried in the same frames), there is no reason they can't be combined into independent fields within a large, composite element, which is what is ususally done. | Examine where these elements are used, and for those have all usage contexts in common, combine into composite elements. | Reject. Agreed to the commenter in principle that elements should be combined if not used independently. The elements have been examined and seem to the assignee that there is no element can be combined. It is notable that 11ah has introudcued quite a number of new features requiring ne w elements.  |