IEEE P802.11
Wireless LANs

|  |
| --- |
| Resolution CID 10636 10637 |
|  |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Santosh Abraham | Qualcomm | 5775 Morehouse Dr. San Diego, CA 92129 | +1-858 651 6107 | sabraham@qti.qualcomm.com |
|  |  |  |  |  |

Abstract

This submission addresses CIDs 10636, 10637

***Instruct the editor to modify section 10.1.4.3.2 as indicated:***

**10.1.4.3.2 Active scanning procedure for a non-DMG STA**

***Modify Paragraph in lines 56 – 60 of page 100 as follows:***

1. Send a probe request to the broadcast destination address. The probe request is sent with the SSID
and BSSID from the MLME-SCAN.request primitive. When the SSID List is present in the MLMESCAN.request primitive, send one or more Probe Request frames, each with an SSID indicated in
the SSID List and the BSSID from the MLME-SCAN.request primitive. The basic access procedure (9.3.4.2 (Basic access)) is performed prior to each probe request transmission.

|  |  |  |  |
| --- | --- | --- | --- |
| CID | Comment | Proposed Change | Proposed Resolution |
| 10636 | What does it mean to send "one or more Probe Request frames". How does the MAC know how to proceed? | Describe what how the MAC and SME interact to execute the primitive. | Revised: Apply changes described in 11-15-1415r0 |
| 10637 | Why is f) restricted to non-FILS STAs | This behavior should be independent whether the STA is a FILS STA or not. | **Reject: Behavior for FILS STA is described in Step g** |

***Instruct the editor to modify section 10.1.4.3.2 as indicated:***

**10.1.4.3.2 Active scanning procedure for a non-DMG STA**

***Change step d) of the procedure in Lines 56-60 of Page 100 as given below***

d) Send a probe request to the broadcast destination address. The probe request is sent with the SSID
and BSSID from the MLME-SCAN.request primitive. When the SSID List is present in the MLMESCAN.request primitive, send one or more Probe Request frames, each with an SSID indicated in
the SSID List and the BSSID from the MLME-SCAN.request primitive. Note, perform basic access procedure ( 9.3.4.2 Basic access) before the transmission of each of the probe request frames.