IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| SB0 Comment Resolutions for Misc. Clause 24 CIDs | | | | |
| Date: 2015-12-01 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Sabita Nahata | Qualcomm Inc. | 1060 Rincon Circle, San Jose, CA-95131 |  | snahata@qti.qualcomm.com |
| Naveen Kakani | Qualcomm Inc. |  |  | nkakani@qti.qualcomm.com |
| Raja Banerjea | Qualcomm Inc. |  |  | rajab@qti.qualcomm.com |
| Hong Wan | Qualcomm Inc. |  |  | hwan@qti.qualcomm.com |
| Eugene Baik | Qualcomm Inc. |  |  | eugeneb@qca.qualcomm.com |
| Alfred Asterjadhi | Qualcomm Inc. |  |  | aasterja@qti.qualcomm.com |

Abstract

This submission provides Sponsor Ballot CID resolutions contained in multiple sections of Clause 24 TGah Draft 5.0.

CIDs: 8212, 8213, 8214, 8215, 8216, 8217, 8218

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Commenter** | **P.L** | **Clause** | **Comment** | **Proposed Change** | **Resolution** |
| 8212 | Naveen Kakani | 437.16 | 24.3.8.2.1.4 | Clarify in the BW field description to what happens when duplicate modes are considered. Basically, what should be the value of BW field in case of duplicate mode. | Table 24.11, Ln 16 change “  Set to 0 for 2 MHz, 1 for 4 MHz, 2 for 8 MHz, 3 for 16 MHz”  to  “If FORMAT is S1G in TXVECTOR, set to:  0 when CH\_BANDWIDTH is CBW2  1 when CH\_BANDWIDTH is CBW4  2 when CH\_BANDWIDTH is CBW8  3 when CH\_BANDWIDTH is CBW16  If FORMAT is S1G\_DUP\_2M in TXVECTOR, set to 0.” | Accepted |


**Discussion: None.**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Commenter** | **P.L** | **Clause** | **Comment** | **Proposed Change** | **Resolution** |
| 8213 | Naveen Kakani | 413.46, | 24.3.4.3.2, | Step ‘a’ should be texted separately for non-duplicate and duplicate mode as given in the resolution table below in the relevant section | Separate the text for non-duplicate and duplcate mode. | Revised.  Instruction to Editor:In Section 24.3.4.3.2, P.L: 413.46  Remove current bullet a) and replace with a) and b) as shown below:  a) Determine FORMAT from TXVECTOR  b) Sequence generation: If FORMAT is S1G, generate the LTF1 field sequence in the frequency-domain over the bandwidth indicated by CH\_BANDWIDTH as described in 24.3.8.2.1.3 (LTF definition). If format is S1G\_DUP\_2M, generate the LTF1 field sequence in the frequency-domain over a 2MHz bandwidth. |
| 8214 | Naveen Kakani | 415.55 | 24.3.4.4.2 | Step ‘a’ should be texted separately for non-duplicate and duplicate mode as given in the resolution table below in the relevant section | Separate the text for non-duplicate and duplcate mode. | Revised.  Instruction to Editor:In Section 24.3.4.4.2, P.L: 415.55  Remove current bullet a) and replace with a) and b) as shown below:  a) Determine FORMAT from TXVECTOR  b) Sequence generation: If FORMAT is S1G, generate the LTF1 field sequence in the frequency-domain over the bandwidth indicated by CH\_BANDWIDTH as described in 24.3.8.3.3 (LTF definition). If FORMAT is S1G\_DUP\_1M, generate the LTF1 field sequence in the frequency-domain over a 1MHz bandwidth. |

**Discussion:**

**24.3.4.3 Construction of the Preamble part in an S1G\_SHORT PPDU**

Section 24.3.4.3.2 describes construction of Preamble in S1G SHORT PPDU. Step ‘b, sequence generation in LTF construction depends on CH\_BANDWIDTH parameter defined in step ‘a’. Again, if we look at Table 24-2 (shown below) CH\_BANDWIDTH is CBW4 when an S1G PPDU of 4 MHz or S1G\_DUP\_2M is transmitted and similar is the case with 8 and 16 MHz transmission with and without duplicate mode.



The LTF1 sequence used for S1G\_DUP\_2M with CBW4 should be different from the LTF1 sequence used for S1G with CBW4. Detailed explanations are as follows.

The DATA field signal is defined in 24.3.9.12.2.2 Equation (24-60):



For each 2MHz sub-band, data and pilot symbols are loaded on subcarrier . For CBW4, the loaded subcarriers are:

However, the LTF defined for HT/VHT 40MHz is:



This LTF sequence is not aligned with the subcarrier indexing of the DATA field in S1G\_DUP\_2M. If we use this LTF sequence for S1G\_DUP\_2M, we can’t perform LTF channel estimation on subcarrier -60, -59, 59, and 60 while these 4 subcarriers are loaded with data symbols.

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Commenter** | **P.L** | **Clause** | **Comment** | **Proposed Change** | **Resolution** | |
| 8215 | Naveen Kakani | 474.4 | 24.3.9.12.2 | Gamma values are not explicitly defined to generate data field of 2 MHz duplicated transmission. Equation (24-6)-(24-20) defines it for only non-duplicate mode. | Define Gamma values | Revised.  Instruction to Editor: please apply the proposed changes described on Page 4-5 of doc. IEEE-802.11-15-1491r0 |

**Discussion:**

**1 MHz and 2 MHz duplicate transmission:** **Section 24.3.9.12:**

This section gives the mathematical equation for the data field for both 1 MHz and 2 MHz duplicate transmission. For 1 MHz duplicate transmission the phase rotation or gamma values are clearly defined in equation 24-10 – 24-13. For >=2 MHz transmissions on the other hand, the gamma values are defined only for non-duplicated S1G transmission (equation 24-6 -24-9). Equations should also cover the S1G\_DUP\_2M cases.

**Proposed change**

**Modify the text immediately before Equations 24-7 to 24-13 as shown below. Changes should be at P.L: 432.36**

**~~For a 4 MHz PPDU transmission,~~**

**For 4MHz PPDU transmissions of S1G or S1G\_DUP\_2M packets**

**~~For a 8 MHz PPDU transmission,~~**

**For 8 MHz PPDU transmissions of S1G or S1G\_DUP\_2M packets**

**~~For a 16 MHz PPDU transmission,~~**

**For 16 MHz PPDU transmissions of S1G or S1G\_DUP\_2M packets**

**~~For a 2 MHz transmission using 1 MHz duplicated mode,~~**

**For 2 MHz transmissions of S1G\_DUP\_1M packets,**

**~~For a 4 MHz transmission using 1 MHz duplicated mode,~~**

**For 4 MHz transmissions of S1G\_DUP\_1M packets,**

**~~For a 8 MHz transmission using 1 MHz duplicated mode,~~**

**For 8 MHz transmissions of S1G\_DUP\_1M packets,**

**~~For a 16 MHz transmission using 1 MHz duplicated mode,~~**

**For 16 MHz transmissions of S1G\_DUP\_1M packets,**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Commenter** | **P.L** | **Clause** | **Comment** | **Proposed Change** | **Resolution** |
| 8216 | Naveen Kakani | 440.52 | 24.3.8.2.1.5 | Maximum degree of the polynomial should be 3.  The order of cofficients in the equation should be reversed. As per the diagram, it is not correct. | Ln 52:  Change crc(D) =  **To** | Accepted. |


**Discussion:**

**24.3.8.2.1.5 CRC calculation for S1G SIG-A fields:**

The CRC polynomial is given as,

cid:image002.png@01D05D96.25360840

Looking at the diagram in figure (24-10), page 441, it seems the maximum degree should be 3 and the order of cofficients should be reversed.



D4

D3

D2

D1

D0

Figure 24-10 above is consistent with the generating polynomial:



Accordingly, the CRC should be written as C3D3 + C2D2 + C1D1 + C0D0.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Commenter** | **P.L** | **Clause** | **Comment** | **Proposed Change** | **Resolution** |
| 8217 | Naveen Kakani | 416.30, | 24.3.4.4.3, | BCC interleaver should be encoded as per legacy interleaver (section 18.3.5.7) or VHT interleaver (section 22.3.10.8)?  Section 24.3.4.4.3 and section 24.3.8.3.4 (points to clause 24.3.9 which defines BCC interleaver in section 24.3.9.8) should specify identical interleaver encoding. | Change “c)BCC interleaver: Interleave as described in 18.3.5.7 (Data interleaving).”  To  **“c)BCC interleaver: Interleave as described in 24.3.9.8 (BCC interleaver).** | Revised**.**  Instruction to Editor: please apply the proposed changes highlighted on Page 6-7 of doc. IEEE-802.11-15-1491r1 |
| 8218 | Naveen Kakani | 464.44 | 24.3.9.8 | BCC interleaver should be encoded as per legacy interleaver (section 18.3.5.7) or VHT interleaver (section 22.3.10.8)?  Section 24.3.4.4.3 and section 24.3.8.3.4 (points to clause 24.3.9 which defines BCC interleaver in section 24.3.9.8) should specify identical interleaver encoding. | Change “c)BCC interleaver: Interleave as described in 18.3.5.7 (Data interleaving).”  To  **“c)BCC interleaver: Interleave as described in 24.3.9.8 (BCC interleaver).** | Revised**.**  Instruction to Editor: please apply the proposed changes highlighted on Page 6-7 of doc. IEEE-802.11-15-1491r1 |

**Discussion:**

We realize that for Nss = 1, legacy interleaver is a special case of VHT interleaver with N\_ROW = 3 and N\_COL = 16 (described in 18.3.5.7 and 22.3.10.8). However, Table 24-20 specifies N\_ROW and N\_COL specifically for 1 MHz interleaver encoding which is not equal to the one specified for VHT, hence the section 24.3.4.4.3 Construction of 1 MHz SIG should reference this section (24.3.9.8) containing Table 24-20 instead of 18.3.5.7.

**(Instruction to Editor: Replace striked out text with new section reference)**

**24.3.4.4.3 Construction of 1 MHz SIG**

1. Obtain the STBC, NUM\_STS, GI\_TYPE, FEC\_CODING, MCS, SMOOTHING, LENGTH, AGGREGATION, RESPONSE\_INDICATION, NDP\_INDICATION and DOPPLER from the TXVECTOR. Add the reserved bits, append the calculated 4 bit CRC, then append the *N*tail tail bits **as shown in 24.3.8.3.4 (SIG definition).** This operation gives as a result 36 uncoded bits.
2. BCC encoder: Encode the data by a convolutional encoder at the rate of R=1/2 as described in

18.3.5.6 (Convolutional encoder) and apply the block-wise 2 times repetition on a per-OFDM

symbol basis.

c) BCC interleaver: Interleave as described in **~~18.3.5.7~~** ~~(Data interleaving)~~**24.3.9.8 (BCC interleaver)**.