IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| CID 5880 | | | | |
| Date: 12/8/2015 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Sigurd Schelstraete | Quantenna Communications | 3450 W. Warren Ave Fremont, CA 94538 | +1 510 743 2288 | sigurd@quantenna.com |
|  |  |  |  |  |

Abstract

This document proposes a resolution for CID 5880.

CID 166

# Introduction

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| 5880 | 8.7.1 | 1228 | 45 | It would be nice to indicate "A-MPDU pre-EOF padding" in the figure | Add arrow showing beginning to end of A-MPDU pre-EOF padding |

# Text Changes

Proposed change:

Replace Figure 8-720 with:

