IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Resolution of CIDs 4776 and 4777 | | | | |
| Date: 2016-02-18 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Dan Harkins | HPE | 1322 Crossman avenue, Sunnyvale, California, United States of America | 408 555 1212 | dharkins at arubanetworks dot com |
|  |  |  |  |  |

Abstract

This submission proposes resolution to CIDs 4776 and 4777

CIDs 4776 and 4777 have identical comments of “The len() function is not described” and identically propose the obvious: “State that it returns the length of its argument in bits.”

Discussion: like to agree but the proposed resolution does not propose anything an editor can work with.

Resolution: Counter: function defined per document 11-16/0280

***Instruct the editor to modify section 12.4.4.2.2 as indicated:***

**12.4.4.2.2 Generation of the password element with ECC groups**

where KDF-Hash-Length is the key derivation function defined in 12.7.1.7.2 (Key derivation function (KDF)) using the hash algorithm defined by the AKM in Table 9-132 (AKM suite selectors) to generate a key of length Length, and len() returns the length of its argument in bits.

***Instruct the editor to modify section 12.4.4.3.2 as indicated:***

**12.4.4.3.2 Generation of the password element with FFC groups**

where KDF-Hash-Length is the key derivation function defined in 12.7.1.7.2 (Key derivation function (KDF)) using the hash algorithm defined by the AKM in Table 9-132 (AKM suite selectors) to generate a key of length Length, and len() returns the length of its argument in bits.

**References:**