IEEE P802.11
Wireless LANs

|  |
| --- |
| CID 8022, 8023, 8024 resolution text |
| Date: 2016-07-15 |
| Author(s): |
| Name | Affiliation | Address | Phone | Email |
| Thomas Handte | Sony Europe Ltd. | Hedelfinger Str. 61,70327 Stuttgart, Germany | +49-711-5858-236 | thomas.handte@eu.sony.com |
|  |  |  |  |  |

Abstract

This contribution is provided as possible resolution of CID 8022, 8023, 8024.

The changes are relative to Draft P802.11REVmc\_D6.0 [1].

## Comment

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| 8022 | 2471,22 |  | (Submitted for Thomas Handte)Table heading is LDPC code rates. However code rate 7/8 is missing. | Add code rate 7/8 to the table | EDITOR |

## Discussion

DMG has a new code rate 7/8. Table 20-20 provides an overview of LDPC code features, but code rate 7/8 is missing.

## Proposed changes:

*All changes are in reference to D6.0 [1]*

****

|  |  |  |
| --- | --- | --- |
| 7/8 | 624 | 546 |

**Comments**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| 8023 | 2472.23 |  | (Submitted for Thomas Handte)LDPC with code rate 7/8 is defined by puncturing of LDPC with CR 13/16. This is likely suboptimal in terms of coding gain and decoder iterations. | Either make a proper definition of a LDPC code table like for code rates 1/2 to 13/16 as in subclause 20.3.8 or consider a distributed rather than a block puncturing. | GEN |
| 8024 | 2472.23 |  | (Submitted for Thomas Handte)LDPC with code rate 7/8 has a lower CW length as other LDPC codes. However, long CW length is a prerequisite for good error performance in channel with strong phase noise. | It is favorable to design a code rate 7/8 LDPC with 588 data and 84 parity bits. | GEN |

## Discussion

The LDPC code with code rate 7/8 has suboptimal performance for the reasons mentioned. However, performance loss is rather small and due to timing pressure of REVmc, I would like to withdraw CID 8023 and 8024 and consider a proposal in TGay.

## References

 [1] Draft P802.11REVmc\_D6.0