IEEE P802.11
Wireless LANs

|  |
| --- |
| DCM TBDs |
| Date: 2016-09-12 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Sriram VenkateswaranRon Porat | Broadcom | 190 Mathilda Place, Sunnyvale, CA 94096 | +1-408-922-7684 | sriram.venkateswaran@broadcom.com |

­­Line 38-39 in Page 244 of D0.4 has the following line: “DCM is only applicable to MCS 0, 1, 3 and 4 with up to TBD number of streams and for TBD RU sizes.”

Propose to replace with the following line “DCM is only applied to MCS0, MCS 1, MCS 3 and MCS 4. DCM is applied only with Nss = 1 or 2 (in the case of single user RU in an HE MU PPDU, Nss,r,u = 1 or 2).”

**Suggest to resolve TBDs in lines 38-39 in Page 244 of D0.4 as follows:**

~~DCM is only applicable to MCS 0, 1, 3 and 4 with up to TBD number of streams and for TBD RU sizes.~~ DCM is only applied to MCS0, MCS 1, MCS 3 and MCS 4. DCM is applied only with Nss = 1 or 2 (in the case of single user RU in an HE MU PPDU, Nss,r,u = 1 or 2).