IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| A-BFT | | | | |
| Date: 2016-12-15 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Yan Xin | Huawei Technologies Co., Ltd. | Suite 400, 303 Terry Fox Drive, Kanata, Ontario K2K 3J1 | +1 613 9791792 | yan.xin@huawei.com |
| Sang G. Kim | LG Electronics | 10225 Willow Creek Rd, San Diego CA 92131 | +1-858-635-5294 | sanggook.kim@lge.com |
| Carlos Cordeiro | Intel |  |  | carlos.cordeiro@intel.com |
|  |  |  |  |  |

Abstract

This submission provides normative text corresponding to Subsection 3.2.3 A-BFT of the 11ay SFD.

**Notice:** This document has been prepared to assist IEEE 802.11. It is offered as a basis for discussion and is not binding on the contributing individual(s) or organization(s). The material in this document is subject to change in form and content after further study. The contributor(s) reserve(s) the right to add, amend or withdraw material contained herein.

**Release:** The contributor grants a free, irrevocable license to the IEEE to incorporate material contained in this contribution, and any modifications thereof, in the creation of an IEEE Standards publication; to copyright in the IEEE’s name any IEEE Standards publication even though it may include portions of this contribution; and at the IEEE’s sole discretion to permit others to reproduce in whole or in part the resulting IEEE Standards publication. The contributor also acknowledges and accepts that this contribution may be made public by IEEE 802.11.

**Patent Policy and Procedures:** The contributor is familiar with the IEEE 802 Patent Policy and Procedures <[http:// ieee802.org/guides/bylaws/sb-bylaws.pdf](#_blank)>, including the statement "IEEE standards may include the known use of patent(s), including patent applications, provided the IEEE receives assurance from the patent holder or applicant with respect to patents essential for compliance with both mandatory and optional portions of the standard." Early disclosure to the Working Group of patent information that might be relevant to the standard is essential to reduce the possibility for delays in the development process and increase the likelihood that the draft publication will be approved for publication. Please notify the Chair <[stuart@ok-brit.com](mailto:stuart.kerry@nxp.com)> as early as possible, in written or electronic form, if patented technology (or technology under patent application) might be incorporated into a draft standard being developed within the IEEE 802.11 Working Group. **If you have questions, contact the IEEE Patent Committee Administrator at <**[patcom@ieee.org](mailto:patcom@ieee.org#_blank)**>**.

* + 1. A-BFT

3.2.3.1 A-BFT over multiple channels in TGay

Modification to “802.11-2016”

**10.38.5 Beamforming in A-BFT**

**10.38.5.1 Allocation of A-BFT**

***Insert the following paragraph after the fourth paragraph of 10.38.5.1***

An EDMG PCP or AP may schedule an A-BFT that spans more than one channel. An EDMG STA that supports this type of A-BFT may access the A-BFT over the different channels where the A-BFT is scheduled.

**10.38.5.2 Operation during the A-BFT**

***Insert the following subclause 10.38.5.2a (including Figure 10-69 and Figure 10-70) after the last paragraph of 10.38.5.2***

**10.38.5.2a A-BFT over multiple channels**

When the EDMG PCP/AP and EDMG STAs in a BSS or PBSS have capabilities to operate over multiple channels, an EDMG STA can transmit SSW frames to the EDMG PCP/AP and the EDMG PCP/AP can transmit an SSW Feedback frame to an EDMG STA over either the primary channel or a secondary channel with the bandwidth of 2.16 GHz. The A-BFT for a DMG STA operates over the primary channel only.

In EDMG, the A-BFT is slotted in the time domain as it in DMG (10.38.5.2). The random backoff procedure for selecting an SSW slot can be specified as that a DMG STA or an EDMG STA randomly selects a SSW slot number from a uniform distribution [0, A-BFT Length-1], where A-BFT Length is the value in the A-BFT Length subfield in the last received DMG Beacon. In the frequency domain, the EDMG STA selects either the primary channel or a secondary channel randomly with the uniform distribution based on the *BSS Operating Channels* in the *EDMG Operation element*. Then SSW frames shall be sent on the selected SSW slot and the selected channel.

The EDMG PCP/AP transmits an SSW-Feedback frame to an STA over the channel on which the SSW frames are sent from that STA to the EDMG PCP/AP. In the case that there is no SSW slot collision due to the random backoff procedure at the start of A-BFT, the SSW-Feedback frame for an STA is sent in the same SSW slot as which the SSW frames are sent from this STA to the EDMG PCP/AP. Otherwise, in the case that there is an SSW slot collision due to the random backoff procedure at the start of A-BFT, the SSW-Feedback frames for SSW slot-collided STAs may be sent in the next available SSW slot(s) if the best Sector ID/Antenna ID in the EDMG PCP/AP for the directions to STAs are different (as shown in Figure 10-69); or the SSW-Feedback frames for SSW slot-collided STAs may be sent in the same SSW slot in which the SSW frames are sent from the STAs over different channels if the best Sector ID/Antenna ID in the EDMG PCP/AP for the directions to the STAs are the same (as shown in Figure 10-70).

**Example of A-BFT with A-BFT Length = 8 over the primary channel and a secondary channel (the same assumption as in Figure 10-68). A possible contention between 3 STAs is shown in the figure below:** STAs A, B and C are competing for access. All STAs choose a random value between [0,7]. STA A chooses value = 2, while STAs B and C choose value = 5. STA B is a DMG STA and STAs A and C are EDMG STAs. STA B can only select the primary channel while STAs A and C select the primary channel and the secondary channel, respectively. Although STAs B and C collide on SSW slot #5, STAs B and C transmit SSW frames over different channels permitting the EGDM PCP/AP to correctly decode the SSW frames sent from STA B and STA C simultaneously. The SSW-Feedback frames for STAs A and B are sent from the EDMG PCP/AP in the same SSW slots (SSW slot #2 and SSW slot #5) in which the SSW frames are sent from STAs A and B respectively. The SSW-Feedback frame for STA C is sent in a next available SSW slot (e.g., SSW slot #6) if the best Sector ID/Antenna ID in the EDMG PCP/AP for the directions to STA B and SAT C are different.

**Figure 10-69 – EDMG A-BFT over multiple channels (the best Sector ID/Antenna ID in the EDMG PCP/AP for the directions to STA B and SAT C are different).**

**Example of A-BFT with A-BFT Length = 8 over the primary channel and a secondary channel (the same assumption as in Figure 10-68). A possible contention between 3 STAs is shown in the figure below:**

Transmission of SSW frames is the same as that in Figure 9-56A. The SSW-Feedback frames for STAs A and B are sent from the EDMG PCP/AP in the same SSW slots (SSW slot #2 and SSW slot #5) over the primary channel, in which the SSW frames are sent from the STAs respectively. If the best Sector ID/Antenna ID in the EDMG PCP/AP for the directions to STA B and SAT C are the same, the SSW-Feedback frame for STA C can also be sent in the SSWS slot #5 but over the secondary channel.

**Figure 10-70 – EDMG A-BFT over multiple channels (the best Sector ID/Antenna ID in the EDMG PCP/AP for the directions to STA B and SAT C are the same).**

3.2.3.2 Dynamic load balance in A-BFT

Modification to “802.11-2016”

**10.38.5.2 Operation during the A-BFT**

…

Each STA maintains a counter, FailedRSSAttempts, of the consecutive number of times the STA initiates RSS during A-BFTs but does not successfully receive an SSW-Feedback frame as a response. If FailedRSSAttempts exceeds dot11RSSRetryLimit, the STA shall select a backoff count as a random integer drawn from a uniform distribution [0, dot11RSSBackoff), i.e., 0 to dot11RSSBackoff – 1. The responder shall decrement the backoff count by one at the end of each A-BFT period in the following beacon intervals. The responder may re-initiate RSS only during an A-BFT when the backoff count becomes zero. The STA shall set FailedRSSAttempts to 0 upon successfully receiving an SSW-Feedback frame during the A-BFT.

***Insert the following paragraph as follows:***

The RSSRetryLimit and RSSBackoff subfields in the EDMG Operation element are used for the purpose of dynamic load balancing in A-BFT. Each EDMG STA follows the same RSS operation as DMG STA using RSSRetryLimt and RSSBackoff parameters instead of dot11RSSRetryLimit and dot11RSSBackoff, respectively.