IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Maximum TRN field duration | | | | |
| Date: 2017-03-02 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Claudio da Silva | Intel |  |  | claudio.da.silva@intel.com |
| Carlos Cordeiro |  |  |  |  |

Abstract

This document suggests text that defines a maximum duration for the TRN field of EDMG PPDUs.

**Discussion**

* In the current version of the draft (D0.2), the duration of the TRN field is limited only by:
  + The maximum number of TRN-Units (8 bits, 255)
  + The maximum values of EDMG TRN-Unit P and EDMG TRN-Unit M
  + The total duration of the PPDU itself
* As a result,
  + For the (EDMG TRN-Unit P = 2, EDMG TRN-Unit M = 6) configuration, the maximum TRN field duration is 8\*255 + 2 = 2042 TRN subfields (~891 us)
  + For the (EDMG TRN-Unit P = 2, EDMG TRN-Unit M = 8) configuration, the maximum TRN field duration is 10\*255 + 2 = 2552 TRN subfields (~1.11 ms)
  + For the (EDMG TRN-Unit P = 4, EDMG TRN-Unit M = 16) configuration, the maximum TRN field duration would be 20\*255 + 4 = 5104 TRN subfields (~2.22 ms), which is greater than the maximum PPDU duration.
* Going into more detail,
  + Only necessary to limit EDMG BRP-TX.
  + To enable practical implementations, instead of limiting the duration of the TRN field, it is actually only necessary to define a maximum number of possible AWVs trained in the EDMG BRP-TX packet, which is given by
  + Observations
    - Number of TRN subfields used for channel estimation has no impact
    - Repetition factor does have an impact 🡪 only one measurement/feedback is made for each EDMG TRN-Unit N TRN subfields.
* Proposal:
  + Limit:
  + Allows both mandatory modes to be used with the maximum number of TRN-Units.
  + The limit is always satisfied when .
    - Only necessary to define a limit for EDMG BRP-TX packets with .
    - For similar reason, it is also not necessary to define limit for EDMG BRP-RX/TX packets.
* Example 1: For (EDMG TRN-Unit P = 2, EDMG TRN-Unit M = 8, EDMG TRN-Unit N = 1), the maximum number of TRN-Units is
  + Number of TRN-Units may be equal to its maximum.
* Example 2: And when (EDMG TRN-Unit P = 4, EDMG TRN-Unit M = 16, EDMG TRN-Unit N = 1), the maximum number of TRN-Units is
  + For “long” configurations, we wouldn’t be able to set the number of TRN-Units used to its maximum when EDMG TRN-Unit N = 1 🡪 In this case, more than one packet would have to be used.

30.9.2.2.5 TRN field definition

*Insert the following paragraph:*

For transmitted EDMG BRP-TX packets with the value of the EDMG TRN-Unit N field in the EDMG-Header-A equal to 1, the EDMG TRN Length field in the EDMG-Header-A shall be less than or equal to 2040/M, where M is the value of the EDMG TRN-Unit M field in the EDMG-Header-A.

**Straw Poll**

Do you agree that the text in contribution 17/0278r0 shall be incorporated into the next draft 11ay specification?

**References:**