IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Comment resolution on CID 7517 for 28.3.11.5 Coding | | | | |
| Date: 2017-02-08 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | Email |
| Jianhan Liu | Mediatek |  |  | Jianhan.liu@mediatek.com |

Abstract:

This document contains comment resolution on the following CID 7517 for 28.3.11.5 Coding:

.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Clause** | **Page** | **Line** | **Comment** | **Proposed Change** | **Resolution** |
| 7517 | 28.3.11.5.4 | 321 | 47 | "a\_init" should be changed to "a" | As per comment | Revised.  11ax editor, please see the discussion for instructions in doc IEEE802.11-17/0436r0. |

**Discussions for CIDs 7517:**

***TGax Editor: Please make the following text change (changed texts are in red) theline 47, page 321* *of D1.0***:

represented by *ainit* for users encoded by LDPC, and represented by *a* for users encoded by BCC,