IEEE P802.11
Wireless LANs

|  |
| --- |
| Length Calculation in EDMG PPDU |
| Date: 2017-05-09 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| SungJin Park | LG Electronics | Yangjae-daero 11gil, Seocho-gu, Seoul, 137-893, Korea |  | allean.park@lge.com |
| Hiroyuki Motozuka  | Panasonic |  |  | motozuka.hiroyuki@jp.panasonic.com |
|  |  |  |  |  |

Abstract

This document proposes draft changes to include the equation to set Length field and Training Length field within L-Header in an EDMG PPDU.

Proposed text: equation to set Length field in L-Header

**30.3.3.2.6 L-Header definition**

*Insert the following after the second paragraph:*

Note: Example of the L-Header fields calculation for an EDMG PPDU

1. The tentative number of SC symbol blocks, is calculated as follows:
2. .The Base MCS field is set to the value such that the following conditions are met:

If and , the Base MCS field shall be set to the value that is greater than 5.

1. The number of SC symbol blocks, , and the value of the Training Length field, , are calculated as follows:

If the Base MCS > 5 (QPSK and 16QAM)

End

If the Base MCS 5 (BPSK) and

If

Else

 and is calculated as follows:

If

Else

End

End

End

1. The maximum length of PSDU, is calculated as follows:

 =

1. The spoofed length of PSDU with compressed BW, is calculated as follows:

If

 =

Else

 =

End

When the Base MCS field is set to 1, the calculated *Length* may not satisfy the requirement for the spoofing error (see 30.3.3.2.6 L-Header definition.) In that case, the Base MCS field shall be set to a value different from 1, and the *Length* and the Training Length shall be calculated by repeating c) to e).