IEEE P802.11
Wireless LANs

|  |
| --- |
| 20.2.3 PHYCONFIG\_VECTOR Parameters |
| Date: 2017-11-19 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Artyom Lomayev | Intel | Turgeneva 30, Nizhny Novgorod 603024, Russia | +7 (831) 2969444 | artyom.lomayev@intel.com |
| Alexander Maltsev | Intel  |  |  | alexander.maltsev@intel.com |
| Claudio da Silva | Intel |  |  | claudio.da.silva@intel.com |
| Carlos Cordeiro | Intel  |  |  | carlos.cordeiro@intel.com |

Abstract

This document proposes specification text for subclause 20.2.3 (PHYCONFIG\_VECTOR parameters), [1], [2].

*Editor: add subclause 20.2.3 PHYCONFIG\_VECTOR parameters to [2]*

**20.2.3 PHYCONFIG\_VECTOR parameters**

The PHYCONFIG\_VECTOR carried in a PHY-CONFIG.request primitive for a DMG PHY contains an OPERATING\_CHANNEL parameter, which identifies the operating 2.16 GHz channel. The PHY shall set the channel number using the value of this parameter defined in the range from 1 to 11.

*Editor: introduce changes into the 20.3.1 Channelization subclause in [2] as below*

**20.3.1 Channelization**

The DMG PHY operates in the channels defined in Annex E and shall support at least channel number 2. The channelization used by DMG STAs is shown in Figure 1.



Figure 1: Channelization used by DMG STAs

The channel center frequency is defined as:

Channel center frequency = Channel starting frequency + Channel spacing × Channel number

where channel starting frequency, channel spacing and channel number are as defined in Annex E.

The OPERATING\_CHANNEL parameter of PHYCONFIG\_VECTOR is used to set up the operating channel number. The OPERATING\_CHANNEL can be set to 1, 3, 5, 7, 9, or 11. The relation between the channel number and OPERATING\_CHANNEL is defined as follows:

Channel number = ½ × (OPERATING\_CHANNEL + 1)

**SP:**

Do you agree to include the proposed text for “20.2.3 PHYCONFIG\_VECTOR parameters” proposed in (11-17-1810-00-000m 20 2 3 PHYCONFIG\_VECTOR Parameters) into the Draft P802.11REVmd\_D0.4?

**References:**

1. IEEE 802.11-2016
2. Draft P802.11REVmd\_D0.4