IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Comment resolutions for 26.8.36 | | | | |
| Date: 2018-01-05 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Alfred Asterjadhi | Qualcomm Inc. | 5775 Morehouse Dr, San Diego, CA 92109 | +1-858-658-5302 | aasterja@qti.qualcomm.com |
| George Cherian | Qualcomm Inc. |  |  |  |
| Abhishek Patil | Qualcomm Inc. |  |  |  |

Abstract

This submission proposes resolutions for multiple comments related to TGax D2.0 with the following CIDs:

* 12046 (1 CID)

Revisions:

* Rev 0: Initial version of the document.

Interpretation of a Motion to Adopt

A motion to approve this submission means that the editing instructions and any changed or added material are actioned in the TGax Draft. This introduction is not part of the adopted material.

***Editing instructions formatted like this are intended to be copied into the TGax Draft (i.e. they are instructions to the 802.11 editor on how to merge the text with the baseline documents).***

***TGax Editor: Editing instructions preceded by “TGax Editor” are instructions to the TGax editor to modify existing material in the TGax draft. As a result of adopting the changes, the TGax editor will execute the instructions rather than copy them to the TGax Draft.***

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Commenter** | **P.L** | **Comment** | **Proposed Change** | **Resolution** |
| 12046 | Jarkko Kneckt | 161.19 | There is only TWT element, no broadcast TWT element. | Change Broadcast TWT element to TWT element, or clarify that it is a TWT elemetn with Broadcast subfield set to 1. | Revised –  Agree with comment. Proposed resolution clarifies the condition as suggested by the proposed change (i.e., the element is not called Broadcast TWT and it is simply a TWT element with Broadcast subfield set to 1.  TGax editor to make the changes shown in 11-18/0010r0 under all headings that include CID 12046. |

**Discussion: *None.***

* FILS Discovery frame format

**TGax Editor: *Change the table below of this subclause as follows (#CID 12046):***

Change Table 9-325a (FILS Discovery frame format) as follows (only modified rows are shown):

|  |  |  |
| --- | --- | --- |
| * FILS Discovery frame format | | |
| Order | Information | Notes |
| ~~6~~ | ~~Vendor Specific element~~ | ~~One or more Vendor Specific elements are optionally~~  ~~present.~~ |
| 7 | TIM element | The TIM element is optionally present when dot11HEOptionImplemented is true, otherwise it is not present.(#3046) |
| 8 | TWT element | The TWT element is optionally present when dot11HEOptionImplemented is true and the Broadcast field of the TWT element is 1, otherwise it is not present. (#12046) (#9958) |