IEEE P802.11
Wireless LANs

|  |
| --- |
| Resolution for CIDs in 9.4.2.245 |
| Date: January 8, 2018 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Abhishek Patil | Qualcomm Inc. |  |  | appatil@qti.qualcomm.com |
| Alfred Asterjadhi | Qualcomm Inc. |  |  | aasterja@qti.qualcomm.com |
| George Cherian | Qualcomm Inc. |  |  | gcherian@qti.qualcomm.com |

Abstract

This submission proposes resolutions for following CIDs received for TGax LB230 (3): 11551, 11707, 13182

Revisions:

* Rev 0: Initial version of the document.

Interpretation of a Motion to Adopt

A motion to approve this submission means that the editing instructions and any changed or added material are actioned in the TGax Draft. This introduction is not part of the adopted material.

***Editing instructions formatted like this are intended to be copied into the TGax Draft (i.e. they are instructions to the 802.11 editor on how to merge the text with the baseline documents).***

***TGax Editor: Editing instructions preceded by “TGax Editor” are instructions to the TGax editor to modify existing material in the TGax draft. As a result of adopting the changes, the TGax editor will execute the instructions rather than copy them to the TGax Draft.***

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Commenter** | **Pg / Ln** | **Section** | **Comment** | **Proposed Change** | **Resolution** |
| 11551 | Dorothy Stanley | 159.39 | 9.4.2.245 | In Table 9-262ag. 0-62 does not match -100 dBm to -37 dBm. Need to change to -38 | as in comment | RevisedAgree with the comment.Replaced -37 with -38 in Table 9-262ag to make the range consistent**TGax editor, please make changes as showing in document 11-18/0066r0 under CID 11551** |
| 11707 | Evgeny Khorov | 159.39 | 9.4.2.245 | Unequal number of values | Replace -37 dBm with -38dBm | RevisedReplaced -37 with -38 in Table 9-262ag to make the range consistent**TGax editor, please make changes as showing in document 11-118/0066r0 under CID 11707** |
| 13182 | Rajesh Kumar | 159.39 | 9.4.2.245 | The numbers don't add up (0 to 62 =! -100 to -37) | Either change Value to 0-63 (and remove the second row in Table 9-262ag) or change Description to say -100 dBm to -38 dBm | RevisedReplaced -37 with -38 in Table 9-262ag to make the range consistent**TGax editor, please make changes as showing in document 11-18/0066r0 under CID 13182** |

*
* ESS Report element(#5163)

TGax Editor: Please make the following changes to Table 9-262ag (11ax D2.0 P159L34):

|  |
| --- |
| * **Recommended BSS Transition Threshold Within ESS subfield encoding**
 |
| **Value** | **Description** |
| 0–62 | –100 dBm to –38 dBm |
| 63 | No recommendation |