IEEE P802.11
Wireless LANs

|  |
| --- |
| 11ax D2.0 Comment Resolution 27.5.3.2.4 remaining CIDs |
| Date: 2018-03-01 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Liwen Chu | Marvell |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

Abstract

This submission proposes resolutions for multiple comments related to TGax D2.0 with the following CIDs:

* 11316, 12505, 12506.

Revisions:

* .

Interpretation of a Motion to Adopt

A motion to approve this submission means that the editing instructions and any changed or added material are actioned in the TGax Draft. This introduction is not part of the adopted material.

***Editing instructions formatted like this are intended to be copied into the TGax Draft (i.e. they are instructions to the 802.11 editor on how to merge the text with the baseline documents).***

***TGax Editor: Editing instructions preceded by “TGax Editor” are instructions to the TGax editor to modify existing material in the TGax draft. As a result of adopting the changes, the TGax editor will execute the instructions rather than copy them to the TGax Draft.***

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **PP** | **LL** | **Comment** | **Proposed Change** | **Resolution** |
| 11316 | 248 | 8 | Logically the third paragraph should be the first paragraph. And the first and second paragraph should be one paragraph that covers: An AP that sends a Trigger frame and 1)receives an HE TB PPDU ... 2) does not receive any HE TB PPDU ... | Organize these three paragraphs as suggested in the comment. | **Revised****Discussion: generally agree with the commenter. Subclause 27.5.3.2.4 is rewritten per CID 13916. No change is needed.**  |
| 12505 | 248 | 13 | if the Trigger solicits the first responding frames in the TXOP. Otherwise PIFS or backoff recovery is applied. | Fix the issue mentioned in comment. | **Revised****Discussion: generally agree with the commenter. Subclause 27.5.3.2.4 is rewritten per CID 13916 and PIFS recovery is allowed. No change is needed.** |
| 12506 | 248 | 18 | primary AC is defined when the backoff is successful. Trigger frame transmission can be transmitted in an A-MPDU with any primary AC. | Change to "the primary AC rules are applied" | **Revised****Discussion: generally agree with the commenter. Subclause 27.5.3.2.4 is rewritten per CID 13916 and the rules in subclause 10.22 (primary AC etc.) are used. No change is needed.** |