IEEE P802.11
Wireless LANs

|  |
| --- |
| Comment Resolution for EDMG Channel Access CIDs |
| Date: 2018-05-07 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| SungJin Park | LG Electronics | Yangjae-daero 11gil, Seocho-gu, Seoul, 137-893, Korea |  | allean.park@lge.com |
| JinMin Kim | LG Electronics |  |  | jinmin1230.kim@lge.com |
| Saehee Bang | LG Electronics |  |  | saehee.bang@lge.com |
| SunWoong Yun | LG Electronics |  |  | sunwoong.yun@lge.com |
| Jinsoo Choi | LG Electronics |  |  | js.choi@lge.com |
| Sanggook Kim | LG Electronics | San Diego/California/US |  | sanggook.kim@lge.com |

Abstract

This document proposes resolutions for EDMG channel access CIDs.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **CID** | **Page** | **Clause** | **Comment** | **Proposed Change** |
| 1010 | 113.27 | 10.22.2.12 | Idle channel In Table 20 is incorrect. | Change "Primary" to "None", "First secondary channel" to "Primary channel", "Second secondary channel" to "Primary channel and first secondary channel", and "Third secondary channel" to "Primary channel, first secondary channel and second secondary channel". |
| 1012 | 114.20 | 10.22.2.12 | If the action d) is allowed even if secondary or secondary1 channel is busy, for example, primary and secondary2 are idle whereas secondary and secondary1 is busy, the channel-list parameter should be extended to define exact busy/idle patterns of all subchannels. | Define additional channel-list parameters. For example, define "secondary\_secondary1" which indicates that the secondary and the secondary1 are busy, and the primary and the secondary2 are idle. Similarly, "secondary\_secondary2", "secondary1\_secondary2" and "secondary\_secondary1\_secondary2" might have to be defined. In that case, the channel-list parameter "secondary" should indicate that only the secondary 2.16GHz channel is busy, i.e. the primary, secondary1 and secondary2 are idle.Alternatively, bitmap-type channel-list parameter may be used, like per20MHzbitmap in 802.11ax-D2.0. |

**Proposed resolution:** revised

**Discussion:** There is the mismatch definition of Table 20 (Channels indicated idle by the channel-list parameter) and Table 8-5 (The channel-list parameter elements) in the current draft.

Table 8-5 — The channel-list parameter elements

|  |  |
| --- | --- |
| channel-list parameter | Meaning |
| primary | In an HT STA that is not a VHT STA, indicates that the primary 20 MHz channel is busy.In a VHT STA, indicates that the primary 20 MHz channel is busy according to the rules specified in 21.3.18.5.3.In a TVHT STA, indicates that the primary channel is busy according to the rules specified in 22.3.18.6.3.In an EDMG STA, indicates that the primary 2.16 GHz channel is busy. |
| secondary | In an HT STA that is not a VHT STA, indicates that the secondary channel is busy.In a VHT STA, indicates that the secondary 20 MHz channel is busy according to the rules specified in 21.3.18.5.4.In a TVHT STA, indicates that the secondary channel is busy according to the rules specified in 22.3.18.6.4.In an EDMG STA, indicates that the secondary 2.16 GHz channel is busy. |
| secondary40 | Indicates that the secondary 40 MHz channel is busy according to the rules specified in 21.3.18.5.4.In a TVHT STA, indicates that the secondary TVHT\_2W channel is busy according to the rules specified in 22.3.18.6.4. |
| secondary80 | Indicates that the secondary 80 MHz channel is busy according to the rules specified in 21.3.18.5.4. |
| secondary1 | Indicates that the second secondary channel is busy. |
| secondary2 | Indicates that the third secondary channel is busy. |

Table 20 —Channels indicated idle by the channel-list parameter

|  |  |
| --- | --- |
| PHY-CCA.indication primitive channel-list element | Idle channels |
| Primary | Primary |
| secondary | First secondary channel |
| secondary1 | Second secondary channel |
| secondary2 | Third secondary channel |

The “meaning” described in Table 8-5 for channel-list parameter and the “Idle channels” described in Table 20 for PHY-CCA.indication primitive channel-list element are mismatched. PHY-CCA.indication primitive channel-list element only indicates which channel is busy, not idle channel. In 11ay, the idle channel is the channel which is not present in the channel-list parameter.

**Modification:** modify Table 20 (Channels indicated idle by the channel-list parameter).

*Change the Table 20 as follows*

Table 20 —Channels indicated busy by the channel-list parameter

|  |  |
| --- | --- |
| PHY-CCA.indication primitive channel-list element |  Busy channels |
| Primary | Primary |
| secondary | First secondary channel |
| secondary1 | Second secondary channel |
| secondary2 | Third secondary channel |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **CID** | **Page** | **Clause** | **Comment** | **Proposed Change** |
| 1011 | 114.04 | 10.22.2.12 | "IDLE" and "PHY-CCA.indication (BUSY)" are inappropriate because PHY-CCA.indication (BUSY, secondary/secondary1/secondary2) should be considered for primary idle condition. | "Change ""the STATE parameter of the most recent PHY-CCA.indication primitive was IDLE"" to ""the most recent PHY-CCA.indication primitive was PHY-CCA.indication (IDLE) or PHY-CCA.indication (BUSY, secondary/secondary1/secondary2)"". |

**Proposed resolution:** reject

**Discussion:** “IDLE” means the primary channel is idle and “no PHY-CCA.indication (BUSY) occurred during the period of PIFS” is about the secondary channel. This paragraph talks about the transmission through idle channels including both primary channel and secondary channel. Therefore, original text is correct. Besides, this paragraph is just duplicated from VHT in REVmd.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **CID** | **Page** | **Clause** | **Comment** | **Proposed Change** |
| 1082 | 114.20 | 10.22.2.12 | Why does d) needed? Isn't the 2.16+2.16 GHz mask PPDU already covered by c)? From Figure 3, c) seems to be correct. | Delete case d). |
| 2128 | 114.20 | 10.22.2.1.2 | "Transmit a 2.16+2.16 GHz mask PPDU if the secondary, secondary1 or secondary2 channel was idle during an interval of PIFS immediately preceding the start of the TXOP" How would this apply to secondary channel width? Remove it | As suggested |
| 2332 | 114.16 | 10.22.2.12 | Remove "2.16+2.16 GHz mask PPDU" from an item c because it is redundant with an item d. | As in comment. |

**Proposed resolution:** revised

**Discussion:** transmission of BW mask PPDU depending on the channel width which is 2.16GHz, 4.32GHz, 6.48GHz, 8.64GHz, 2.16+2.16GHz and 4.32+4.32GHz was already resolved in “***11-18-0377-03-00ay-CCA Indication CID***s” as follows:

**10.22.2.12 EDCA channel access in an EDMG BSS***Modify after the fifth paragraph as follow:*

1. Transmit a 8.64 GHz mask PPDU, if primary, secondary, secondary1 and secondary2 channels are contiguous and secondary, secondary1 and secondary2 were idle during an interval of PIFS immediately preceding the start of the TXOP.
2. Transmit a 4.32+4.32 GHz mask PPDU if primary and secondary are contiguous, secondary1 and secondary2 channels are contiguous and secondary, secondary1 and secondary2 channels were idle during an interval of PIFS immediately preceding the start of the TXOP
3. Transmit a 6.48 GHz mask PPDU if primary, secondary and secondary1 channels are contiguous and secondary and secondary1 were idle during an interval of PIFS immediately preceding the start of the TXOP or if primary, secondary1 and secondary2 channels are contiguous and secondary1 and secondary2 were idle during an interval of PIFS immediately preceding the start of the TXOP
4. Transmit a 4.32 GHz mask PPDU if primary and secondary channels are contiguous and secondary channel was idle during an interval of PIFS immediately preceding the start of the TXOP or if primary and secondary1 channels are contiguous and the secondary1 channel was idle during an interval of PIFS immediately preceding the start of the TXOP
5. Transmit a 2.16+2.16 GHz mask PPDU if the secondary, secondary1 or secondary2 channel was idle during an interval of PIFS immediately preceding the start of the TXOP
6. Transmit a 2.16 GHz mask PPDU on the primary channel
7. Restart the channel access attempt by invoking the backoff procedure as specified in 10.22.2 (HCF contention based channel access (EDCA)) as though the medium is busy on the primary channel as indicated by either physical or virtual CS and the backoff timer has a value of 0

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **CID** | **Page** | **Clause** | **Comment** | **Proposed Change** |
| 1216 | 113.27 |  | "channel-list element" - it's not an element | Change "element" to "parameter" |

**Proposed resolution:** Accept

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **CID** | **Page** | **Clause** | **Comment** | **Proposed Change** |
| 1733 | 113.19 | 10.22.2.12 | This seems contradictory with P27L8, which states that a PHY-CCA(IDLE) with the channel list absent means all channels are free. The text here says if the PHY-CCA has a channel list present, then the channels are considered idle. And, surely this is only true if the PHY-CCA.indication had an IDLE STATE parameter. This sentence is just very confusing. | Fix this sentence, or delete, because 8.3.5.12.2 already said everything that needs to be said. |

**Proposed resolution:** reject

**Discussion:** the mentioned paragraphis as follows:

*If the MAC receives a PHY-CCA.indication primitive with the channel-list parameter present, the channels considered idle are defined in Table 20.*

The Table 20 shows which channels are considered idle if the PHY-CCA.indication primitive with the channel-list parameter present. The channel-list parameter is absent when all channels are idle or CCA is determined by a single channel. Besides, this paragraph is just duplicated from VHT in REVmd.

**SP/M:** Do you accept the resolutions of CIDs 1010, 1011, 1012, 1082, 1216, 1733, 2128, and 2332?