### **IEEE P802.11 Wireless LANs**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Spec Text on DFS | | | | |
| Date: 2018-07-DD | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | Email |
| Steve Shellhammer | Qualcomm |  |  | [shellhammer@ieee.org](mailto:shellhammer@ieee.org) |
| Bin Tian | Qualcomm |  |  | [btian@qti.qualcomm.com](mailto:btian@qti.qualcomm.com) |
|  |  |  |  |  |

**Abstract**

This document contains text on “DFS Channel Operation” to be adopted into Draft 0.4.

**Discussion**

According to the SFD [1] operation in DFS channels is disallowed. This document provides specification text regarding this requirement.

[1] Po-Kai Huang, “Specification Framework for TGba,” IEEE 802.11-17/0575r11, March 2018

**Straw Poll**

Do you support the Spec Text in this document 802.11-18/1197r2?

Yes 28

No 0

Abstain 1

**Motion**

Move to adopt the text in IEEE 802.11-18/1197r3 into the next 802.11ba Draft.

Moved: Steve Shellhammer

Second:

---------------------------------------------------------------------------

***Instructions to 802.11ba Editor***

***Editor Instructions: In subclause 32.1 add the text shown in Red.***

A WUR AP shall not transmit a WUR PPDU in an operating class for which the behavior limits set listed in Annex E includes the DFS\_50\_100\_Behavior.