IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| DCM π/2-BPSK EVM Requirement | | | | |
| Date: 2018-08-20 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Claudio da Silva | Intel |  |  | claudio.da.silva@intel.com |
| Artyom Lomayev | Intel |  |  |  |
| Tao Wu | Huawei |  |  | walnut.wutao@huawei.com |
| Yan Xin | Huawei |  |  | yan.xin@huawei.com |

Abstract

This submission proposes EVM requirements for DCM π/2-BPSK signals.

**Discussion**

* Frequency domain diversity for transmissions over 2.16+2.16 GHz or 4.32+4.32 GHz channels.
* After LDPC encoding, encoded bits of each space-time stream are broken into two groups (for a given block): and . Each pair of bits is modulated as follows:

Each symbol or is a QPSK symbol.

* With appropriate combining at the receiver, for an AWGN channel, the performance of DCM π/2-BPSK signals transmitted over 2.16+2.16 GHz or 4.32+4.32 GHz channels is the same as BPSK (due to a 3 dB gain obtained due to noise averaging). Impact of RF impairments is approximately the same as for BPSK modulations. EVM requirements for DCM π/2-BPSK signals should thus be aligned with the corresponding BPSK signals coded with the same code rates.

**Modifications**

Modify Table 94 (D2.0, page 473) as follows

|  |  |  |  |
| --- | --- | --- | --- |
| **MCS** | **Modulation** | **Code rate** | **EVM value [dB]** |
| 2 | DCM π/2-BPSK | 1/2 | -7 |
| 3 | DCM π/2-BPSK | 5/8 | -9 |
| 4 | DCM π/2-BPSK | 3/4 | -10 |
| 5 | DCM π/2-BPSK | 13/16 | -12 |
| 6 | DCM π/2-BPSK | 7/8 | -13 |