IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Comment resolutions for 10.43.1 | | | | |
| Date: 2018-09-01 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Alfred Asterjadhi | Qualcomm Inc. | 5775 Morehouse Dr, San Diego, CA 92109 | +1-858-658-5302 | aasterja@qti.qualcomm.com |
| Abhishek Patil | Qualcomm Inc. |  |  |  |
| George Cherian | Qualcomm Inc. |  |  |  |

Abstract

This submission proposes resolutions for multiple comments related to TGax D3.0 with the following CIDs (3 CIDs):

* 15290, 15291, 15292

Revisions:

* Rev 0: Initial version of the document.

Interpretation of a Motion to Adopt

A motion to approve this submission means that the editing instructions and any changed or added material are actioned in the TGax Draft. This introduction is not part of the adopted material.

***Editing instructions formatted like this are intended to be copied into the TGax Draft (i.e. they are instructions to the 802.11 editor on how to merge the text with the baseline documents).***

***TGax Editor: Editing instructions preceded by “TGax Editor” are instructions to the TGax editor to modify existing material in the TGax draft. As a result of adopting the changes, the TGax editor will execute the instructions rather than copy them to the TGax Draft.***

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Commenter** | **P.L** | **Comment** | **Proposed Change** | **Resolution** |
| 15290 | Amelia Andersdotter | 234.56 | It says that "In general, the meaning of .... [etc]". Are there specific exceptions to this rule introduced elsewhere in the document? | Not sure. | Revised –  Agree in principle with the comment. There is no reason for stating “in general”. Proposed resolution is to remove the wording.  TGax editor to make the changes shown in 11-18/ 1466r0 under all headings that include CID 15290. |
| 15291 | Amelia Andersdotter | 234.58 | Why is this a "transmitting STA" rather than a "requesting STA" (within the meaning of 10.42.1 paragraph 2)? | As in comment. | Revised –  Agree in principle with the comment. Proposed resolution is to replace it with “requesting STA” to be consistent with the term responding STA.  TGax editor to make the changes shown in 11-18/1466r0 under all headings that include CID 15291 |
| 15292 | Amelia Andersdotter | 234.62 | Why is this a "transmitting STA" rather than a "requesting STA" (within the meaning of 10.42.1 paragraph 2)? | As in comment. | Revised –  Agree in principle with the comment. Proposed resolution is to replace it with “requesting STA” to be consistent with the term responding STA.  TGax editor to make the changes shown in 11-18/1466r0 under all headings that include CID 15292 |

**Discussion: *None.***

**10.43 Target wake time (TWT)**

**10.43.1 TWT overview**

**TGax Editor: *Change the paragraph below of this subclause as follows (#CID15290, 15291, 15292):***

The result of an exchange of TWT Setup frames between a TWT requesting STA and a TWT responding STA is defined in Table 10-19a (TWT setup exchange command interpretation). The*(#15290)* meaning of Request TWT is that the requesting*(#15291)* STA does not provide a set of TWT parameters for a TWT agreement, leaving the choice of parameters to the responding STA, “Suggest TWT” indicates that the requesting*(#15292)* STA offers a set of preferred TWT parameters for a TWT agreement but might accept alternative TWT parameters that the responding STA indicates and “Demand TWT” indicates that the requesting*(#15292)* STA will currently accept only the indicated TWT parameters for a TWT agreement. When transmitted by a responding STA, “Accept TWT” indicates that the responding STA has initiated a TWT agreement with the given parameters, Alternate TWT indicates a counter-offer of TWT parameters (although alternative TWT parameters might be accepted as well) without the creation of a TWT agreement, “Dictate TWT” indicates that no TWT agreement is created, but one is likely to be accepted only if the requesting STA transmits a new TWT setup request with the indicated TWT parameters (i.e., no other TWT parameters will be accepted), and "Reject TWT" transmitted by a responding STA as part of a negotiation for a new TWT agreement is used to indicate that the negotiation has ended in failure to create a new TWT agreement.