IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Resolution to CID 1180 | | | | |
| Date: 2018-09-12 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Chris Hansen | Peraso |  |  | chris@covariantcorp.com |
|  |  |  |  |  |

Abstract

Resolution to CID 1180

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 1180 | Hiroyuki Motozuka | 20.3.4 | aSCGILength is defined in Table 20-28 while N\_GI, which shall be equal to aSCGILength, is defined in Table 20-4 as N\_GI=64. Table 20-4 should refer aSCGILength instead of the value "64". Also, "512" is referred in the definition for T\_HEADER and T\_Data. aSCBlockSize should be referred instead. | Replace the "Value" for N\_GI with "aSCGILength (64) as defined in Table 20-28 (DMG PHY characteristics)." (64) is for reader's convinience.     Replace the "Value" for T\_HEADER with "0.582 us=2 x aSCBlockSize x Tc (for SC and low-power SC)     Replace the "Value" for T\_Data with "(N\_BLKS x aSCBlockSize + aSCGILength) x Tc (for SC)  NOTE - N\_BLKS is defined in 20.5.3.2.3.3 (LDPC encoding process) and aSCBlockSize and aSCGILength are defined in Table 20-28 (DMG PHY characteristics)" |

Resolution: Revise

Discussion: Commentor is correct, however the additional (64) is the resolution should be removed. Updated the editor instructions to follow table numbers for 802.11md revision 1.5.

*Instruct the Editor to:*

Replace the Value for N\_GI with "aSCGILength as defined in Table 20-29 (DMG PHY characteristics)."  
  
Replace the Value for T\_HEADER with "0.582 us=2 x aSCBlockSize x Tc (for SC and low-power SC)"  
  
Replace the Value for T\_Data with "(N\_BLKS x aSCBlockSize + aSCGILength) x Tc (for SC)"  
  
 NOTE - N\_BLKS is defined in 20.5.3.2.3.3 (LDPC encoding process) and aSCBlockSize and aSCGILength are defined in Table 20-29 (DMG PHY characteristics)"